<?xml version="1.0" encoding="utf-8"?>
<!--/5619982/1088951/2.50/17/3/Integrated Circuit/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;Motor / Motion / Ignition Controllers &amp; Drivers 37-V, 3.5-A brushed DC motor driver with integrated current sensing and current sense output 16-VQFN -40 to 125&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="QFN50P300X300X100-17N">
<description>&lt;b&gt;RGT001&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="DRV8876RGTR">
<pin name="NSLEEP" direction="io"/>
<pin name="NFAULT" direction="io"/>
<pin name="VREF" direction="io"/>
<pin name="IPROPI" direction="io"/>
<pin name="IMODE" direction="io"/>
<pin name="OUT1" direction="io"/>
<pin name="PGND" direction="io"/>
<pin name="OUT2" direction="io"/>
<pin name="CPL" direction="io"/>
<pin name="CPH" direction="io"/>
<pin name="VCP" direction="io"/>
<pin name="VM" direction="io"/>
<pin name="EP" direction="io"/>
<pin name="PH/IN2" direction="io"/>
<pin name="EN/IN1" direction="io"/>
<pin name="PMODE" direction="io"/>
<pin name="GND" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DRV8876RGTR" prefix="IC">
<description>&lt;b&gt;Motor / Motion / Ignition Controllers &amp; Drivers 37-V, 3.5-A brushed DC motor driver with integrated current sensing and current sense output 16-VQFN -40 to 125&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/gpn/drv8876"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="DRV8876RGTR"/>
</gates>
<devices>
<device name="" package="QFN50P300X300X100-17N">
<connects>
<connect gate="G$1" pin="NSLEEP" pad="1"/>
<connect gate="G$1" pin="NFAULT" pad="2"/>
<connect gate="G$1" pin="VREF" pad="3"/>
<connect gate="G$1" pin="IPROPI" pad="4"/>
<connect gate="G$1" pin="IMODE" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="PGND" pad="7"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="VM" pad="9"/>
<connect gate="G$1" pin="VCP" pad="10"/>
<connect gate="G$1" pin="CPH" pad="11"/>
<connect gate="G$1" pin="CPL" pad="12"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="PMODE" pad="14"/>
<connect gate="G$1" pin="EN/IN1" pad="15"/>
<connect gate="G$1" pin="PH/IN2" pad="16"/>
<connect gate="G$1" pin="EP" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="Mouser_Part_Number" value="595-DRV8876RGTR"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/DRV8876RGTR?qs=T3oQrply3y%2F6lJwB3MIeHA%3D%3D"/>
<attribute name="Manufacturer_Name" value="Texas Instruments"/>
<attribute name="Manufacturer_Part_Number" value="DRV8876RGTR"/>
<attribute name="Description" value="Motor / Motion / Ignition Controllers &amp; Drivers 37-V, 3.5-A brushed DC motor driver with integrated current sensing and current sense output 16-VQFN -40 to 125"/>
<attribute name="Height" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
