<?xml version="1.0" encoding="utf-8"?>
<!--/315446/1088951/2.50/12/4/Filter/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;Common Mode Filter &amp; ESD Prot. USB uQFN8 STMicroelectronics ECMF02 Series, Signal Filter uQFN SMD, Flat Contact Termination, 2.6 x 1.3 x 0.6mm&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="ECMF024CMX8">
<description>&lt;b&gt;Micro QFN-8L&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="ECMF02-4CMX8">
<pin name="VBUS" direction="io"/>
<pin name="D-_1" direction="io"/>
<pin name="D+_1" direction="io"/>
<pin name="ID" direction="io"/>
<pin name="GND_1" direction="io"/>
<pin name="D+_2" direction="io"/>
<pin name="D-_2" direction="io"/>
<pin name="GND_2" direction="io"/>
<pin name="9" direction="io"/>
<pin name="10" direction="io"/>
<pin name="11" direction="io"/>
<pin name="12" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ECMF02-4CMX8" prefix="FL">
<description>&lt;b&gt;Common Mode Filter &amp; ESD Prot. USB uQFN8 STMicroelectronics ECMF02 Series, Signal Filter uQFN SMD, Flat Contact Termination, 2.6 x 1.3 x 0.6mm&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.st.com/content/ccc/resource/technical/document/datasheet/group3/1c/93/cf/72/85/cf/4d/d6/DM00039389/files/DM00039389.pdf/jcr:content/translations/en.DM00039389.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ECMF02-4CMX8"/>
</gates>
<devices>
<device name="" package="ECMF024CMX8">
<connects>
<connect gate="G$1" pin="VBUS" pad="1"/>
<connect gate="G$1" pin="D-_1" pad="2"/>
<connect gate="G$1" pin="D+_1" pad="3"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="GND_1" pad="5"/>
<connect gate="G$1" pin="D+_2" pad="6"/>
<connect gate="G$1" pin="D-_2" pad="7"/>
<connect gate="G$1" pin="GND_2" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="Mouser_Part_Number" value="511-ECMF02-4CMX8"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/STMicroelectronics/ECMF02-4CMX8?qs=xYt8xtm2zhmK7GoDlDZR3A%3D%3D"/>
<attribute name="Manufacturer_Name" value="STMicroelectronics"/>
<attribute name="Manufacturer_Part_Number" value="ECMF02-4CMX8"/>
<attribute name="Description" value="Common Mode Filter &amp; ESD Prot. USB uQFN8 STMicroelectronics ECMF02 Series, Signal Filter uQFN SMD, Flat Contact Termination, 2.6 x 1.3 x 0.6mm"/>
<attribute name="Height" value="mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
