<?xml version="1.0" encoding="utf-8"?>
<!--/529621/1088951/2.50/8/2/Connector/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;PCB terminal block, nominal current: 6 A, rated voltage (III/2): 160 V, nominal cross section: 0.5 mm?, Number of potentials: 8, Number of rows: 1, Number of positions per row: 8, product range: PTSM 0,5/..-H-SMD, pitch: 2.5 mm, connection method: Push-in spring connection, mounting: SMD soldering, conductor/PCB connection direction: 0 ?, color: black, Pin layout: Linear pad geometry, type of packaging: packed in cardboard&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="1771088">
<description>&lt;b&gt;1771088&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="1771088">
<pin name="1" direction="io"/>
<pin name="2" direction="io"/>
<pin name="3" direction="io"/>
<pin name="4" direction="io"/>
<pin name="5" direction="io"/>
<pin name="6" direction="io"/>
<pin name="7" direction="io"/>
<pin name="8" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="1771088" prefix="J">
<description>&lt;b&gt;PCB terminal block, nominal current: 6 A, rated voltage (III/2): 160 V, nominal cross section: 0.5 mm?, Number of potentials: 8, Number of rows: 1, Number of positions per row: 8, product range: PTSM 0,5/..-H-SMD, pitch: 2.5 mm, connection method: Push-in spring connection, mounting: SMD soldering, conductor/PCB connection direction: 0 ?, color: black, Pin layout: Linear pad geometry, type of packaging: packed in cardboard&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.phoenixcontact.net/product/1771088"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="1771088"/>
</gates>
<devices>
<device name="" package="1771088">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="Mouser_Part_Number" value="651-1771088"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/Phoenix-Contact/1771088?qs=Q77YN%2FRrsKIDMojcNKtpFQ%3D%3D"/>
<attribute name="Manufacturer_Name" value="Phoenix Contact"/>
<attribute name="Manufacturer_Part_Number" value="1771088"/>
<attribute name="Description" value="PCB terminal block, nominal current: 6 A, rated voltage (III/2): 160 V, nominal cross section: 0.5 mm?, Number of potentials: 8, Number of rows: 1, Number of positions per row: 8, product range: PTSM 0,5/..-H-SMD, pitch: 2.5 mm, connection method: Push-in spring connection, mounting: SMD soldering, conductor/PCB connection direction: 0 ?, color: black, Pin layout: Linear pad geometry, type of packaging: packed in cardboard"/>
<attribute name="Height" value="5.22mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
