<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.2">
<drawing>
<board>
<plain>
<text>https://openmv.io</text>
<text>MT9V024-MOD R1</text>
<text>01/10/22</text>
<wire x1="0" y1="16.51" x2="0" y2="11.176" width="0" layer="20"/>
<wire x1="0" y1="5.334" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="16.51" y2="0" width="0" layer="20"/>
<wire x1="16.51" y1="0" x2="16.51" y2="5.334" width="0" layer="20"/>
<wire x1="16.51" y1="11.176" x2="16.51" y2="16.51" width="0" layer="20"/>
<wire x1="16.51" y1="16.51" x2="0" y2="16.51" width="0" layer="20"/>
<wire x1="0" y1="11.176" x2="-6.731" y2="11.176" width="0" layer="20"/>
<wire x1="-6.731" y1="11.176" x2="-9.525" y2="8.255" width="0" layer="20" curve="90"/>
<wire x1="-9.525" y1="8.255" x2="-6.731" y2="5.334" width="0" layer="20" curve="90"/>
<wire x1="-6.731" y1="5.334" x2="0" y2="5.334" width="0" layer="20"/>
<wire x1="16.51" y1="11.176" x2="23.241" y2="11.176" width="0" layer="20"/>
<wire x1="23.241" y1="11.176" x2="26.035" y2="8.255" width="0" layer="20" curve="-90"/>
<wire x1="26.035" y1="8.255" x2="23.241" y2="5.334" width="0" layer="20" curve="-90"/>
<wire x1="23.241" y1="5.334" x2="16.51" y2="5.334" width="0" layer="20"/>
</plain>
<libraries>
<library name="sfe">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
</package>
<package name="0805">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="openmv">
<packages>
<package name="WEEE">
</package>
<package name="ROHS">
</package>
</packages>
</library>
<library name="DF12">
<packages>
<package name="DF12-36-DP">
</package>
</packages>
</library>
<library name="omnivision">
<description>&lt;b&gt;OmniVision Technologies, Inc.&lt;/b&gt;&lt;p&gt;
www.ovt.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LENSMOUNT-20MM">
</package>
</packages>
</library>
<library name="resistor-dil">
<description>&lt;b&gt;Resistors in DIL Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EXBV8V">
<description>&lt;b&gt;Chip Resistor Array 0603x4&lt;/b&gt; 4 resistors in 3.20 mm x 1.60 mm size&lt;p&gt;
Source: PANASONIC .. aoc0000ce1.pdf</description>
</package>
</packages>
</library>
<library name="MT9V022">
<packages>
<package name="IBGA52">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C5" library="sfe" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="sfe" package="0603" value="MPZ1608S181ATAH0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="sfe" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="openmv" package="WEEE" value=""/>
<element name="U$2" library="openmv" package="ROHS" value=""/>
<element name="LM1" library="omnivision" package="LENSMOUNT-20MM" value="LENSMOUNT20MM"/>
<element name="RN1" library="resistor-dil" package="EXBV8V" value="10K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="DF12" package="DF12-36-DP" value="DF12-36-DP"/>
<element name="U4" library="MT9V022" package="IBGA52" value="MT9V022">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="U$3" pad="5"/>
<contactref element="U$3" pad="19"/>
<contactref element="U$3" pad="27"/>
<contactref element="U4" pad="B1"/>
<contactref element="U4" pad="C3"/>
<contactref element="U4" pad="C6"/>
<contactref element="U4" pad="F3"/>
<contactref element="U4" pad="C7"/>
<contactref element="U4" pad="F6"/>
<contactref element="U4" pad="H7"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="N$64">
</signal>
<signal name="N$65">
</signal>
<signal name="N$66">
</signal>
<signal name="N$67">
</signal>
<signal name="N$68">
</signal>
<signal name="N$69">
</signal>
<signal name="N$70">
</signal>
<signal name="N$71">
</signal>
<signal name="N$72">
</signal>
<signal name="N$73">
</signal>
<signal name="N$74">
</signal>
<signal name="N$75">
</signal>
<signal name="N$76">
</signal>
<signal name="N$77">
</signal>
<signal name="N$57">
</signal>
<signal name="N$19">
<contactref element="U4" pad="G7"/>
<contactref element="RN1" pad="5"/>
</signal>
<signal name="N$20">
<contactref element="U4" pad="H8"/>
<contactref element="RN1" pad="6"/>
</signal>
<signal name="VDDA">
<contactref element="L1" pad="1"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$3" pad="10"/>
<contactref element="U$3" pad="20"/>
<contactref element="U$3" pad="30"/>
<contactref element="U$3" pad="36"/>
<contactref element="U4" pad="B4"/>
<contactref element="U4" pad="E2"/>
<contactref element="U4" pad="A4"/>
<contactref element="U4" pad="H6"/>
<contactref element="RN1" pad="1"/>
<contactref element="RN1" pad="3"/>
<contactref element="RN1" pad="4"/>
<contactref element="U4" pad="A1"/>
</signal>
<signal name="DCMI_D2">
<contactref element="U$3" pad="31"/>
<contactref element="U4" pad="A7"/>
</signal>
<signal name="DCMI_D3">
<contactref element="U$3" pad="29"/>
<contactref element="U4" pad="A8"/>
</signal>
<signal name="DCMI_PCLK">
<contactref element="U$3" pad="14"/>
<contactref element="U4" pad="B5"/>
</signal>
<signal name="DCMI_HSYNC">
<contactref element="U$3" pad="18"/>
<contactref element="U4" pad="H2"/>
</signal>
<signal name="DCMI_VSYNC">
<contactref element="U$3" pad="16"/>
<contactref element="U4" pad="G2"/>
</signal>
<signal name="DCMI_CLK">
<contactref element="U$3" pad="12"/>
<contactref element="U4" pad="A5"/>
</signal>
<signal name="DCMI_RST">
<contactref element="U$3" pad="21"/>
<contactref element="U4" pad="G8"/>
<contactref element="RN1" pad="8"/>
</signal>
<signal name="DCMI_PWDN">
<contactref element="U$3" pad="25"/>
<contactref element="U4" pad="F8"/>
<contactref element="RN1" pad="7"/>
</signal>
<signal name="DCMI_D4">
<contactref element="U$3" pad="35"/>
<contactref element="U4" pad="B7"/>
</signal>
<signal name="DCMI_D5">
<contactref element="U$3" pad="28"/>
<contactref element="U4" pad="E1"/>
</signal>
<signal name="DCMI_D6">
<contactref element="U$3" pad="26"/>
<contactref element="U4" pad="F1"/>
</signal>
<signal name="DCMI_D7">
<contactref element="U$3" pad="33"/>
<contactref element="U4" pad="F2"/>
</signal>
<signal name="DCMI_D8">
<contactref element="U$3" pad="24"/>
<contactref element="U4" pad="G1"/>
</signal>
<signal name="DCMI_D9">
<contactref element="U$3" pad="22"/>
<contactref element="U4" pad="H1"/>
</signal>
<signal name="DCMI_SCL">
<contactref element="U$3" pad="32"/>
<contactref element="U4" pad="H4"/>
</signal>
<signal name="DCMI_SDA">
<contactref element="U$3" pad="34"/>
<contactref element="U4" pad="G4"/>
</signal>
<signal name="DCMI_FSIN">
<contactref element="U$3" pad="23"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="SPI3_SCLK">
<contactref element="U$3" pad="13"/>
<contactref element="U4" pad="G5"/>
</signal>
<signal name="SPI3_MISO">
<contactref element="U$3" pad="15"/>
<contactref element="U4" pad="H3"/>
</signal>
<signal name="SPI3_MOSI">
<contactref element="U$3" pad="17"/>
<contactref element="U4" pad="G3"/>
</signal>
<signal name="SPI3_SSEL">
<contactref element="U$3" pad="11"/>
<contactref element="U4" pad="G6"/>
</signal>
<signal name="VAA">
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U4" pad="C8"/>
<contactref element="U4" pad="F7"/>
<contactref element="U4" pad="B8"/>
</signal>
<signal name="RSVD1">
<contactref element="U$3" pad="1"/>
</signal>
<signal name="RSVD2">
<contactref element="U$3" pad="3"/>
</signal>
<signal name="RSVD5">
<contactref element="U$3" pad="6"/>
</signal>
<signal name="RSVD6">
<contactref element="U$3" pad="8"/>
</signal>
<signal name="DCMI_D0">
<contactref element="U$3" pad="9"/>
<contactref element="U4" pad="A6"/>
</signal>
<signal name="DCMI_D1">
<contactref element="U$3" pad="7"/>
<contactref element="U4" pad="B6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
