<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="44.45" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="35.56" y2="0" width="0" layer="20"/>
<wire x1="35.56" y1="0" x2="35.56" y2="44.45" width="0" layer="20"/>
<wire x1="35.56" y1="44.45" x2="0" y2="44.45" width="0" layer="20"/>
<text>P6</text>
<text>P4</text>
<text>P5</text>
<text>P3</text>
<text>P2</text>
<text>P1</text>
<text>BT0</text>
<text>RST</text>
<text>P7</text>
<text>GND</text>
<text>3.3V</text>
<text>VIN</text>
<text>P8</text>
<text>P0</text>
<text>3.3V</text>
<text>P6</text>
<text>P5</text>
<text>P4</text>
<text>P3</text>
<text>P2</text>
<text>P1</text>
<text>P0</text>
<text>GND</text>
<text>VIN</text>
<text>P7</text>
<text>P8</text>
<text>RST</text>
<text>BT0</text>
<text>OpenMV4-PRO R1</text>
<text>12/28/2021</text>
<text>VIN Max
Voltage: 5v</text>
<text>P10</text>
<text>P10</text>
<text>P9</text>
<text>P9</text>
<text>IR</text>
<text>W</text>
<text>VBUS</text>
<text>GND</text>
<text>GND</text>
<text>VBUS</text>
</plain>
<libraries>
<library name="sfe">
<packages>
<package name="0805">
</package>
<package name="SOT23-3">
</package>
<package name="LED-1206">
</package>
<package name="EIA3216">
</package>
<package name="1007">
<description>1007 (2518 metric) package</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0603">
</package>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 2.8 mm, round</description>
</package>
</packages>
</library>
<library name="openmv">
<packages>
<package name="OMV-LOGO">
</package>
<package name="WEEE">
</package>
<package name="ROHS">
</package>
<package name="OMV-LOGO-SMALL">
</package>
</packages>
</library>
<library name="stm32">
<packages>
<package name="UFGBGA-176">
</package>
</packages>
</library>
<library name="regulators">
<packages>
<package name="TSOT25">
</package>
</packages>
</library>
<library name="adafruit-updated">
<packages>
<package name="JST-PH-2-THM-RA">
<description>&lt;b&gt;S2B-PH-K-S&lt;/b&gt; 
&lt;p&gt;
JST PH 2-pin thru-home side entry</description>
</package>
</packages>
</library>
<library name="DF12">
<packages>
<package name="DF12-36-DS">
</package>
</packages>
</library>
<library name="molex">
<packages>
<package name="1040310811">
</package>
</packages>
</library>
<library name="STANDOFFS">
<packages>
<package name="9774030151R">
</package>
</packages>
</library>
<library name="ISSI">
<packages>
<package name="BGA90">
</package>
</packages>
</library>
<library name="W25Q256JVEIQ_TR">
<packages>
<package name="SON127P800X600X80-9N">
</package>
</packages>
</library>
<library name="esd">
<packages>
<package name="QFN3.5">
</package>
</packages>
</library>
<library name="Microchip - USB3320C-EZK-TR">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="MICROCHIP_USB3320C-EZK-TR_1">
<description>IC TRANSCEIVER HALF 1/1 32QFN</description>
</package>
</packages>
</library>
<library name="LBEE5KL1DX-TEMP">
<packages>
<package name="XCVR_LBEE5KL1DX-TEMP">
</package>
</packages>
</library>
<library name="SiTime - SIT1533AI-H4-DCC-32.768E">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="SITIME_SIT1533AI-H4-DCC-32.768E_0">
<description>20 ppm, Ultra-Low Power 32.768 kHz Quartz XTAL Replacement</description>
</package>
</packages>
</library>
<library name="OSC_DSC6083CI2A-032K768">
<packages>
<package name="OSC_DSC6083CI2A-032K768">
</package>
</packages>
</library>
<library name="PP_Connectors">
<packages>
<package name="105450-0101">
</package>
</packages>
</library>
<library name="STMicroelectronics - ECMF02-4CMX8">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="STMICROELECTRONICS_ECMF02-4CMX8_0">
<description>2 Line Common Mode Choke Surface Mount   DCR 4Ohm</description>
</package>
</packages>
</library>
<library name="Samtec - FTSH-105-01-F-DV">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="SAMTEC_FTSH-105-01-F-DV_0">
<description>Conn Unshrouded Header HDR 10 POS 1.27mm Solder ST SMD Tube</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="LSM6DS3">
<packages>
<package name="PQFN50P300X250X86-14N">
</package>
</packages>
</library>
<library name="STMicroelectronics - VL53L1CXV0FY">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="STMICROELECTRONICS_VL53L1CXV0FY-1_0">
<description>Optical Sensor 157.480" (4m) I²C Output</description>
</package>
</packages>
</library>
<library name="Z01SDZ">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="NXP_SEMICONDUCTORS_SE050C2HQ1-Z01SDZ_1">
<description>SE050 Series 6 V 10 mA 600 mW Surface Mount IoT Secure Element - HX2QFN-20</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0201">
<description>Source: http://www.avxcorp.com/docs/catalogs/cx5r.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="leptonCustom">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;SOT23-5&lt;/b&gt; Zetex&lt;p&gt;
Source: http://www.zetex.com/3.0/pdf/ZXSC300.pdf</description>
</package>
</packages>
</library>
<library name="Texas Instruments - BQ24072TRGTR">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="TEXAS_INSTRUMENTS_BQ24072TRGTR_0">
<description>TI-BQ24072TRGT16-1700X1700TP</description>
</package>
</packages>
</library>
<library name="Vishay - VCUT05E1-SD0-G4-08">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="VISHAY_VCUT05E1-SD0-G4-08_0">
<description>ESD Suppressor TVS 3kV 2-Pin CLP T/R</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Cree - CLM3C-WKW-CWBYA453">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="CREE_CLM3C-WKW-CWBYA453_0">
<description>LED, Cool White, SMD, 2.7mm x 2mm, 20 mA, 3.2 V, 3.55 cd</description>
</package>
</packages>
</library>
<library name="Cree - UHD1110-FKA-CL1A13R3Q1BBQFMF3">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="CREE_UHD1110-FKA-CL1A13R3Q1BBQFMF3_0">
<description>Red, Green, Blue (RGB) - LED Indication - Discrete 1.9V Red, 2.9V Green, 2.9V Blue 0404 (1010 Metric)</description>
</package>
</packages>
</library>
<library name="HIROSE - U.FL-R-SMT-1(10)">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="HIROSE_U_FL-R-SMT-1_10_0">
<description>U.FL (UMCC) Connector Receptacle, Male Pin 50Ohm Surface Mount Solder</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_2_NC_PASTE_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="H2" library="holes" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8">
<attribute name="POPULARITY" value="6"/>
</element>
<element name="H1" library="holes" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8">
<attribute name="POPULARITY" value="6"/>
</element>
<element name="Q1" library="sfe" package="SOT23-3" value="BSS138">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="sfe" package="0402-RES" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="openmv" package="OMV-LOGO" value=""/>
<element name="U$1" library="openmv" package="WEEE" value=""/>
<element name="U$2" library="openmv" package="ROHS" value=""/>
<element name="U$4" library="openmv" package="OMV-LOGO-SMALL" value=""/>
<element name="LED2" library="sfe" package="LED-1206" value="VSMY12850">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="sfe" package="LED-1206" value="VSMY12850">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="sfe" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="sfe" package="0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="sfe" package="1007" value="4.7uH/1.4A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="regulators" package="TSOT25" value="PAM2305AABADJ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="adafruit-updated" package="JST-PH-2-THM-RA" value="S2B-PH-K-S(LF)(SN)">
<attribute name="NAME"/>
</element>
<element name="X2" library="molex" package="1040310811" value="USD-1040310811">
<attribute name="NAME"/>
</element>
<element name="R6" library="sfe" package="0402-RES" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="sfe" package="0402-RES" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M1" library="STANDOFFS" package="9774030151R" value="9774030243R"/>
<element name="M2" library="STANDOFFS" package="9774030151R" value="9774030243R"/>
<element name="C6" library="sfe" package="EIA3216" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="DF12" package="DF12-36-DS" value="DF12-36-DS">
<attribute name="NAME"/>
</element>
<element name="C20" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="sfe" package="EIA3216" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="U14" library="ISSI" package="BGA90" value="IS42S32800">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U10" library="stm32" package="UFGBGA-176" value="STM32H743IIK6">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="sfe" package="0402-CAP" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="sfe" package="0402-CAP" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="sfe" package="0402-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="sfe" package="0402-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="sfe" package="C0402" value="MPZ1608S181ATAH0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="W25Q256JVEIQ_TR" package="SON127P800X600X80-9N" value="W25Q256JVEIQ_TR">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" FLASH - NOR Memory IC 256Mb (32M x 8) SPI - Quad I/O 133MHz 8-WSON (8x6) "/>
<attribute name="MF" value="Winbond"/>
<attribute name="MP" value="W25Q256JVEIQ TR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="WSON-8 Winbond"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="esd" package="QFN3.5" value="EMIF06-MSD02N16">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="Microchip - USB3320C-EZK-TR" package="MICROCHIP_USB3320C-EZK-TR_1" value="MICROCHIP_USB3320C-EZK-TRMICROCHIP_USB3320C-EZK-TR_0_1">
<attribute name="AMBIENT_TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="AMBIENT_TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="DATASHEET" value="http://ww1.microchip.com/downloads/en/DeviceDoc/00001792E.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Integrated Circuits (ICs)"/>
<attribute name="DEVICE_CLASS_L2" value="Interface ICs"/>
<attribute name="DEVICE_CLASS_L3" value="USB Interface ICs"/>
<attribute name="DIGIKEY_DESCRIPTION" value="IC TRANSCEIVER HALF 1/1 32QFN"/>
<attribute name="DIGIKEY_PART_NUMBER" value="USB3320C-EZK-CT-ND"/>
<attribute name="FOOTPRINT_PARAMETERS_1" value="{&quot;fp_type&quot;:&quot;QFN&quot;,&quot;params&quot;:{&quot;N1&quot;:{&quot;nom&quot;:8,&quot;long name&quot;:&quot;Leads on long side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N1&quot;,&quot;type&quot;:&quot;count&quot;},&quot;N2&quot;:{&quot;nom&quot;:8,&quot;long name&quot;:&quot;Leads on wide side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N2&quot;,&quot;type&quot;:&quot;count&quot;},&quot;A&quot;:{&quot;nom&quot;:850000,&quot;long name&quot;:&quot;Height&quot;,&quot;min&quot;:700000,&quot;max&quot;:1451100,&quot;short name&quot;:&quot;A&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A1&quot;:{&quot;nom&quot;:20000,&quot;long name&quot;:&quot;Package clearance&quot;,&quot;min&quot;:0,&quot;max&quot;:50000,&quot;short name&quot;:&quot;A1&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A2&quot;:{&quot;nom&quot;:650000,&quot;long name&quot;:&quot;Package height&quot;,&quot;min&quot;:false,&quot;max&quot;:900000,&quot;short name&quot;:&quot;A2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;D&quot;:{&quot;nom&quot;:5000000,&quot;long name&quot;:&quot;Package length&quot;,&quot;min&quot;:4900000,&quot;max&quot;:5100000,&quot;short name&quot;:&quot;D&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E&quot;:{&quot;nom&quot;:5000000,&quot;long name&quot;:&quot;Package width&quot;,&quot;min&quot;:4900000,&quot;max&quot;:5100000,&quot;short name&quot;:&quot;E&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;B&quot;:{&quot;nom&quot;:250000,&quot;long name&quot;:&quot;Lead width&quot;,&quot;min&quot;:180000,&quot;max&quot;:300000,&quot;short name&quot;:&quot;B&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;C&quot;:{&quot;nom&quot;:200000,&quot;long name&quot;:&quot;Lead thickness&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;C&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;L&quot;:{&quot;nom&quot;:400000,&quot;long name&quot;:&quot;Lead foot length&quot;,&quot;min&quot;:300000,&quot;max&quot;:500000,&quot;short name&quot;:&quot;L&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;e&quot;:{&quot;nom&quot;:500000,&quot;long name&quot;:&quot;Lead pitch&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;e&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;HT&quot;:{&quot;default&quot;:&quot;Yes&quot;,&quot;long name&quot;:&quot;Thermal pad&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;HT&quot;,&quot;children&quot;:[&quot;D2&quot;,&quot;E2&quot;,&quot;PC&quot;]},&quot;offset x&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;X Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset x&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;offset y&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Y Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset y&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;LS&quot;:{&quot;default&quot;:&quot;Rounded rectangle&quot;,&quot;long name&quot;:&quot;Land shape&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS&quot;},&quot;LS1&quot;:{&quot;default&quot;:&quot;Rectangle&quot;,&quot;long name&quot;:&quot;Land shape (Pin 1)&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS1&quot;},&quot;solder toe&quot;:{&quot;nom&quot;:400000,&quot;long name&quot;:&quot;Solder fillet (toe)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder toe&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder heel&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Solder fillet (heel)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder heel&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder side&quot;:{&quot;nom&quot;:-40000,&quot;long name&quot;:&quot;Solder fillet (side)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder side&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;courtyard&quot;:{&quot;nom&quot;:500000,&quot;long name&quot;:&quot;Courtyard&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;courtyard&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;SF&quot;:{&quot;default&quot;:&quot;A&quot;,&quot;long name&quot;:&quot;Packing level&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;SF&quot;,&quot;help&quot;:&quot;http://support.upverter.com/customer/portal/articles/978783-what-is-a-footprint-packing-level&quot;,&quot;children&quot;:[&quot;solder toe&quot;,&quot;solder heel&quot;,&quot;solder side&quot;,&quot;courtyard&quot;]},&quot;D2&quot;:{&quot;nom&quot;:3300000,&quot;long name&quot;:&quot;Thermal pad length&quot;,&quot;min&quot;:3200000,&quot;max&quot;:3400000,&quot;short name&quot;:&quot;D2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E2&quot;:{&quot;nom&quot;:3300000,&quot;long name&quot;:&quot;Thermal pad width&quot;,&quot;min&quot;:3200000,&quot;max&quot;:3400000,&quot;short name&quot;:&quot;E2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;PC&quot;:{&quot;long name&quot;:&quot;Paste coverage (%)&quot;,&quot;type&quot;:&quot;percentage&quot;,&quot;short name&quot;:&quot;PC&quot;,&quot;value&quot;:40}}}"/>
<attribute name="FOOTPRINT_PARAMETERS_2" value="{&quot;fp_type&quot;:&quot;QFN&quot;,&quot;params&quot;:{&quot;N1&quot;:{&quot;nom&quot;:8,&quot;long name&quot;:&quot;Leads on long side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N1&quot;,&quot;type&quot;:&quot;count&quot;},&quot;N2&quot;:{&quot;nom&quot;:8,&quot;long name&quot;:&quot;Leads on wide side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N2&quot;,&quot;type&quot;:&quot;count&quot;},&quot;A&quot;:{&quot;nom&quot;:850000,&quot;long name&quot;:&quot;Height&quot;,&quot;min&quot;:700000,&quot;max&quot;:1451100,&quot;short name&quot;:&quot;A&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A1&quot;:{&quot;nom&quot;:20000,&quot;long name&quot;:&quot;Package clearance&quot;,&quot;min&quot;:0,&quot;max&quot;:50000,&quot;short name&quot;:&quot;A1&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A2&quot;:{&quot;nom&quot;:650000,&quot;long name&quot;:&quot;Package height&quot;,&quot;min&quot;:false,&quot;max&quot;:900000,&quot;short name&quot;:&quot;A2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;D&quot;:{&quot;nom&quot;:5000000,&quot;long name&quot;:&quot;Package length&quot;,&quot;min&quot;:4900000,&quot;max&quot;:5100000,&quot;short name&quot;:&quot;D&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E&quot;:{&quot;nom&quot;:5000000,&quot;long name&quot;:&quot;Package width&quot;,&quot;min&quot;:4900000,&quot;max&quot;:5100000,&quot;short name&quot;:&quot;E&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;B&quot;:{&quot;nom&quot;:250000,&quot;long name&quot;:&quot;Lead width&quot;,&quot;min&quot;:180000,&quot;max&quot;:300000,&quot;short name&quot;:&quot;B&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;C&quot;:{&quot;nom&quot;:200000,&quot;long name&quot;:&quot;Lead thickness&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;C&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;L&quot;:{&quot;nom&quot;:400000,&quot;long name&quot;:&quot;Lead foot length&quot;,&quot;min&quot;:300000,&quot;max&quot;:500000,&quot;short name&quot;:&quot;L&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;e&quot;:{&quot;nom&quot;:500000,&quot;long name&quot;:&quot;Lead pitch&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;e&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;D2&quot;:{&quot;nom&quot;:3300000,&quot;long name&quot;:&quot;Thermal pad length&quot;,&quot;min&quot;:3200000,&quot;max&quot;:3400000,&quot;short name&quot;:&quot;D2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E2&quot;:{&quot;nom&quot;:3300000,&quot;long name&quot;:&quot;Thermal pad width&quot;,&quot;min&quot;:3200000,&quot;max&quot;:3400000,&quot;short name&quot;:&quot;E2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;PC&quot;:{&quot;long name&quot;:&quot;Paste coverage (%)&quot;,&quot;type&quot;:&quot;percentage&quot;,&quot;short name&quot;:&quot;PC&quot;,&quot;value&quot;:40},&quot;HT&quot;:{&quot;default&quot;:&quot;Yes&quot;,&quot;long name&quot;:&quot;Thermal pad&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;HT&quot;,&quot;children&quot;:[&quot;D2&quot;,&quot;E2&quot;,&quot;PC&quot;]},&quot;offset x&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;X Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset x&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;offset y&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Y Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset y&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;LS&quot;:{&quot;default&quot;:&quot;Rounded rectangle&quot;,&quot;long name&quot;:&quot;Land shape&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS&quot;},&quot;LS1&quot;:{&quot;default&quot;:&quot;Rectangle&quot;,&quot;long name&quot;:&quot;Land shape (Pin 1)&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS1&quot;},&quot;solder toe&quot;:{&quot;nom&quot;:300000,&quot;long name&quot;:&quot;Solder fillet (toe)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder toe&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder heel&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Solder fillet (heel)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder heel&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder side&quot;:{&quot;nom&quot;:-40000,&quot;long name&quot;:&quot;Solder fillet (side)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder side&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;courtyard&quot;:{&quot;nom&quot;:250000,&quot;long name&quot;:&quot;Courtyard&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;courtyard&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;SF&quot;:{&quot;default&quot;:&quot;B&quot;,&quot;long name&quot;:&quot;Packing level&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;SF&quot;,&quot;help&quot;:&quot;http://support.upverter.com/customer/portal/articles/978783-what-is-a-footprint-packing-level&quot;,&quot;children&quot;:[&quot;solder toe&quot;,&quot;solder heel&quot;,&quot;solder side&quot;,&quot;courtyard&quot;]}}}"/>
<attribute name="FOOTPRINT_PARAMETERS_3" value="{&quot;fp_type&quot;:&quot;QFN&quot;,&quot;params&quot;:{&quot;N1&quot;:{&quot;nom&quot;:8,&quot;long name&quot;:&quot;Leads on long side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N1&quot;,&quot;type&quot;:&quot;count&quot;},&quot;N2&quot;:{&quot;nom&quot;:8,&quot;long name&quot;:&quot;Leads on wide side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N2&quot;,&quot;type&quot;:&quot;count&quot;},&quot;A&quot;:{&quot;nom&quot;:850000,&quot;long name&quot;:&quot;Height&quot;,&quot;min&quot;:700000,&quot;max&quot;:1451100,&quot;short name&quot;:&quot;A&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A1&quot;:{&quot;nom&quot;:20000,&quot;long name&quot;:&quot;Package clearance&quot;,&quot;min&quot;:0,&quot;max&quot;:50000,&quot;short name&quot;:&quot;A1&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A2&quot;:{&quot;nom&quot;:650000,&quot;long name&quot;:&quot;Package height&quot;,&quot;min&quot;:false,&quot;max&quot;:900000,&quot;short name&quot;:&quot;A2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;D&quot;:{&quot;nom&quot;:5000000,&quot;long name&quot;:&quot;Package length&quot;,&quot;min&quot;:4900000,&quot;max&quot;:5100000,&quot;short name&quot;:&quot;D&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E&quot;:{&quot;nom&quot;:5000000,&quot;long name&quot;:&quot;Package width&quot;,&quot;min&quot;:4900000,&quot;max&quot;:5100000,&quot;short name&quot;:&quot;E&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;B&quot;:{&quot;nom&quot;:250000,&quot;long name&quot;:&quot;Lead width&quot;,&quot;min&quot;:180000,&quot;max&quot;:300000,&quot;short name&quot;:&quot;B&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;C&quot;:{&quot;nom&quot;:200000,&quot;long name&quot;:&quot;Lead thickness&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;C&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;L&quot;:{&quot;nom&quot;:400000,&quot;long name&quot;:&quot;Lead foot length&quot;,&quot;min&quot;:300000,&quot;max&quot;:500000,&quot;short name&quot;:&quot;L&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;e&quot;:{&quot;nom&quot;:500000,&quot;long name&quot;:&quot;Lead pitch&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;e&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;D2&quot;:{&quot;nom&quot;:3300000,&quot;long name&quot;:&quot;Thermal pad length&quot;,&quot;min&quot;:3200000,&quot;max&quot;:3400000,&quot;short name&quot;:&quot;D2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E2&quot;:{&quot;nom&quot;:3300000,&quot;long name&quot;:&quot;Thermal pad width&quot;,&quot;min&quot;:3200000,&quot;max&quot;:3400000,&quot;short name&quot;:&quot;E2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;PC&quot;:{&quot;long name&quot;:&quot;Paste coverage (%)&quot;,&quot;type&quot;:&quot;percentage&quot;,&quot;short name&quot;:&quot;PC&quot;,&quot;value&quot;:40},&quot;HT&quot;:{&quot;default&quot;:&quot;Yes&quot;,&quot;long name&quot;:&quot;Thermal pad&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;HT&quot;,&quot;children&quot;:[&quot;D2&quot;,&quot;E2&quot;,&quot;PC&quot;]},&quot;offset x&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;X Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset x&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;offset y&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Y Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset y&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;LS&quot;:{&quot;default&quot;:&quot;Rounded rectangle&quot;,&quot;long name&quot;:&quot;Land shape&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS&quot;},&quot;LS1&quot;:{&quot;default&quot;:&quot;Rectangle&quot;,&quot;long name&quot;:&quot;Land shape (Pin 1)&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS1&quot;},&quot;solder toe&quot;:{&quot;nom&quot;:200000,&quot;long name&quot;:&quot;Solder fillet (toe)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder toe&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder heel&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Solder fillet (heel)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder heel&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder side&quot;:{&quot;nom&quot;:-40000,&quot;long name&quot;:&quot;Solder fillet (side)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder side&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;courtyard&quot;:{&quot;nom&quot;:100000,&quot;long name&quot;:&quot;Courtyard&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;courtyard&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;SF&quot;:{&quot;default&quot;:&quot;C&quot;,&quot;long name&quot;:&quot;Packing level&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;SF&quot;,&quot;help&quot;:&quot;http://support.upverter.com/customer/portal/articles/978783-what-is-a-footprint-packing-level&quot;,&quot;children&quot;:[&quot;solder toe&quot;,&quot;solder heel&quot;,&quot;solder side&quot;,&quot;courtyard&quot;]}}}"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="FOOTPRINT_VARIANT_NAME_1" value="IPC_A"/>
<attribute name="FOOTPRINT_VARIANT_NAME_2" value="IPC_B"/>
<attribute name="FOOTPRINT_VARIANT_NAME_3" value="IPC_C"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="INTERFACE" value="UART,USB"/>
<attribute name="IPC_LAND_PATTERN_NAME" value="QFN50P500X500X85-32"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_SUPPLY_VOLTAGE" value="5.5V"/>
<attribute name="MF" value="Microchip"/>
<attribute name="MFG_PACKAGE_IDENT" value="32QFN-3304-5X5B"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="07/2004"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="H"/>
<attribute name="MIN_SUPPLY_VOLTAGE" value="1.6V"/>
<attribute name="MOUSER_DESCRIPTION" value="Microchip USB3320C-EZK-TR, USB Transceiver, USB 2.0, 1.8 V, 3.3 V, 32-Pin QFN"/>
<attribute name="MOUSER_PART_NUMBER" value="886-USB3320C-EZK-TR"/>
<attribute name="MPN" value="USB3320C-EZK-TR"/>
<attribute name="NAME"/>
<attribute name="NOMINAL_SUPPLY_CURRENT" value="0.7-29400uA"/>
<attribute name="NUMBER_OF_PORTS" value="1"/>
<attribute name="PACKAGE" value="QFN32"/>
<attribute name="PREFIX" value="U"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="USB_STANDARD" value="USB 2.0"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C8" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="sfe" package="0402-RES" value="8.06K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="sfe" package="0402-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="LBEE5KL1DX-TEMP" package="XCVR_LBEE5KL1DX-TEMP" value="LBEE5KL1DX-TEMP">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" WICED Transceiver; 802.11 b/g/n _Wi-Fi, WiFi, WLAN_, Bluetooth® Smart Ready 4.x Dual Mode For Use With BCM4343W, i.MX 6 "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MP" value="LBEE5KL1DX-TEMP"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="sfe" package="0402-CAP" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="sfe" package="0603" value="LQM18PN2R2MGHD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y0" library="SiTime - SIT1533AI-H4-DCC-32.768E" package="SITIME_SIT1533AI-H4-DCC-32.768E_0" value="SITIME_SIT1533AI-H4-DCC-32.768ESITIME_SIT1533AI-H4-DCC-32.768E_0_0">
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="DATASHEET" value="https://www.sitime.com/datasheet/SiT1533"/>
<attribute name="DIGIKEY_DESCRIPTION" value="CRYS OSC MEMS 32.768KHZ LVCMOS SMD"/>
<attribute name="DIGIKEY_PART_NUMBER" value="1473-1239-1-ND"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MF" value="SiTime"/>
<attribute name="MFG_PACKAGE_IDENT" value="SiT1533-E"/>
<attribute name="MOUSER_PART_NUMBER" value="788-1533AIH4DCC32.76"/>
<attribute name="MPN" value="SIT1533AI-H4-DCC-32.768E"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SMT_2MM0_1MM2"/>
<attribute name="PREFIX" value="Y"/>
<attribute name="ROHS" value="yes"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
</element>
<element name="C36" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="OSC_DSC6083CI2A-032K768" package="OSC_DSC6083CI2A-032K768" value="DSC1001BI1-024.0000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L6" library="sfe" package="C0402" value="MPZ1608S101ATAH0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L7" library="sfe" package="C0402" value="MPZ1608S101ATAH0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="PP_Connectors" package="105450-0101" value="">
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
</element>
<element name="R1" library="sfe" package="0402-RES" value="5.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="sfe" package="0402-RES" value="5.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FL1" library="STMicroelectronics - ECMF02-4CMX8" package="STMICROELECTRONICS_ECMF02-4CMX8_0" value="STMICROELECTRONICS_ECMF02-4CMX8STMICROELECTRONICS_ECMF02-4CMX8_0_0">
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="DATASHEET" value="https://www.st.com/resource/en/datasheet/ecmf02-4cmx8.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Passive Components"/>
<attribute name="DEVICE_CLASS_L2" value="EMI / RFI Components"/>
<attribute name="DEVICE_CLASS_L3" value="Common Mode Chokes"/>
<attribute name="DIGIKEY_DESCRIPTION" value="COMMON MODE CHOKE 2LN SMD ESD"/>
<attribute name="DIGIKEY_PART_NUMBER" value="497-13420-1-ND"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+125°C"/>
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MFG_PACKAGE_IDENT" value="Micro QFN-8L"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="1cb8684c97c5681f"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="ECMF02 Series 1 mA 4 Ohm USB 2.0 ESD Protection Common Mode Filter - UQFN-8"/>
<attribute name="MOUSER_PART_NUMBER" value="511-ECMF02-4CMX8"/>
<attribute name="MPN" value="ECMF02-4CMX8"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="Micro QFN-8L"/>
<attribute name="PREFIX" value="FL"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="SERIES_RESISTANCE" value="3Ω"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+125°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C1" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="Samtec - FTSH-105-01-F-DV" package="SAMTEC_FTSH-105-01-F-DV_0" value="SAMTEC_FTSH-105-01-F-DVSAMTEC_FTSH-105-01-F-DV_0_0">
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CONN_GENDER" value="Male"/>
<attribute name="CONN_ORIENTATION" value="Vertical"/>
<attribute name="CONTACT_MATERIAL" value="Tin,Nickel"/>
<attribute name="CURRENT_RATING" value="3.4A"/>
<attribute name="DATASHEET" value="http://suddendocs.samtec.com/prints/ftsh-1xx-xx-xxx-dv-xxx-xxx-mkt.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Connectors"/>
<attribute name="DEVICE_CLASS_L2" value="Headers and Wire Housings"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="CONN HEADER 10POS DUAL .05&quot; SMD"/>
<attribute name="DIGIKEY_PART_NUMBER" value="SAM8795-ND"/>
<attribute name="FOOTPRINT_URL" value="http://suddendocs.samtec.com/prints/ftsh-1xx-xx-xxx-dv-xxx-footprint.pdf"/>
<attribute name="HEIGHT" value="6.23mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MF" value="Samtec"/>
<attribute name="MFG_PACKAGE_IDENT" value="FTSH-105-01-F-DV"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_PART_NUMBER" value="200-FTSH10501FDV"/>
<attribute name="MPN" value="FTSH-105-01-F-DV"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CONTACTS" value="10"/>
<attribute name="NUMBER_OF_ROWS" value="2"/>
<attribute name="PACKAGE" value="HDR10"/>
<attribute name="PREFIX" value="J"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.46mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+125°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="R21" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="sfe" package="0402-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="rcl" package="C0201" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D2" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D3" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D4" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D5" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D6" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D7" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D8" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D9" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D10" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D11" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D12" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D13" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D15" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D16" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D17" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D18" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D19" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="U5" library="LSM6DS3" package="PQFN50P300X250X86-14N" value="LSM6DS3TR-C">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Accelerometer, Gyroscope, Temperature, 6 Axis Sensor I²C, SPI Output "/>
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MP" value="LSM6DS3"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="LGA-14 STMicroelectronics"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="sfe" package="0402-RES" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="sfe" package="0402-RES" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U8" library="STMicroelectronics - VL53L1CXV0FY" package="STMICROELECTRONICS_VL53L1CXV0FY-1_0" value="STMICROELECTRONICS_VL53L1CXV0FY-1STMICROELECTRONICS_VL53L1CXV0FY-1_0_0">
<attribute name="AMBIENT_TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="AMBIENT_TEMPERATURE_RANGE_LOW" value="-20°C"/>
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="DATASHEET" value="https://www.st.com/resource/en/datasheet/vl53l1x.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Sensors"/>
<attribute name="DEVICE_CLASS_L2" value="Proximity Sensors"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="SENSOR OPTICAL 4M I2C"/>
<attribute name="DIGIKEY_PART_NUMBER" value="497-17764-1-ND"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="FREQUENCY" value="50Hz"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_SUPPLY_VOLTAGE" value="3.5V"/>
<attribute name="MF" value="STMicroelectronics"/>
<attribute name="MFG_PACKAGE_IDENT" value="LGA12-DM00319387"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="8ae530ee8fafb8d8"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="2"/>
<attribute name="MIN_SUPPLY_VOLTAGE" value="1.6V"/>
<attribute name="MOUSER_DESCRIPTION" value="ToF Proximity 4m Distance"/>
<attribute name="MOUSER_PART_NUMBER" value="511-VL53L1CXV0FY/1"/>
<attribute name="MPN" value="VL53L1CXV0FY/1"/>
<attribute name="NAME"/>
<attribute name="OPERATING_SUPPLY_CURRENT" value="20-16000uA"/>
<attribute name="PACKAGE" value="LGA12"/>
<attribute name="PREFIX" value="U"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="SENSING_DISTANCE" value="4m"/>
<attribute name="SENSING_METHOD" value="IR"/>
<attribute name="SENSOR_OUTPUT" value="I2C"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-20°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C47" library="SparkFun-Capacitors" package="0603" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08280"/>
<attribute name="VALUE" value="4.7uF"/>
</element>
<element name="C48" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U9" library="Z01SDZ" package="NXP_SEMICONDUCTORS_SE050C2HQ1-Z01SDZ_1" value="NXP_SEMICONDUCTORS_SE050C2HQ1-Z01SDZNXP_SEMICONDUCTORS_SE050C2HQ1-Z01SDZ_0_1">
<attribute name="AMBIENT_TEMPERATURE_RANGE_HIGH" value="+105°C"/>
<attribute name="AMBIENT_TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="DATASHEET" value="https://www.nxp.com/docs/en/data-sheet/SE050-DATASHEET.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Integrated Circuits (ICs)"/>
<attribute name="DEVICE_CLASS_L2" value="Interface ICs"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="ECC RSA AES DES MIFARE KDF CL-IF"/>
<attribute name="DIGIKEY_PART_NUMBER" value="568-15378-1-ND"/>
<attribute name="FOOTPRINT_PARAMETERS_1" value="{&quot;fp_type&quot;:&quot;QFN&quot;,&quot;params&quot;:{&quot;N1&quot;:{&quot;nom&quot;:5,&quot;long name&quot;:&quot;Leads on long side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N1&quot;,&quot;type&quot;:&quot;count&quot;},&quot;N2&quot;:{&quot;nom&quot;:5,&quot;long name&quot;:&quot;Leads on wide side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N2&quot;,&quot;type&quot;:&quot;count&quot;},&quot;A&quot;:{&quot;nom&quot;:315000,&quot;long name&quot;:&quot;Height&quot;,&quot;min&quot;:300000,&quot;max&quot;:330000,&quot;short name&quot;:&quot;A&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A1&quot;:{&quot;nom&quot;:25000,&quot;long name&quot;:&quot;Package clearance&quot;,&quot;min&quot;:0,&quot;max&quot;:50000,&quot;short name&quot;:&quot;A1&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A2&quot;:{&quot;nom&quot;:290000,&quot;long name&quot;:&quot;Package height&quot;,&quot;min&quot;:250000,&quot;max&quot;:330000,&quot;short name&quot;:&quot;A2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;D&quot;:{&quot;nom&quot;:3000000,&quot;long name&quot;:&quot;Package length&quot;,&quot;min&quot;:2900000,&quot;max&quot;:3100000,&quot;short name&quot;:&quot;D&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E&quot;:{&quot;nom&quot;:3000000,&quot;long name&quot;:&quot;Package width&quot;,&quot;min&quot;:2900000,&quot;max&quot;:3100000,&quot;short name&quot;:&quot;E&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;B&quot;:{&quot;nom&quot;:200000,&quot;long name&quot;:&quot;Lead width&quot;,&quot;min&quot;:150000,&quot;max&quot;:250000,&quot;short name&quot;:&quot;B&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;C&quot;:{&quot;nom&quot;:100000,&quot;long name&quot;:&quot;Lead thickness&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;C&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;L&quot;:{&quot;nom&quot;:300000,&quot;long name&quot;:&quot;Lead foot length&quot;,&quot;min&quot;:250000,&quot;max&quot;:350000,&quot;short name&quot;:&quot;L&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;e&quot;:{&quot;nom&quot;:400000,&quot;long name&quot;:&quot;Lead pitch&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;e&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;HT&quot;:{&quot;default&quot;:&quot;Yes&quot;,&quot;long name&quot;:&quot;Thermal pad&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;HT&quot;,&quot;children&quot;:[&quot;D2&quot;,&quot;E2&quot;,&quot;PC&quot;]},&quot;offset x&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;X Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset x&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;offset y&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Y Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset y&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;LS&quot;:{&quot;default&quot;:&quot;Rounded rectangle&quot;,&quot;long name&quot;:&quot;Land shape&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS&quot;},&quot;LS1&quot;:{&quot;default&quot;:&quot;Rectangle&quot;,&quot;long name&quot;:&quot;Land shape (Pin 1)&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS1&quot;},&quot;solder toe&quot;:{&quot;nom&quot;:400000,&quot;long name&quot;:&quot;Solder fillet (toe)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder toe&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder heel&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Solder fillet (heel)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder heel&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder side&quot;:{&quot;nom&quot;:-40000,&quot;long name&quot;:&quot;Solder fillet (side)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder side&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;courtyard&quot;:{&quot;nom&quot;:500000,&quot;long name&quot;:&quot;Courtyard&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;courtyard&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;SF&quot;:{&quot;default&quot;:&quot;A&quot;,&quot;long name&quot;:&quot;Packing level&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;SF&quot;,&quot;help&quot;:&quot;http://support.upverter.com/customer/portal/articles/978783-what-is-a-footprint-packing-level&quot;,&quot;children&quot;:[&quot;solder toe&quot;,&quot;solder heel&quot;,&quot;solder side&quot;,&quot;courtyard&quot;]},&quot;D2&quot;:{&quot;nom&quot;:1900000,&quot;long name&quot;:&quot;Thermal pad length&quot;,&quot;min&quot;:1850000,&quot;max&quot;:1950000,&quot;short name&quot;:&quot;D2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E2&quot;:{&quot;nom&quot;:1900000,&quot;long name&quot;:&quot;Thermal pad width&quot;,&quot;min&quot;:1850000,&quot;max&quot;:1950000,&quot;short name&quot;:&quot;E2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;PC&quot;:{&quot;long name&quot;:&quot;Paste coverage (%)&quot;,&quot;type&quot;:&quot;percentage&quot;,&quot;short name&quot;:&quot;PC&quot;,&quot;value&quot;:40}}}"/>
<attribute name="FOOTPRINT_PARAMETERS_2" value="{&quot;fp_type&quot;:&quot;QFN&quot;,&quot;params&quot;:{&quot;N1&quot;:{&quot;nom&quot;:5,&quot;long name&quot;:&quot;Leads on long side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N1&quot;,&quot;type&quot;:&quot;count&quot;},&quot;N2&quot;:{&quot;nom&quot;:5,&quot;long name&quot;:&quot;Leads on wide side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N2&quot;,&quot;type&quot;:&quot;count&quot;},&quot;A&quot;:{&quot;nom&quot;:315000,&quot;long name&quot;:&quot;Height&quot;,&quot;min&quot;:300000,&quot;max&quot;:330000,&quot;short name&quot;:&quot;A&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A1&quot;:{&quot;nom&quot;:25000,&quot;long name&quot;:&quot;Package clearance&quot;,&quot;min&quot;:0,&quot;max&quot;:50000,&quot;short name&quot;:&quot;A1&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A2&quot;:{&quot;nom&quot;:290000,&quot;long name&quot;:&quot;Package height&quot;,&quot;min&quot;:250000,&quot;max&quot;:330000,&quot;short name&quot;:&quot;A2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;D&quot;:{&quot;nom&quot;:3000000,&quot;long name&quot;:&quot;Package length&quot;,&quot;min&quot;:2900000,&quot;max&quot;:3100000,&quot;short name&quot;:&quot;D&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E&quot;:{&quot;nom&quot;:3000000,&quot;long name&quot;:&quot;Package width&quot;,&quot;min&quot;:2900000,&quot;max&quot;:3100000,&quot;short name&quot;:&quot;E&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;B&quot;:{&quot;nom&quot;:200000,&quot;long name&quot;:&quot;Lead width&quot;,&quot;min&quot;:150000,&quot;max&quot;:250000,&quot;short name&quot;:&quot;B&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;C&quot;:{&quot;nom&quot;:100000,&quot;long name&quot;:&quot;Lead thickness&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;C&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;L&quot;:{&quot;nom&quot;:300000,&quot;long name&quot;:&quot;Lead foot length&quot;,&quot;min&quot;:250000,&quot;max&quot;:350000,&quot;short name&quot;:&quot;L&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;e&quot;:{&quot;nom&quot;:400000,&quot;long name&quot;:&quot;Lead pitch&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;e&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;D2&quot;:{&quot;nom&quot;:1900000,&quot;long name&quot;:&quot;Thermal pad length&quot;,&quot;min&quot;:1850000,&quot;max&quot;:1950000,&quot;short name&quot;:&quot;D2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E2&quot;:{&quot;nom&quot;:1900000,&quot;long name&quot;:&quot;Thermal pad width&quot;,&quot;min&quot;:1850000,&quot;max&quot;:1950000,&quot;short name&quot;:&quot;E2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;PC&quot;:{&quot;long name&quot;:&quot;Paste coverage (%)&quot;,&quot;type&quot;:&quot;percentage&quot;,&quot;short name&quot;:&quot;PC&quot;,&quot;value&quot;:40},&quot;HT&quot;:{&quot;default&quot;:&quot;Yes&quot;,&quot;long name&quot;:&quot;Thermal pad&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;HT&quot;,&quot;children&quot;:[&quot;D2&quot;,&quot;E2&quot;,&quot;PC&quot;]},&quot;offset x&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;X Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset x&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;offset y&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Y Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset y&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;LS&quot;:{&quot;default&quot;:&quot;Rounded rectangle&quot;,&quot;long name&quot;:&quot;Land shape&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS&quot;},&quot;LS1&quot;:{&quot;default&quot;:&quot;Rectangle&quot;,&quot;long name&quot;:&quot;Land shape (Pin 1)&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS1&quot;},&quot;solder toe&quot;:{&quot;nom&quot;:300000,&quot;long name&quot;:&quot;Solder fillet (toe)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder toe&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder heel&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Solder fillet (heel)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder heel&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder side&quot;:{&quot;nom&quot;:-40000,&quot;long name&quot;:&quot;Solder fillet (side)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder side&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;courtyard&quot;:{&quot;nom&quot;:250000,&quot;long name&quot;:&quot;Courtyard&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;courtyard&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;SF&quot;:{&quot;default&quot;:&quot;B&quot;,&quot;long name&quot;:&quot;Packing level&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;SF&quot;,&quot;help&quot;:&quot;http://support.upverter.com/customer/portal/articles/978783-what-is-a-footprint-packing-level&quot;,&quot;children&quot;:[&quot;solder toe&quot;,&quot;solder heel&quot;,&quot;solder side&quot;,&quot;courtyard&quot;]}}}"/>
<attribute name="FOOTPRINT_PARAMETERS_3" value="{&quot;fp_type&quot;:&quot;QFN&quot;,&quot;params&quot;:{&quot;N1&quot;:{&quot;nom&quot;:5,&quot;long name&quot;:&quot;Leads on long side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N1&quot;,&quot;type&quot;:&quot;count&quot;},&quot;N2&quot;:{&quot;nom&quot;:5,&quot;long name&quot;:&quot;Leads on wide side&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;N2&quot;,&quot;type&quot;:&quot;count&quot;},&quot;A&quot;:{&quot;nom&quot;:315000,&quot;long name&quot;:&quot;Height&quot;,&quot;min&quot;:300000,&quot;max&quot;:330000,&quot;short name&quot;:&quot;A&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A1&quot;:{&quot;nom&quot;:25000,&quot;long name&quot;:&quot;Package clearance&quot;,&quot;min&quot;:0,&quot;max&quot;:50000,&quot;short name&quot;:&quot;A1&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;A2&quot;:{&quot;nom&quot;:290000,&quot;long name&quot;:&quot;Package height&quot;,&quot;min&quot;:250000,&quot;max&quot;:330000,&quot;short name&quot;:&quot;A2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;D&quot;:{&quot;nom&quot;:3000000,&quot;long name&quot;:&quot;Package length&quot;,&quot;min&quot;:2900000,&quot;max&quot;:3100000,&quot;short name&quot;:&quot;D&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E&quot;:{&quot;nom&quot;:3000000,&quot;long name&quot;:&quot;Package width&quot;,&quot;min&quot;:2900000,&quot;max&quot;:3100000,&quot;short name&quot;:&quot;E&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;B&quot;:{&quot;nom&quot;:200000,&quot;long name&quot;:&quot;Lead width&quot;,&quot;min&quot;:150000,&quot;max&quot;:250000,&quot;short name&quot;:&quot;B&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;C&quot;:{&quot;nom&quot;:100000,&quot;long name&quot;:&quot;Lead thickness&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;C&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;L&quot;:{&quot;nom&quot;:300000,&quot;long name&quot;:&quot;Lead foot length&quot;,&quot;min&quot;:250000,&quot;max&quot;:350000,&quot;short name&quot;:&quot;L&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;e&quot;:{&quot;nom&quot;:400000,&quot;long name&quot;:&quot;Lead pitch&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;e&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;D2&quot;:{&quot;nom&quot;:1900000,&quot;long name&quot;:&quot;Thermal pad length&quot;,&quot;min&quot;:1850000,&quot;max&quot;:1950000,&quot;short name&quot;:&quot;D2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;E2&quot;:{&quot;nom&quot;:1900000,&quot;long name&quot;:&quot;Thermal pad width&quot;,&quot;min&quot;:1850000,&quot;max&quot;:1950000,&quot;short name&quot;:&quot;E2&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;PC&quot;:{&quot;long name&quot;:&quot;Paste coverage (%)&quot;,&quot;type&quot;:&quot;percentage&quot;,&quot;short name&quot;:&quot;PC&quot;,&quot;value&quot;:40},&quot;HT&quot;:{&quot;default&quot;:&quot;Yes&quot;,&quot;long name&quot;:&quot;Thermal pad&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;HT&quot;,&quot;children&quot;:[&quot;D2&quot;,&quot;E2&quot;,&quot;PC&quot;]},&quot;offset x&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;X Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset x&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;offset y&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Y Center offset&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;offset y&quot;,&quot;type&quot;:&quot;measurement&quot;},&quot;LS&quot;:{&quot;default&quot;:&quot;Rounded rectangle&quot;,&quot;long name&quot;:&quot;Land shape&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS&quot;},&quot;LS1&quot;:{&quot;default&quot;:&quot;Rectangle&quot;,&quot;long name&quot;:&quot;Land shape (Pin 1)&quot;,&quot;type&quot;:&quot;multichoice&quot;,&quot;short name&quot;:&quot;LS1&quot;},&quot;solder toe&quot;:{&quot;nom&quot;:200000,&quot;long name&quot;:&quot;Solder fillet (toe)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder toe&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder heel&quot;:{&quot;nom&quot;:0,&quot;long name&quot;:&quot;Solder fillet (heel)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder heel&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;solder side&quot;:{&quot;nom&quot;:-40000,&quot;long name&quot;:&quot;Solder fillet (side)&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;solder side&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;courtyard&quot;:{&quot;nom&quot;:100000,&quot;long name&quot;:&quot;Courtyard&quot;,&quot;min&quot;:null,&quot;max&quot;:null,&quot;short name&quot;:&quot;courtyard&quot;,&quot;type&quot;:&quot;fixedmeasurement&quot;},&quot;SF&quot;:{&quot;default&quot;:&quot;C&quot;,&quot;long name&quot;:&quot;Packing level&quot;,&quot;type&quot;:&quot;multichoiceparent&quot;,&quot;short name&quot;:&quot;SF&quot;,&quot;help&quot;:&quot;http://support.upverter.com/customer/portal/articles/978783-what-is-a-footprint-packing-level&quot;,&quot;children&quot;:[&quot;solder toe&quot;,&quot;solder heel&quot;,&quot;solder side&quot;,&quot;courtyard&quot;]}}}"/>
<attribute name="FOOTPRINT_URL" value="https://www.nxp.com/docs/en/package-information/SOT1969-1.pdf"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="FOOTPRINT_VARIANT_NAME_1" value="IPC_A"/>
<attribute name="FOOTPRINT_VARIANT_NAME_2" value="IPC_B"/>
<attribute name="FOOTPRINT_VARIANT_NAME_3" value="IPC_C"/>
<attribute name="HEIGHT" value="0.33mm"/>
<attribute name="INTERFACE" value="I2C,UART"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MAX_SUPPLY_VOLTAGE" value="3.6V"/>
<attribute name="MF" value="NXP Semiconductors"/>
<attribute name="MFG_PACKAGE_IDENT" value="SOT1969-1"/>
<attribute name="MFG_PACKAGE_IDENT_COMPONENT_ID" value="9e2fe40fc878a527"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="05/2019"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MIN_SUPPLY_VOLTAGE" value="1.62V"/>
<attribute name="MOUSER_PART_NUMBER" value="771-SE050C2HQ1Z01SDZ"/>
<attribute name="MPN" value="SE050C2HQ1/Z01SDZ"/>
<attribute name="NAME"/>
<attribute name="NOMINAL_SUPPLY_CURRENT" value="430-14400uA"/>
<attribute name="PACKAGE" value="HX2QFN20"/>
<attribute name="PREFIX" value="U"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="STANDOFF_HEIGHT" value="0mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+105°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C49" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="sfe" package="0402-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="sfe" package="0402-RES" value="1.8K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D14" library="SparkFun-LED" package="LED-0603" value="RED (SML-D12V1WT86)">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-00819"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="sfe" package="0402-RES" value="1.5K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="sfe" package="0402-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C57" library="sfe" package="0402-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="leptonCustom" package="SOT23-5" value="ME6211C18M5G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="sfe" package="0402-RES" value="435K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U11" library="Texas Instruments - BQ24072TRGTR" package="TEXAS_INSTRUMENTS_BQ24072TRGTR_0" value="TEXAS_INSTRUMENTS_BQ24072TRGTRTEXAS_INSTRUMENTS_BQ24072TRGTR_0_0">
<attribute name="CIIVA_IDS" value="1416690"/>
<attribute name="CODE__JEDEC" value="MO-220"/>
<attribute name="DATASHEET" value="http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=BQ24072T&amp;fileType=pdf"/>
<attribute name="DATASHEET_VERSION" value="SLUS937A"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Manufacturer Recommended"/>
<attribute name="IMPORTED" value="yes"/>
<attribute name="IMPORTED_FROM" value="vault"/>
<attribute name="IMPORT_TS" value="1521843159"/>
<attribute name="LEAD_ACID" value="N"/>
<attribute name="LI__ION" value="Y"/>
<attribute name="LI__POLYMER" value="Y"/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MOUNTING_TECHNOLOGY" value="Surface Mount"/>
<attribute name="MPN" value="BQ24072TRGTR"/>
<attribute name="NAME"/>
<attribute name="NI_CD" value="N"/>
<attribute name="NI_MH" value="N"/>
<attribute name="OVER_VOLTAGE_PROTECTION" value="N"/>
<attribute name="PACKAGE" value="RGT0016C"/>
<attribute name="PACKAGE_DESCRIPTION" value="16-Pin Plastic Quad Flat No-Lead, 3 x 3 mm Body, 0.5 mm Pitch, 1.7 x 1.7 mm Exposed Pad"/>
<attribute name="PACKAGE_VERSION" value="revH, Oct-2011"/>
<attribute name="PREFIX" value="U"/>
<attribute name="RELEASE_DATE" value="1464339320"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="SUB_FAMILY" value="Battery Charge Management"/>
<attribute name="VAULT_GUID" value="C57694E4-D7CE-4F6A-B4D6-227FFECCAB15"/>
<attribute name="VAULT_REVISION" value="7F5595AE-654F-4CD5-AF4A-A259C64C5444"/>
<attribute name="VIN_MIN_V" value="4.3"/>
</element>
<element name="C53" library="SparkFun-Capacitors" package="0603" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08280"/>
<attribute name="VALUE" value="4.7uF"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08280"/>
<attribute name="VALUE" value="4.7uF"/>
</element>
<element name="C51" library="sfe" package="0402-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="sfe" package="SOT23-3" value="AO3401">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D20" library="sfe" package="SOD-323" value="BAT60BE6327">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="sfe" package="0402-RES" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D21" library="Vishay - VCUT05E1-SD0-G4-08" package="VISHAY_VCUT05E1-SD0-G4-08_0" value="VISHAY_VCUT05E1-SD0-G4-08VISHAY_VCUT05E1-SD0-G4-08_0_0">
<attribute name="BREAKDOWN_VOLTAGE" value="8V"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CLAMPING_VOLTAGE" value="11V"/>
<attribute name="DATASHEET" value="http://www.vishay.com/docs/85900/vcut05e1-sd0.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Circuit Protection"/>
<attribute name="DEVICE_CLASS_L2" value="TVS Diodes"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE TVS DIODE 5.5V 11V CLP0603"/>
<attribute name="DIGIKEY_PART_NUMBER" value="VCUT05E1-SD0-G4-08GICT-ND"/>
<attribute name="DIRECTION" value="Bidirectional"/>
<attribute name="FOOTPRINT_URL" value="http://www.vishay.com/docs/85917/soldrecclp.pdf"/>
<attribute name="HEIGHT" value="0.3mm"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MAX_JUNCTION_TEMP" value="+150°C"/>
<attribute name="MF" value="Vishay"/>
<attribute name="MFG_PACKAGE_IDENT" value="S8-V-3906.04-023"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="11/2016"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="8"/>
<attribute name="MOUSER_PART_NUMBER" value="78-VCUT05E1SD0G408"/>
<attribute name="MPN" value="VCUT05E1-SD0-G4-08"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CHANNELS" value="1"/>
<attribute name="PACKAGE" value="CLP0603-2L"/>
<attribute name="PEAK_PULSE_CURRENT" value="6A"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_STANDOFF_VOLTAGE" value="5.5V"/>
<attribute name="ROHS" value="yes"/>
<attribute name="STANDOFF_HEIGHT" value="0.01mm"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+150°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-55°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="C5" library="sfe" package="EIA3216" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D22" library="Cree - CLM3C-WKW-CWBYA453" package="CREE_CLM3C-WKW-CWBYA453_0" value="CREE_CLM3C-WKW-CWBYA453CREE_CLM3C-WKW-CWBYA453_0_0">
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLOUR" value="White"/>
<attribute name="DATASHEET" value="https://www.cree.com/led-components/media/documents/CLM3C-1076.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Optoelectronics"/>
<attribute name="DEVICE_CLASS_L2" value="LEDs"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE LED COOL WHITE DIFF 2PLCC SMD"/>
<attribute name="DIGIKEY_PART_NUMBER" value="CLM3C-WKW-CWBYA453CT-ND"/>
<attribute name="FOOTPRINT_URL" value="https://www.cree.com/led-components/media/documents/sh-HB.pdf"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="FORWARD_CURRENT" value="20mA"/>
<attribute name="FORWARD_VOLTAGE" value="3.2V"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="LED_ORIENTATION" value="Top View"/>
<attribute name="LUMINOUS_FLUX" value="4.2lm"/>
<attribute name="LUMINOUS_INTENSITY" value="1850mcd"/>
<attribute name="MAX_JUNCTION_TEMP" value="+110°C"/>
<attribute name="MF" value="Cree"/>
<attribute name="MFG_PACKAGE_IDENT" value="CLM3C-WKW"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Standard LEDs - SMD White LED"/>
<attribute name="MOUSER_PART_NUMBER" value="941-CLM3CWKWCWBYA453"/>
<attribute name="MPN" value="CLM3C-WKW-CWBYA453"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SMD2"/>
<attribute name="POWER_DISSIPATION" value="100mW"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_VOLTAGE" value="5V"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+100°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D23" library="Cree - CLM3C-WKW-CWBYA453" package="CREE_CLM3C-WKW-CWBYA453_0" value="CREE_CLM3C-WKW-CWBYA453CREE_CLM3C-WKW-CWBYA453_0_0">
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLOUR" value="White"/>
<attribute name="DATASHEET" value="https://www.cree.com/led-components/media/documents/CLM3C-1076.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Optoelectronics"/>
<attribute name="DEVICE_CLASS_L2" value="LEDs"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="DIODE LED COOL WHITE DIFF 2PLCC SMD"/>
<attribute name="DIGIKEY_PART_NUMBER" value="CLM3C-WKW-CWBYA453CT-ND"/>
<attribute name="FOOTPRINT_URL" value="https://www.cree.com/led-components/media/documents/sh-HB.pdf"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="FORWARD_CURRENT" value="20mA"/>
<attribute name="FORWARD_VOLTAGE" value="3.2V"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="LED_ORIENTATION" value="Top View"/>
<attribute name="LUMINOUS_FLUX" value="4.2lm"/>
<attribute name="LUMINOUS_INTENSITY" value="1850mcd"/>
<attribute name="MAX_JUNCTION_TEMP" value="+110°C"/>
<attribute name="MF" value="Cree"/>
<attribute name="MFG_PACKAGE_IDENT" value="CLM3C-WKW"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="Standard LEDs - SMD White LED"/>
<attribute name="MOUSER_PART_NUMBER" value="941-CLM3CWKWCWBYA453"/>
<attribute name="MPN" value="CLM3C-WKW-CWBYA453"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SMD2"/>
<attribute name="POWER_DISSIPATION" value="100mW"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_VOLTAGE" value="5V"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+100°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.1"/>
</element>
<element name="D24" library="Cree - UHD1110-FKA-CL1A13R3Q1BBQFMF3" package="CREE_UHD1110-FKA-CL1A13R3Q1BBQFMF3_0" value="CREE_UHD1110-FKA-CL1A13R3Q1BBQFMF3CREE_UHD1110-FKA-CL1A13R3Q1BBQFMF3_0_0">
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="COLOUR" value="Red, Green, Blue"/>
<attribute name="DATASHEET" value="https://cree-led.com/media/documents/ds-UHD1110-FKA.pdf"/>
<attribute name="DEVICE_CLASS_L1" value="Optoelectronics"/>
<attribute name="DEVICE_CLASS_L2" value="LEDs"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIGIKEY_DESCRIPTION" value="HB, SMD, RGB"/>
<attribute name="DIGIKEY_PART_NUMBER" value="UHD1110-FKA-CL1A13R3Q1BBQFMF3CT-ND"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="FORWARD_CURRENT" value="5mA"/>
<attribute name="FORWARD_VOLTAGE" value="1.9/2.9/2.9V"/>
<attribute name="HEIGHT" value="0.7mm"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="LED_ORIENTATION" value="Top View"/>
<attribute name="LUMINOUS_INTENSITY" value="78/106/24mcd"/>
<attribute name="MAX_JUNCTION_TEMP" value="+110°C"/>
<attribute name="MF" value="Cree"/>
<attribute name="MFG_PACKAGE_IDENT" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_PART_NUMBER" value="941-UHD0FKAC11BQFMF3"/>
<attribute name="MPN" value="UHD1110-FKA-CL1A13R3Q1BBQFMF3"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0404"/>
<attribute name="POWER_DISSIPATION" value="25/36/36mW"/>
<attribute name="PREFIX" value="D"/>
<attribute name="REVERSE_VOLTAGE" value="5V"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
<attribute name="WAVELENGTH" value="621.5/529.5/468.5nm"/>
</element>
<element name="J6" library="HIROSE - U.FL-R-SMT-1(10)" package="HIROSE_U_FL-R-SMT-1_10_0" value="2337019-1">
<attribute name="AUTOMOTIVE" value="No"/>
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CONN_ORIENTATION" value="Straight"/>
<attribute name="CONTACT_MATERIAL" value="Gold,Silver"/>
<attribute name="DATASHEET" value="https://www.hirose.com/product/document?clcode=CL0331-0472-2-10&amp;productname=U.FL-R-SMT-1(10)&amp;series=U.FL&amp;documenttype=Catalog&amp;lang=en&amp;documentid=D31697_en"/>
<attribute name="DEVICE_CLASS_L1" value="Connectors"/>
<attribute name="DEVICE_CLASS_L2" value="RF / Coaxial Connectors"/>
<attribute name="DEVICE_CLASS_L3" value="unset"/>
<attribute name="DIELECTRIC_MATERIAL" value="LCP"/>
<attribute name="DIGIKEY_DESCRIPTION" value="CONN U.FL RCPT STR 50 OHM SMD"/>
<attribute name="DIGIKEY_PART_NUMBER" value="H11891CT-ND"/>
<attribute name="FOOTPRINT_URL" value="https://www.hirose.com/product/document?clcode=CL0331-0472-2-10&amp;productname=U.FL-R-SMT-1(10)&amp;series=U.FL&amp;documenttype=2DDrawing&amp;lang=en&amp;documentid=0000940684"/>
<attribute name="FOOTPRINT_VARIANT_NAME_0" value="Recommended_Land_Pattern"/>
<attribute name="FREQUENCY" value="8GHz"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="IMPEDANCE" value="50Ω"/>
<attribute name="IS_FEMALE" value="yes"/>
<attribute name="LEAD_FREE" value="Yes"/>
<attribute name="MF" value="HIROSE"/>
<attribute name="MFG_PACKAGE_IDENT" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_DATE" value="0"/>
<attribute name="MFG_PACKAGE_IDENT_REV" value="0"/>
<attribute name="MOUSER_DESCRIPTION" value="HIROSE(HRS) - U.FL-R-SMT-1(10) - RF COAXIAL, U.FL, STRAIGHT JACK, 50OHM"/>
<attribute name="MOUSER_PART_NUMBER" value="798-U.FL-R-SMT-110"/>
<attribute name="MPN" value="U.FL-R-SMT-1(10)"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_CONTACTS" value="1"/>
<attribute name="PACKAGE" value="CONN_RF_2MM6_2MM6"/>
<attribute name="PREFIX" value="J"/>
<attribute name="ROHS" value="Yes"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+105°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-40°C"/>
<attribute name="VERIFICATION_VERSION" value="0.0.0.3"/>
</element>
<element name="C32" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="SparkFun-Capacitors" package="0603" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08280"/>
<attribute name="VALUE"/>
</element>
<element name="C54" library="SparkFun-Capacitors" package="0603" value="4.7uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08280"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="sfe" package="0402-RES" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="sfe" package="0402-RES" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="sfe" package="0402-RES" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="sfe" package="0402-RES" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="sfe" package="0402-RES" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="Q1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U4" pad="2"/>
<contactref element="C6" pad="C"/>
<contactref element="X3" pad="19"/>
<contactref element="X3" pad="27"/>
<contactref element="X3" pad="5"/>
<contactref element="C19" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C16" pad="C"/>
<contactref element="C25" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="U10" pad="K7"/>
<contactref element="U10" pad="G6"/>
<contactref element="U10" pad="G8"/>
<contactref element="U10" pad="H12"/>
<contactref element="U10" pad="J10"/>
<contactref element="U10" pad="M9"/>
<contactref element="U10" pad="G2"/>
<contactref element="U10" pad="F9"/>
<contactref element="U10" pad="J7"/>
<contactref element="U10" pad="F6"/>
<contactref element="U10" pad="H10"/>
<contactref element="U10" pad="M8"/>
<contactref element="U10" pad="F2"/>
<contactref element="U10" pad="D9"/>
<contactref element="U10" pad="F8"/>
<contactref element="U10" pad="G12"/>
<contactref element="U10" pad="H7"/>
<contactref element="U10" pad="K9"/>
<contactref element="U10" pad="L4"/>
<contactref element="U10" pad="G10"/>
<contactref element="U10" pad="K6"/>
<contactref element="U10" pad="F12"/>
<contactref element="U10" pad="D8"/>
<contactref element="U10" pad="J9"/>
<contactref element="U10" pad="K8"/>
<contactref element="U10" pad="G7"/>
<contactref element="U10" pad="F10"/>
<contactref element="U10" pad="J6"/>
<contactref element="U10" pad="H9"/>
<contactref element="U10" pad="J8"/>
<contactref element="U10" pad="F7"/>
<contactref element="U10" pad="K10"/>
<contactref element="U10" pad="G9"/>
<contactref element="U10" pad="D5"/>
<contactref element="U10" pad="H6"/>
<contactref element="U10" pad="H8"/>
<contactref element="U10" pad="D7"/>
<contactref element="U10" pad="N1"/>
<contactref element="U10" pad="M1"/>
<contactref element="U14" pad="F1"/>
<contactref element="U14" pad="L3"/>
<contactref element="U14" pad="R3"/>
<contactref element="U14" pad="A3"/>
<contactref element="U14" pad="B8"/>
<contactref element="U14" pad="L9"/>
<contactref element="U14" pad="N1"/>
<contactref element="U14" pad="P8"/>
<contactref element="U14" pad="B3"/>
<contactref element="U14" pad="D1"/>
<contactref element="U14" pad="M1"/>
<contactref element="U14" pad="C1"/>
<contactref element="U14" pad="E9"/>
<contactref element="U14" pad="P3"/>
<contactref element="C12" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="9"/>
<contactref element="C31" pad="2"/>
<contactref element="U2" pad="GND"/>
<contactref element="X2" pad="CD$2"/>
<contactref element="X2" pad="P$6"/>
<contactref element="X2" pad="G$1"/>
<contactref element="X2" pad="G$2"/>
<contactref element="X2" pad="G$3"/>
<contactref element="X2" pad="G$4"/>
<contactref element="C7" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="U6" pad="33"/>
<contactref element="C35" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="Y0" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="Y1" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="R18" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="L7" pad="2"/>
<contactref element="J1" pad="B12"/>
<contactref element="J1" pad="B1"/>
<contactref element="J1" pad="A1"/>
<contactref element="J1" pad="A12"/>
<contactref element="R1" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="FL1" pad="5"/>
<contactref element="FL1" pad="8"/>
<contactref element="C9" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="J2" pad="9"/>
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="5"/>
<contactref element="R22" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="C43" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J5" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="D6" pad="2"/>
<contactref element="D12" pad="2"/>
<contactref element="D11" pad="2"/>
<contactref element="D10" pad="2"/>
<contactref element="D9" pad="2"/>
<contactref element="D8" pad="2"/>
<contactref element="D7" pad="2"/>
<contactref element="D13" pad="2"/>
<contactref element="D19" pad="2"/>
<contactref element="D18" pad="2"/>
<contactref element="D17" pad="2"/>
<contactref element="D16" pad="2"/>
<contactref element="D15" pad="2"/>
<contactref element="U5" pad="7"/>
<contactref element="U5" pad="6"/>
<contactref element="U5" pad="3"/>
<contactref element="U5" pad="2"/>
<contactref element="U5" pad="1"/>
<contactref element="C46" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U8" pad="2"/>
<contactref element="U8" pad="3"/>
<contactref element="U8" pad="4"/>
<contactref element="U8" pad="6"/>
<contactref element="U8" pad="12"/>
<contactref element="C48" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="D5" pad="1"/>
<contactref element="U9" pad="19"/>
<contactref element="U9" pad="1"/>
<contactref element="U9" pad="17"/>
<contactref element="U9" pad="21"/>
<contactref element="C49" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="X4" pad="2"/>
<contactref element="R29" pad="2"/>
<contactref element="R32" pad="2"/>
<contactref element="C56" pad="1"/>
<contactref element="C57" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="U11" pad="8"/>
<contactref element="U11" pad="17"/>
<contactref element="U11" pad="17-2"/>
<contactref element="U11" pad="15"/>
<contactref element="C53" pad="1"/>
<contactref element="U11" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="U11" pad="5"/>
<contactref element="R30" pad="1"/>
<contactref element="D21" pad="2"/>
<contactref element="C5" pad="C"/>
<contactref element="U7" pad="1"/>
<contactref element="U7" pad="12"/>
<contactref element="U7" pad="21"/>
<contactref element="U7" pad="40"/>
<contactref element="U7" pad="44"/>
<contactref element="U7" pad="35"/>
<contactref element="U7" pad="42"/>
<contactref element="U7" pad="19"/>
<contactref element="U7" pad="29"/>
<contactref element="U7" pad="45"/>
<contactref element="U7" pad="46"/>
<contactref element="U7" pad="43"/>
<contactref element="C38" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="J6" pad="3"/>
<contactref element="J6" pad="2"/>
<contactref element="C41" pad="2"/>
<contactref element="U7" pad="32"/>
<contactref element="U7" pad="33"/>
<contactref element="C32" pad="2"/>
<contactref element="C52" pad="2"/>
<contactref element="C54" pad="2"/>
</signal>
<signal name="NRST">
<contactref element="J2" pad="10"/>
<contactref element="C15" pad="1"/>
<contactref element="U10" pad="J1"/>
<contactref element="R24" pad="1"/>
<contactref element="J5" pad="8"/>
<contactref element="D4" pad="2"/>
</signal>
<signal name="SWDIO">
<contactref element="U10" pad="A15"/>
<contactref element="J2" pad="2"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="SWCLK">
<contactref element="U10" pad="A14"/>
<contactref element="J2" pad="4"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="BOOT0">
<contactref element="U10" pad="D6"/>
<contactref element="R25" pad="2"/>
<contactref element="J5" pad="7"/>
<contactref element="D15" pad="1"/>
</signal>
<signal name="VBUS">
<contactref element="R13" pad="2"/>
<contactref element="L6" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="FL1" pad="1"/>
<contactref element="U11" pad="13"/>
<contactref element="C51" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="LED2" pad="A"/>
<contactref element="C3" pad="2"/>
<contactref element="L1" pad="2"/>
<contactref element="C6" pad="A"/>
<contactref element="X3" pad="10"/>
<contactref element="X3" pad="20"/>
<contactref element="X3" pad="30"/>
<contactref element="X3" pad="36"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="X3" pad="2"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C16" pad="A"/>
<contactref element="C30" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="U10" pad="C6"/>
<contactref element="U10" pad="C1"/>
<contactref element="U10" pad="H13"/>
<contactref element="U10" pad="G3"/>
<contactref element="U10" pad="J12"/>
<contactref element="U10" pad="N8"/>
<contactref element="U10" pad="G13"/>
<contactref element="U10" pad="C7"/>
<contactref element="U10" pad="C5"/>
<contactref element="U10" pad="F3"/>
<contactref element="U10" pad="C8"/>
<contactref element="U10" pad="N9"/>
<contactref element="U10" pad="N10"/>
<contactref element="U10" pad="J13"/>
<contactref element="U10" pad="K4"/>
<contactref element="U10" pad="C9"/>
<contactref element="U14" pad="F9"/>
<contactref element="U14" pad="L7"/>
<contactref element="U14" pad="A7"/>
<contactref element="U14" pad="R7"/>
<contactref element="U14" pad="M9"/>
<contactref element="U14" pad="C9"/>
<contactref element="U14" pad="E1"/>
<contactref element="U14" pad="B2"/>
<contactref element="U14" pad="P2"/>
<contactref element="U14" pad="B7"/>
<contactref element="U14" pad="L1"/>
<contactref element="U14" pad="N9"/>
<contactref element="U14" pad="D9"/>
<contactref element="U14" pad="P7"/>
<contactref element="R8" pad="1"/>
<contactref element="L2" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="C31" pad="1"/>
<contactref element="U2" pad="P$15"/>
<contactref element="U2" pad="P$16"/>
<contactref element="X2" pad="P$4"/>
<contactref element="C7" pad="1"/>
<contactref element="U6" pad="20"/>
<contactref element="U6" pad="32"/>
<contactref element="C33" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U6" pad="21"/>
<contactref element="U6" pad="23"/>
<contactref element="Y0" pad="4"/>
<contactref element="C36" pad="1"/>
<contactref element="Y1" pad="4"/>
<contactref element="C37" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="C43" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="U5" pad="5"/>
<contactref element="U5" pad="8"/>
<contactref element="U5" pad="12"/>
<contactref element="R26" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="C48" pad="1"/>
<contactref element="U8" pad="1"/>
<contactref element="U8" pad="11"/>
<contactref element="C47" pad="1"/>
<contactref element="U8" pad="5"/>
<contactref element="U9" pad="15"/>
<contactref element="U9" pad="12"/>
<contactref element="U9" pad="14"/>
<contactref element="U9" pad="18"/>
<contactref element="U9" pad="13"/>
<contactref element="U9" pad="3"/>
<contactref element="U9" pad="16"/>
<contactref element="C49" pad="1"/>
<contactref element="C50" pad="1"/>
<contactref element="X3" pad="4"/>
<contactref element="C56" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="1"/>
<contactref element="R34" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="D5" pad="2"/>
<contactref element="U6" pad="11"/>
<contactref element="U6" pad="8"/>
<contactref element="U6" pad="14"/>
<contactref element="C5" pad="A"/>
<contactref element="D22" pad="1"/>
<contactref element="D23" pad="1"/>
<contactref element="D24" pad="4"/>
</signal>
<signal name="DCMI_D0">
<contactref element="X3" pad="31"/>
<contactref element="U10" pad="E15"/>
</signal>
<signal name="DCMI_D1">
<contactref element="X3" pad="29"/>
<contactref element="U10" pad="D15"/>
</signal>
<signal name="DCMI_PCLK">
<contactref element="X3" pad="14"/>
<contactref element="U10" pad="P3"/>
</signal>
<signal name="DCMI_HSYNC">
<contactref element="X3" pad="18"/>
<contactref element="U10" pad="N4"/>
</signal>
<signal name="DCMI_VSYNC">
<contactref element="X3" pad="16"/>
<contactref element="U10" pad="C10"/>
</signal>
<signal name="DCMI_CLK">
<contactref element="X3" pad="12"/>
<contactref element="U10" pad="F15"/>
</signal>
<signal name="DCMI_RST">
<contactref element="X3" pad="21"/>
<contactref element="R21" pad="2"/>
<contactref element="U10" pad="D1"/>
</signal>
<signal name="DCMI_PWDN">
<contactref element="X3" pad="25"/>
<contactref element="U10" pad="D2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="DCMI_D2">
<contactref element="X3" pad="35"/>
<contactref element="U10" pad="B10"/>
</signal>
<signal name="DCMI_D3">
<contactref element="X3" pad="28"/>
<contactref element="U10" pad="B9"/>
</signal>
<signal name="DCMI_D4">
<contactref element="X3" pad="26"/>
<contactref element="U10" pad="B1"/>
</signal>
<signal name="DCMI_D5">
<contactref element="X3" pad="33"/>
</signal>
<signal name="DCMI_D6">
<contactref element="X3" pad="24"/>
<contactref element="U10" pad="B2"/>
</signal>
<signal name="DCMI_D7">
<contactref element="X3" pad="22"/>
<contactref element="U10" pad="B3"/>
</signal>
<signal name="SDIO_D0">
<contactref element="U10" pad="G14"/>
<contactref element="U2" pad="P$7"/>
</signal>
<signal name="SDIO_D1">
<contactref element="U10" pad="F14"/>
<contactref element="U2" pad="P$8"/>
</signal>
<signal name="SDIO_D2">
<contactref element="U10" pad="B14"/>
<contactref element="U2" pad="P$3"/>
</signal>
<signal name="SDIO_CLK">
<contactref element="U10" pad="A12"/>
<contactref element="U2" pad="P$6"/>
</signal>
<signal name="SDIO_CMD">
<contactref element="U10" pad="D12"/>
<contactref element="U2" pad="P$5"/>
</signal>
<signal name="LED_G">
<contactref element="U10" pad="N2"/>
<contactref element="R36" pad="2"/>
</signal>
<signal name="LED_B">
<contactref element="U10" pad="P2"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="LED_R">
<contactref element="U10" pad="N3"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="TIM3_CH1">
<contactref element="U10" pad="H15"/>
<contactref element="J5" pad="3"/>
<contactref element="D19" pad="1"/>
</signal>
<signal name="TIM3_CH2">
<contactref element="U10" pad="G15"/>
<contactref element="J5" pad="4"/>
<contactref element="D18" pad="1"/>
</signal>
<signal name="SDIO_D3">
<contactref element="U10" pad="B13"/>
<contactref element="U2" pad="P$4"/>
</signal>
<signal name="LED_R_INT">
<contactref element="D24" pad="3"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="LED_IR">
<contactref element="U10" pad="M11"/>
<contactref element="Q1" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="SPI2_SCLK">
<contactref element="U10" pad="B15"/>
<contactref element="J4" pad="6"/>
<contactref element="D9" pad="1"/>
</signal>
<signal name="I2C2_SCL">
<contactref element="U10" pad="H4"/>
<contactref element="R6" pad="2"/>
<contactref element="X3" pad="32"/>
</signal>
<signal name="I2C2_SDA">
<contactref element="U10" pad="J4"/>
<contactref element="R7" pad="2"/>
<contactref element="X3" pad="34"/>
</signal>
<signal name="RAW">
<contactref element="C2" pad="2"/>
<contactref element="U4" pad="3"/>
<contactref element="U4" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="D20" pad="1"/>
</signal>
<signal name="ADC">
<contactref element="U10" pad="P5"/>
<contactref element="J4" pad="2"/>
<contactref element="D13" pad="1"/>
</signal>
<signal name="SPI2_NSS">
<contactref element="U10" pad="C15"/>
<contactref element="J4" pad="5"/>
<contactref element="D10" pad="1"/>
</signal>
<signal name="SPI2_MISO">
<contactref element="U10" pad="M4"/>
<contactref element="J4" pad="7"/>
<contactref element="D8" pad="1"/>
</signal>
<signal name="SPI2_MOSI">
<contactref element="U10" pad="M3"/>
<contactref element="J4" pad="8"/>
<contactref element="D7" pad="1"/>
</signal>
<signal name="LED_IR_DRIVE_1">
<contactref element="LED3" pad="A"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="LED_G_INT">
<contactref element="D24" pad="2"/>
<contactref element="R36" pad="1"/>
</signal>
<signal name="SW">
<contactref element="L1" pad="1"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="P10">
<contactref element="X3" pad="23"/>
<contactref element="R22" pad="2"/>
<contactref element="U10" pad="C11"/>
<contactref element="J5" pad="6"/>
<contactref element="D16" pad="1"/>
</signal>
<signal name="WIFI_D2/SWO">
<contactref element="U10" pad="A10"/>
<contactref element="U7" pad="23"/>
<contactref element="R16" pad="1"/>
<contactref element="J2" pad="6"/>
<contactref element="D3" pad="2"/>
</signal>
<signal name="RSVD1">
<contactref element="X3" pad="1"/>
</signal>
<signal name="RSVD2">
<contactref element="X3" pad="3"/>
</signal>
<signal name="RSVD3">
<contactref element="X3" pad="7"/>
</signal>
<signal name="RSVD5">
<contactref element="X3" pad="6"/>
</signal>
<signal name="RSVD6">
<contactref element="X3" pad="8"/>
</signal>
<signal name="RSVD4">
<contactref element="X3" pad="9"/>
</signal>
<signal name="DRAM_D0">
<contactref element="U14" pad="R8"/>
<contactref element="U10" pad="M14"/>
</signal>
<signal name="DRAM_D1">
<contactref element="U14" pad="N7"/>
<contactref element="U10" pad="L14"/>
</signal>
<signal name="DRAM_D2">
<contactref element="U14" pad="R9"/>
<contactref element="U10" pad="B12"/>
</signal>
<signal name="DRAM_D3">
<contactref element="U14" pad="N8"/>
<contactref element="U10" pad="C12"/>
</signal>
<signal name="DRAM_D4">
<contactref element="U14" pad="P9"/>
<contactref element="U10" pad="R8"/>
</signal>
<signal name="DRAM_D5">
<contactref element="U14" pad="M8"/>
<contactref element="U10" pad="P8"/>
<contactref element="U10" pad="D11"/>
</signal>
<signal name="DRAM_D6">
<contactref element="U14" pad="M7"/>
<contactref element="U10" pad="P9"/>
</signal>
<signal name="DRAM_D7">
<contactref element="U14" pad="L8"/>
<contactref element="U10" pad="R9"/>
</signal>
<signal name="DRAM_A0">
<contactref element="U14" pad="G8"/>
<contactref element="U10" pad="E2"/>
</signal>
<signal name="DRAM_A1">
<contactref element="U14" pad="G9"/>
<contactref element="U10" pad="H3"/>
</signal>
<signal name="DRAM_A2">
<contactref element="U14" pad="F7"/>
<contactref element="U10" pad="H2"/>
</signal>
<signal name="DRAM_A3">
<contactref element="U14" pad="F3"/>
<contactref element="U10" pad="J2"/>
</signal>
<signal name="DRAM_A4">
<contactref element="U14" pad="G1"/>
<contactref element="U10" pad="J3"/>
</signal>
<signal name="DRAM_A5">
<contactref element="U14" pad="G2"/>
<contactref element="U10" pad="K3"/>
</signal>
<signal name="DRAM_A6">
<contactref element="U14" pad="G3"/>
<contactref element="U10" pad="P6"/>
</signal>
<signal name="DRAM_A7">
<contactref element="U14" pad="H1"/>
<contactref element="U10" pad="N6"/>
</signal>
<signal name="DRAM_A8">
<contactref element="U14" pad="H2"/>
<contactref element="U10" pad="R7"/>
</signal>
<signal name="DRAM_A9">
<contactref element="U14" pad="J3"/>
<contactref element="U10" pad="P7"/>
</signal>
<signal name="DRAM_A10">
<contactref element="U14" pad="G7"/>
<contactref element="U10" pad="N7"/>
</signal>
<signal name="DRAM_A11">
<contactref element="U14" pad="H9"/>
<contactref element="U10" pad="M7"/>
</signal>
<signal name="DRAM_BA0">
<contactref element="U14" pad="J7"/>
<contactref element="U10" pad="K14"/>
</signal>
<signal name="DRAM_BA1">
<contactref element="U14" pad="H8"/>
<contactref element="U10" pad="K13"/>
</signal>
<signal name="DRAM_RAS">
<contactref element="U14" pad="J9"/>
<contactref element="U10" pad="R6"/>
</signal>
<signal name="DRAM_CAS">
<contactref element="U14" pad="K7"/>
<contactref element="U10" pad="B7"/>
</signal>
<signal name="DRAM_WE">
<contactref element="U14" pad="K8"/>
<contactref element="U10" pad="R3"/>
</signal>
<signal name="DRAM_CS">
<contactref element="R8" pad="2"/>
<contactref element="U14" pad="J8"/>
<contactref element="U10" pad="G4"/>
</signal>
<signal name="DRAM_CLK">
<contactref element="U14" pad="J1"/>
<contactref element="U10" pad="H14"/>
</signal>
<signal name="DRAM_CLKE">
<contactref element="U14" pad="J2"/>
<contactref element="U10" pad="F4"/>
</signal>
<signal name="DRAM_D8">
<contactref element="U14" pad="L2"/>
<contactref element="U10" pad="P10"/>
</signal>
<signal name="DRAM_D9">
<contactref element="U14" pad="M3"/>
<contactref element="U10" pad="R10"/>
</signal>
<signal name="DRAM_D10">
<contactref element="U14" pad="M2"/>
<contactref element="U10" pad="N11"/>
</signal>
<signal name="DRAM_D11">
<contactref element="U14" pad="P1"/>
<contactref element="U10" pad="P11"/>
</signal>
<signal name="DRAM_D12">
<contactref element="U14" pad="N2"/>
<contactref element="U10" pad="R11"/>
</signal>
<signal name="DRAM_D13">
<contactref element="U14" pad="R1"/>
<contactref element="U10" pad="P15"/>
</signal>
<signal name="DRAM_D14">
<contactref element="U14" pad="N3"/>
<contactref element="U10" pad="P14"/>
</signal>
<signal name="DRAM_D15">
<contactref element="U14" pad="R2"/>
<contactref element="U10" pad="N15"/>
</signal>
<signal name="SD_CD">
<contactref element="X2" pad="CD$1"/>
<contactref element="U10" pad="J14"/>
<contactref element="U2" pad="P$1"/>
</signal>
<signal name="DRAM_DQM0">
<contactref element="U14" pad="K9"/>
<contactref element="U10" pad="A4"/>
</signal>
<signal name="DRAM_DQM1">
<contactref element="U14" pad="K1"/>
<contactref element="U10" pad="A3"/>
</signal>
<signal name="DRAM_DQM2">
<contactref element="U14" pad="F8"/>
<contactref element="U10" pad="D4"/>
</signal>
<signal name="DRAM_DQM3">
<contactref element="U14" pad="F2"/>
<contactref element="U10" pad="C4"/>
</signal>
<signal name="DRAM_D16">
<contactref element="U14" pad="E8"/>
<contactref element="U10" pad="M12"/>
</signal>
<signal name="DRAM_D17">
<contactref element="U14" pad="D7"/>
<contactref element="U10" pad="M13"/>
</signal>
<signal name="DRAM_D18">
<contactref element="U14" pad="D8"/>
<contactref element="U10" pad="L13"/>
</signal>
<signal name="DRAM_D19">
<contactref element="U14" pad="B9"/>
<contactref element="U10" pad="L12"/>
</signal>
<signal name="DRAM_D20">
<contactref element="U14" pad="C8"/>
<contactref element="U10" pad="K12"/>
</signal>
<signal name="DRAM_D21">
<contactref element="U14" pad="A9"/>
<contactref element="U10" pad="E12"/>
</signal>
<signal name="DRAM_D22">
<contactref element="U14" pad="C7"/>
<contactref element="U10" pad="E13"/>
</signal>
<signal name="DRAM_D23">
<contactref element="U14" pad="A8"/>
<contactref element="U10" pad="D13"/>
</signal>
<signal name="DRAM_D24">
<contactref element="U14" pad="A2"/>
<contactref element="U10" pad="E14"/>
</signal>
<signal name="DRAM_D25">
<contactref element="U14" pad="C3"/>
<contactref element="U10" pad="D14"/>
</signal>
<signal name="DRAM_D26">
<contactref element="U14" pad="A1"/>
<contactref element="U10" pad="C14"/>
</signal>
<signal name="DRAM_D27">
<contactref element="U14" pad="C2"/>
<contactref element="U10" pad="C13"/>
</signal>
<signal name="DRAM_D28">
<contactref element="U14" pad="B1"/>
<contactref element="U10" pad="C3"/>
</signal>
<signal name="DRAM_D29">
<contactref element="U14" pad="D2"/>
<contactref element="U10" pad="C2"/>
</signal>
<signal name="DRAM_D30">
<contactref element="U14" pad="D3"/>
<contactref element="U10" pad="D3"/>
</signal>
<signal name="DRAM_D31">
<contactref element="U14" pad="E2"/>
<contactref element="U10" pad="E3"/>
</signal>
<signal name="VCAP2">
<contactref element="C12" pad="1"/>
<contactref element="U10" pad="M10"/>
</signal>
<signal name="VCAP1">
<contactref element="C11" pad="1"/>
<contactref element="U10" pad="F13"/>
</signal>
<signal name="VDDA">
<contactref element="C13" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="L2" pad="1"/>
<contactref element="U10" pad="R1"/>
<contactref element="U10" pad="P1"/>
</signal>
<signal name="FLASH_IO0">
<contactref element="U1" pad="5"/>
<contactref element="U10" pad="N14"/>
</signal>
<signal name="FLASH_IO1">
<contactref element="U1" pad="2"/>
<contactref element="U10" pad="N13"/>
</signal>
<signal name="FLASH_IO2">
<contactref element="U1" pad="3"/>
<contactref element="U10" pad="A2"/>
</signal>
<signal name="FLASH_IO3">
<contactref element="U1" pad="7"/>
<contactref element="U10" pad="M15"/>
</signal>
<signal name="FLASH_CLK">
<contactref element="U1" pad="6"/>
<contactref element="U10" pad="L1"/>
</signal>
<signal name="FLASH_!CS">
<contactref element="U1" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="DAT0">
<contactref element="X2" pad="P$7"/>
<contactref element="U2" pad="P$10"/>
</signal>
<signal name="DAT1">
<contactref element="X2" pad="P$8"/>
<contactref element="U2" pad="P$9"/>
</signal>
<signal name="DAT2">
<contactref element="X2" pad="P$1"/>
<contactref element="U2" pad="P$14"/>
</signal>
<signal name="DAT3">
<contactref element="X2" pad="P$2"/>
<contactref element="U2" pad="P$13"/>
</signal>
<signal name="CLK">
<contactref element="X2" pad="P$5"/>
<contactref element="U2" pad="P$11"/>
</signal>
<signal name="CMD">
<contactref element="X2" pad="P$3"/>
<contactref element="U2" pad="P$12"/>
</signal>
<signal name="ULPI_DIR">
<contactref element="U10" pad="E4"/>
<contactref element="U6" pad="31"/>
</signal>
<signal name="RBIAS">
<contactref element="R12" pad="2"/>
<contactref element="U6" pad="24"/>
</signal>
<signal name="FLASH_CS">
<contactref element="U10" pad="J15"/>
</signal>
<signal name="SPI6_SSEL">
<contactref element="X3" pad="11"/>
<contactref element="U10" pad="A13"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="SPI6_SCLK">
<contactref element="X3" pad="13"/>
<contactref element="U10" pad="A8"/>
</signal>
<signal name="SPI6_MOSI">
<contactref element="X3" pad="17"/>
<contactref element="U10" pad="A7"/>
</signal>
<signal name="SPI6_MISO">
<contactref element="U10" pad="B8"/>
<contactref element="X3" pad="15"/>
</signal>
<signal name="ULPI_D3">
<contactref element="U10" pad="R12"/>
<contactref element="U6" pad="6"/>
</signal>
<signal name="ULPI_D4">
<contactref element="U10" pad="R13"/>
<contactref element="U6" pad="7"/>
</signal>
<signal name="ULPI_D5">
<contactref element="U10" pad="P12"/>
<contactref element="U6" pad="9"/>
</signal>
<signal name="ULPI_D6">
<contactref element="U10" pad="P13"/>
<contactref element="U6" pad="10"/>
</signal>
<signal name="WIFI_D0">
<contactref element="U10" pad="R14"/>
<contactref element="U7" pad="24"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="WIFI_D1">
<contactref element="U10" pad="R15"/>
<contactref element="U7" pad="26"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="ULPI_STP">
<contactref element="U10" pad="M2"/>
<contactref element="U6" pad="29"/>
</signal>
<signal name="ULPI_NXT">
<contactref element="U10" pad="M5"/>
<contactref element="U6" pad="2"/>
</signal>
<signal name="WIFI_CLK">
<contactref element="U10" pad="B11"/>
<contactref element="U7" pad="20"/>
</signal>
<signal name="WIFI_CMD">
<contactref element="U10" pad="A11"/>
<contactref element="U7" pad="22"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="32.768KHZ_CLK">
<contactref element="U10" pad="E1"/>
<contactref element="Y0" pad="3"/>
<contactref element="U7" pad="37"/>
</signal>
<signal name="ULPI_D1">
<contactref element="U10" pad="R5"/>
<contactref element="U6" pad="4"/>
</signal>
<signal name="ULPI_D2">
<contactref element="U10" pad="R4"/>
<contactref element="U6" pad="5"/>
</signal>
<signal name="WIFI_D3">
<contactref element="U10" pad="A9"/>
<contactref element="U7" pad="25"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="ULPI_D7">
<contactref element="U10" pad="A6"/>
<contactref element="U6" pad="13"/>
</signal>
<signal name="ULPI_D0">
<contactref element="U6" pad="3"/>
<contactref element="U10" pad="R2"/>
</signal>
<signal name="ULPI_CK">
<contactref element="U10" pad="P4"/>
<contactref element="U6" pad="1"/>
</signal>
<signal name="USBEN">
<contactref element="U6" pad="27"/>
<contactref element="R19" pad="1"/>
<contactref element="U10" pad="F1"/>
</signal>
<signal name="USB_DM">
<contactref element="U6" pad="19"/>
<contactref element="FL1" pad="6"/>
</signal>
<signal name="USB_DP">
<contactref element="U6" pad="18"/>
<contactref element="FL1" pad="7"/>
</signal>
<signal name="VBUS_SENSE">
<contactref element="U6" pad="22"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="I2C1_SCL">
<contactref element="U10" pad="A5"/>
<contactref element="J4" pad="4"/>
<contactref element="D11" pad="1"/>
</signal>
<signal name="I2C1_SDA">
<contactref element="U10" pad="B4"/>
<contactref element="J4" pad="3"/>
<contactref element="D12" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="U7" pad="30"/>
<contactref element="C42" pad="1"/>
<contactref element="U7" pad="36"/>
<contactref element="R9" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="C41" pad="1"/>
<contactref element="C38" pad="1"/>
<contactref element="C54" pad="1"/>
</signal>
<signal name="VIN_LDO">
<contactref element="U7" pad="31"/>
<contactref element="L3" pad="2"/>
<contactref element="C32" pad="1"/>
<contactref element="C52" pad="1"/>
</signal>
<signal name="WL_REG_ON">
<contactref element="U7" pad="28"/>
<contactref element="U10" pad="M6"/>
</signal>
<signal name="WL_HOST_WAKE">
<contactref element="U7" pad="27"/>
<contactref element="U10" pad="N5"/>
</signal>
<signal name="SR)VLX">
<contactref element="U7" pad="34"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="BT_HOST_WAKE">
<contactref element="U7" pad="38"/>
<contactref element="U10" pad="K15"/>
</signal>
<signal name="BT_REG_ON">
<contactref element="U7" pad="14"/>
<contactref element="U10" pad="A1"/>
</signal>
<signal name="UART7_TX">
<contactref element="U7" pad="2"/>
<contactref element="U10" pad="K1"/>
</signal>
<signal name="UART7_RTS">
<contactref element="U7" pad="4"/>
<contactref element="U10" pad="L3"/>
</signal>
<signal name="UART7_CTS">
<contactref element="U7" pad="5"/>
<contactref element="U10" pad="L2"/>
</signal>
<signal name="UART7_RX">
<contactref element="U7" pad="3"/>
<contactref element="U10" pad="K2"/>
</signal>
<signal name="BT_DEV_WAKE">
<contactref element="U7" pad="39"/>
<contactref element="U10" pad="N12"/>
</signal>
<signal name="ANT">
<contactref element="U7" pad="41"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="24MHZ_CLK">
<contactref element="Y1" pad="3"/>
<contactref element="U10" pad="G1"/>
<contactref element="U6" pad="26"/>
</signal>
<signal name="OSCEN">
<contactref element="Y1" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="U10" pad="H1"/>
</signal>
<signal name="VBUS_INT">
<contactref element="L6" pad="1"/>
<contactref element="J1" pad="A4"/>
<contactref element="J1" pad="B4"/>
<contactref element="J1" pad="B9"/>
<contactref element="J1" pad="A9"/>
<contactref element="C1" pad="1"/>
<contactref element="FL1" pad="4"/>
</signal>
<signal name="DN">
<contactref element="J1" pad="A7"/>
<contactref element="J1" pad="B7"/>
<contactref element="FL1" pad="3"/>
</signal>
<signal name="DP">
<contactref element="J1" pad="B6"/>
<contactref element="J1" pad="A6"/>
<contactref element="FL1" pad="2"/>
</signal>
<signal name="SHIELD_INT">
<contactref element="L7" pad="1"/>
<contactref element="J1" pad="S_T1"/>
<contactref element="J1" pad="S_T3"/>
<contactref element="J1" pad="S_T2"/>
<contactref element="J1" pad="S_T4"/>
</signal>
<signal name="CC1">
<contactref element="J1" pad="A5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="CC2">
<contactref element="J1" pad="B5"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="I2C4_SCL">
<contactref element="U10" pad="B6"/>
<contactref element="U5" pad="13"/>
<contactref element="R26" pad="2"/>
<contactref element="U8" pad="10"/>
<contactref element="U9" pad="10"/>
</signal>
<signal name="I2C4_SDA">
<contactref element="U10" pad="B5"/>
<contactref element="U5" pad="14"/>
<contactref element="R27" pad="2"/>
<contactref element="U8" pad="9"/>
<contactref element="U9" pad="9"/>
</signal>
<signal name="P9">
<contactref element="U10" pad="D10"/>
<contactref element="J5" pad="5"/>
<contactref element="D17" pad="1"/>
</signal>
<signal name="1.8V">
<contactref element="U6" pad="28"/>
<contactref element="C35" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="U6" pad="30"/>
<contactref element="C57" pad="2"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="VIN">
<contactref element="J5" pad="2"/>
<contactref element="D6" pad="1"/>
<contactref element="D20" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="CRYPTOEN">
<contactref element="U9" pad="11"/>
<contactref element="U10" pad="L15"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="TS">
<contactref element="R29" pad="1"/>
<contactref element="U11" pad="1"/>
</signal>
<signal name="ISET">
<contactref element="R32" pad="1"/>
<contactref element="U11" pad="16"/>
</signal>
<signal name="FB">
<contactref element="U4" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="BAT">
<contactref element="U11" pad="2"/>
<contactref element="U11" pad="3"/>
<contactref element="X4" pad="1"/>
<contactref element="C53" pad="2"/>
<contactref element="D21" pad="1"/>
</signal>
<signal name="CHG">
<contactref element="D14" pad="C"/>
<contactref element="U11" pad="9"/>
</signal>
<signal name="CHG_LED">
<contactref element="D14" pad="A"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="OUT">
<contactref element="Q2" pad="3"/>
<contactref element="U11" pad="11"/>
<contactref element="U11" pad="10"/>
<contactref element="C4" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="U11" pad="6"/>
</signal>
<signal name="LED_B_INT">
<contactref element="D24" pad="1"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="LED_W_DRIVE_0">
<contactref element="R2" pad="2"/>
<contactref element="D22" pad="2"/>
</signal>
<signal name="LED_W_DRIVE_1">
<contactref element="R31" pad="2"/>
<contactref element="D23" pad="2"/>
</signal>
<signal name="LED_IR_DRIVE_0">
<contactref element="R5" pad="2"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="LED_W_DRIVE">
<contactref element="R2" pad="1"/>
<contactref element="R31" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="LED_DRAIN">
<contactref element="Q1" pad="3"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="LED_IR_DRIVE">
<contactref element="JP1" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
