<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="26.67" y2="0" width="0" layer="20"/>
<wire x1="26.67" y1="0" x2="26.67" y2="21.717" width="0" layer="20"/>
<wire x1="26.67" y1="21.717" x2="0" y2="21.717" width="0" layer="20"/>
<wire x1="0" y1="21.717" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>VCC</text>
<text>Antenna trace 12mils (50Ohms impedance)</text>
<text>1 oz copper</text>
<text>6.7 mil prepreg</text>
<text>0.5 oz copper</text>
<text>47 mil core</text>
<text>0.5 oz copper</text>
<text>6.7 mil prepreg</text>
<text>1 oz copper</text>
<text>er is 3.66</text>
<text>Stackup:</text>
<text>IRQ</text>
<text>ENA</text>
<text>SEL</text>
<text>SDI</text>
<text>SDO</text>
<text>SCK</text>
<text>BLE R1</text>
<text>OpenMV</text>
</plain>
<libraries>
<library name="sfe">
<packages>
<package name="0805">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="JST-2-PTH">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="iofault">
<packages>
<package name="OSHW_FILLX100_NOTEXT">
</package>
<package name="QFN-32">
</package>
<package name="2450BM14A0002">
</package>
</packages>
</library>
<library name="CC3000">
<packages>
<package name="ANTENNA">
</package>
</packages>
</library>
<library name="openmv">
<packages>
<package name="OPENMV-SMALL">
</package>
</packages>
</library>
<library name="mux">
<packages>
<package name="CRYSTAL3.2X2.5">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LOGO1" library="iofault" package="OSHW_FILLX100_NOTEXT" value="OSHW_LOGO_FILLX0100-NT"/>
<element name="U2" library="CC3000" package="ANTENNA" value="ANT-YAGEO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="sfe" package="JST-2-PTH" value="JP3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="openmv" package="OPENMV-SMALL" value="OPENMVSMALL"/>
<element name="Y1" library="mux" package="CRYSTAL3.2X2.5" value="16Mhz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="sfe" package="0402-CAP" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="sfe" package="0402-CAP" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="sfe" package="0402-RES" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="sfe" package="0402-CAP" value="2.2nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="iofault" package="QFN-32" value="NRF8001"/>
<element name="C14" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="sfe" package="0402-CAP" value="0.33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="sfe" package="0402-CAP" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="sfe" package="0402-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun" package="SOT23-5" value="2.8V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="sfe" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="sfe" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="iofault" package="2450BM14A0002" value="2450BM14A0002">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="U5" pad="6"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="U$2" pad="P$8"/>
<contactref element="U$2" pad="P$17"/>
<contactref element="U$2" pad="P$18"/>
<contactref element="U$2" pad="P$23"/>
<contactref element="C18" pad="2"/>
<contactref element="U$2" pad="P$30"/>
<contactref element="U$2" pad="P$31"/>
<contactref element="U$2" pad="P$33"/>
<contactref element="U3" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="Y1" pad="4"/>
<contactref element="Y1" pad="2"/>
<contactref element="U1" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="P$1"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="U$2" pad="P$9"/>
<contactref element="C18" pad="1"/>
<contactref element="U$2" pad="P$29"/>
<contactref element="U$2" pad="P$24"/>
<contactref element="U$2" pad="P$26"/>
<contactref element="R2" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="SCLK">
<contactref element="U5" pad="5"/>
<contactref element="U$2" pad="P$11"/>
</signal>
<signal name="N$69">
</signal>
<signal name="N$18">
<contactref element="C17" pad="1"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="VIN">
<contactref element="JP1" pad="2"/>
<contactref element="U5" pad="8"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="C13" pad="1"/>
<contactref element="U$2" pad="P$20"/>
<contactref element="U1" pad="P$5"/>
</signal>
<signal name="DCC">
<contactref element="U$2" pad="P$32"/>
</signal>
<signal name="N$2">
<contactref element="C9" pad="1"/>
<contactref element="U$2" pad="P$28"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="C8" pad="1"/>
<contactref element="U$2" pad="P$27"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="P$14"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="P$13"/>
<contactref element="U5" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="P$22"/>
<contactref element="U1" pad="P$3"/>
</signal>
<signal name="N$10">
<contactref element="U2" pad="P$1"/>
<contactref element="U1" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="U$2" pad="P$21"/>
<contactref element="U1" pad="P$4"/>
</signal>
<signal name="REQ">
<contactref element="U$2" pad="P$12"/>
<contactref element="U5" pad="7"/>
</signal>
<signal name="RDY">
<contactref element="U$2" pad="P$16"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="C16" pad="1"/>
<contactref element="U$2" pad="P$3"/>
</signal>
<signal name="N$20">
<contactref element="U$2" pad="P$25"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U$2" pad="P$19"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="ACTIVE">
<contactref element="U$2" pad="P$6"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="P$7"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="P$10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
