<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.56" y2="0" width="0" layer="20"/>
<wire x1="35.56" y1="0" x2="35.56" y2="26.67" width="0" layer="20"/>
<wire x1="35.56" y1="26.67" x2="0" y2="26.67" width="0" layer="20"/>
<wire x1="0" y1="26.67" x2="0" y2="0" width="0" layer="20"/>
<text>OpenMV</text>
<text>Proto</text>
<text>https://openmv.io</text>
<text>P6</text>
<text>P4</text>
<text>P5</text>
<text>P3</text>
<text>P2</text>
<text>P1</text>
<text>3v3</text>
<text>P0</text>
<text>P6</text>
<text>P4</text>
<text>P5</text>
<text>P3</text>
<text>P2</text>
<text>P1</text>
<text>3v3</text>
<text>P0</text>
<text>SWD</text>
<text>SWC</text>
<text>BOOT</text>
<text>RST</text>
<text>GND</text>
<text>VCC</text>
<text>P8</text>
<text>P7</text>
<text>SWD</text>
<text>SWC</text>
<text>BOOT</text>
<text>RST</text>
<text>GND</text>
<text>VCC</text>
<text>P8</text>
<text>P7</text>
</plain>
<libraries>
<library name="openmv">
<packages>
<package name="OPENMV3">
</package>
<package name="WEEE">
</package>
<package name="ROHS">
</package>
</packages>
</library>
<library name="iofault">
<packages>
<package name="OSHW_FILLX150_NOTEXT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="openmv" package="OPENMV3" value="OPENMV3"/>
<element name="U$1" library="iofault" package="OSHW_FILLX150_NOTEXT" value=""/>
<element name="U$4" library="openmv" package="WEEE" value=""/>
<element name="U$3" library="openmv" package="ROHS" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="28"/>
<contactref element="U$2" pad="28"/>
</signal>
<signal name="N$69">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="SDA">
<contactref element="U$2" pad="16"/>
</signal>
<signal name="SCL">
<contactref element="U$2" pad="15"/>
</signal>
<signal name="3.3V">
<contactref element="U$2" pad="18"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$12">
</signal>
<signal name="N$11">
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
<signal name="N$19">
</signal>
<signal name="N$20">
</signal>
<signal name="N$21">
</signal>
<signal name="N$22">
</signal>
<signal name="N$23">
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="N$27">
</signal>
<signal name="DAC">
<contactref element="U$2" pad="17"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="11"/>
</signal>
<signal name="N$43">
</signal>
<signal name="N$44">
</signal>
<signal name="N$45">
</signal>
<signal name="N$46">
</signal>
<signal name="N$47">
</signal>
<signal name="N$48">
</signal>
<signal name="N$49">
</signal>
<signal name="N$50">
</signal>
<signal name="N$51">
</signal>
<signal name="N$52">
</signal>
<signal name="PWM2">
<contactref element="U$2" pad="25"/>
</signal>
<signal name="PWM1">
<contactref element="U$2" pad="26"/>
</signal>
<signal name="VIN">
<contactref element="U$2" pad="27"/>
</signal>
<signal name="N$60">
</signal>
<signal name="N$61">
</signal>
<signal name="N$62">
</signal>
<signal name="N$63">
</signal>
<signal name="N$64">
</signal>
<signal name="N$65">
</signal>
<signal name="N$66">
</signal>
<signal name="N$67">
</signal>
<signal name="N$68">
</signal>
<signal name="N$70">
</signal>
<signal name="N$71">
</signal>
<signal name="SSEL">
<contactref element="U$2" pad="14"/>
</signal>
<signal name="SCLK">
<contactref element="U$2" pad="13"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="12"/>
</signal>
<signal name="SWC">
<contactref element="U$2" pad="21"/>
</signal>
<signal name="SWD">
<contactref element="U$2" pad="22"/>
</signal>
<signal name="RESET">
<contactref element="U$2" pad="24"/>
</signal>
<signal name="BOOT">
<contactref element="U$2" pad="23"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$28">
</signal>
<signal name="N$29">
</signal>
<signal name="N$30">
</signal>
<signal name="N$31">
</signal>
</signals>
</board>
</drawing>
</eagle>
