<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.4" y2="0" width="0" layer="20"/>
<wire x1="25.4" y1="0" x2="25.4" y2="33.02" width="0" layer="20"/>
<wire x1="25.4" y1="33.02" x2="0" y2="33.02" width="0" layer="20"/>
<wire x1="0" y1="33.02" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>VCC</text>
<text>Antenna trace 12mils (50Ohms impedance)</text>
<text>1 oz copper</text>
<text>6.7 mil prepreg</text>
<text>0.5 oz copper</text>
<text>47 mil core</text>
<text>0.5 oz copper</text>
<text>6.7 mil prepreg</text>
<text>1 oz copper</text>
<text>er is 3.66</text>
<text>Stackup:</text>
<text>IRQ</text>
<text>ENA</text>
<text>SEL</text>
<text>SDI</text>
<text>SDO</text>
<text>SCK</text>
<text>OpenMV</text>
<text>CC Shield R1</text>
</plain>
<libraries>
<library name="sfe">
<packages>
<package name="0805">
</package>
<package name="1210">
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="JST-2-PTH">
</package>
<package name="U.FL">
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="EIA3528">
</package>
</packages>
</library>
<library name="iofault">
<packages>
<package name="OSHW_FILLX100_NOTEXT">
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="CC3000">
<packages>
<package name="CC3000">
</package>
<package name="ANTENNA">
</package>
</packages>
</library>
<library name="openmv">
<packages>
<package name="OPENMV">
</package>
</packages>
</library>
<library name="mux">
<packages>
<package name="SOIC8">
<description>&lt;b&gt;Small Outline IC&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LOGO1" library="iofault" package="OSHW_FILLX100_NOTEXT" value="OSHW_LOGO_FILLX0100-NT"/>
<element name="U1" library="CC3000" package="CC3000" value="CC3000">
<attribute name="AUTHOR" value="Matt Bigarani"/>
<attribute name="DATASHEET" value="http://www.ti.com/lit/ds/symlink/cc3000.pdf"/>
<attribute name="DATE" value="2/8/2013"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="CC3000" package="ANTENNA" value="ANT-YAGEO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="sfe" package="0402-CAP" value="2.2pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="sfe" package="0402-CAP" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="iofault" package="C0402" value="2.2nH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="sfe" package="0402-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="sfe" package="0402-CAP" value="10pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="sfe" package="U.FL" value="U.FL"/>
<element name="JP1" library="sfe" package="JST-2-PTH" value="JP3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="openmv" package="OPENMV" value="OPENMV"/>
<element name="SJ1" library="sfe" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
</element>
<element name="SJ2" library="sfe" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
</element>
<element name="U4" library="mux" package="SOIC8" value="TPS768">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="sfe" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="sfe" package="1210" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="sfe" package="EIA3528" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="P$1"/>
<contactref element="U1" pad="P$10"/>
<contactref element="U1" pad="P$11"/>
<contactref element="U1" pad="P$16"/>
<contactref element="U1" pad="P$18"/>
<contactref element="U1" pad="P$31"/>
<contactref element="U1" pad="P$32"/>
<contactref element="U1" pad="P$33"/>
<contactref element="U1" pad="P$34"/>
<contactref element="U1" pad="P$37"/>
<contactref element="U1" pad="P$39"/>
<contactref element="U1" pad="P$40"/>
<contactref element="U1" pad="P$41"/>
<contactref element="U1" pad="P$42"/>
<contactref element="U1" pad="P$43"/>
<contactref element="U1" pad="P$44"/>
<contactref element="U1" pad="P$45"/>
<contactref element="U1" pad="P$46"/>
<contactref element="U1" pad="P$46"/>
<contactref element="U1" pad="P$45"/>
<contactref element="U1" pad="P$44"/>
<contactref element="U1" pad="P$43"/>
<contactref element="U1" pad="P$42"/>
<contactref element="U1" pad="P$41"/>
<contactref element="U1" pad="P$37"/>
<contactref element="U1" pad="P$38"/>
<contactref element="U1" pad="P$39"/>
<contactref element="U1" pad="P$40"/>
<contactref element="U1" pad="P$20"/>
<contactref element="U1" pad="P$22"/>
<contactref element="U1" pad="P$25"/>
<contactref element="U1" pad="P$11"/>
<contactref element="U1" pad="P$16"/>
<contactref element="U1" pad="P$18"/>
<contactref element="U1" pad="P$10"/>
<contactref element="U1" pad="P$9"/>
<contactref element="U1" pad="P$1"/>
<contactref element="U1" pad="P$21"/>
<contactref element="U1" pad="P$34"/>
<contactref element="U1" pad="P$33"/>
<contactref element="U1" pad="P$32"/>
<contactref element="U1" pad="P$31"/>
<contactref element="U1" pad="P$36"/>
<contactref element="L2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U3" pad="P$1"/>
<contactref element="U3" pad="P$2"/>
<contactref element="JP1" pad="1"/>
<contactref element="U5" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="U4" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C8" pad="C"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="P$23"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="P$19"/>
<contactref element="U4" pad="5"/>
<contactref element="C2" pad="1"/>
<contactref element="U4" pad="6"/>
<contactref element="C8" pad="A"/>
</signal>
<signal name="CC_EN">
<contactref element="U1" pad="P$26"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="P$35"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="C7" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U2" pad="P$1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="P$30"/>
<contactref element="U1" pad="P$29"/>
</signal>
<signal name="CC_CS">
<contactref element="U1" pad="P$12"/>
<contactref element="U5" pad="7"/>
</signal>
<signal name="CC_MISO">
<contactref element="U1" pad="P$13"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="CC_IRQ">
<contactref element="U1" pad="P$14"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="CC_MOSI">
<contactref element="U1" pad="P$15"/>
<contactref element="U5" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U3" pad="P$3"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="CC_SCLK">
<contactref element="U1" pad="P$17"/>
<contactref element="U5" pad="5"/>
</signal>
<signal name="N$69">
</signal>
<signal name="N$3">
<contactref element="U1" pad="P$5"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="P$28"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="VIN">
<contactref element="U4" pad="3"/>
<contactref element="U4" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="U5" pad="8"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="P$7"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="P$27"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="N$12">
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
