<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="37.846" y2="0" width="0" layer="20"/>
<wire x1="37.846" y1="0" x2="37.846" y2="47.498" width="0" layer="20"/>
<wire x1="37.846" y1="47.498" x2="0" y2="47.498" width="0" layer="20"/>
<wire x1="0" y1="47.498" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>SDI</text>
<text>SCK</text>
<text>VCC</text>
<text>RS</text>
<text>RST</text>
<text>CS</text>
<text>LED</text>
<text>https://openmv.io</text>
<text>LCD Shield Rev 2</text>
<text>2/11/2016</text>
<text>Made in USA</text>
<text>Built by MacroFab</text>
</plain>
<libraries>
<library name="sfe">
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="0603">
</package>
<package name="SOT23-3">
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="JD-T1800">
</package>
</packages>
</library>
<library name="sullins">
<packages>
<package name="1X8">
</package>
</packages>
</library>
<library name="openmv">
<packages>
<package name="ROHS">
</package>
<package name="WEEE">
</package>
<package name="OMV-LOGO-BIG">
</package>
</packages>
</library>
<library name="iofault">
<packages>
<package name="OSHW_FILLX150_NOTEXT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C4" library="sfe" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LCD1" library="adafruit" package="JD-T1800" value="JD-T1800"/>
<element name="FB1" library="sfe" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="sfe" package="0603-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="sfe" package="0603-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="sfe" package="0603-RES" value="2.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="sfe" package="SOT23-3" value="MOSFET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="sfe" package="0603-RES" value="10ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="sfe" package="0603-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="sfe" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="sullins" package="1X8" value="1X8"/>
<element name="J2" library="sullins" package="1X8" value="1X8"/>
<element name="U$2" library="openmv" package="ROHS" value=""/>
<element name="U$3" library="openmv" package="WEEE" value=""/>
<element name="U$5" library="iofault" package="OSHW_FILLX150_NOTEXT" value=""/>
<element name="U$4" library="openmv" package="OMV-LOGO-BIG" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="LCD1" pad="13"/>
<contactref element="LCD1" pad="5"/>
<contactref element="LCD1" pad="2"/>
<contactref element="LCD1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="J2" pad="P$8"/>
</signal>
<signal name="N$69">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="RST">
<contactref element="LCD1" pad="6"/>
<contactref element="J2" pad="P$6"/>
</signal>
<signal name="RS">
<contactref element="LCD1" pad="7"/>
<contactref element="J2" pad="P$5"/>
</signal>
<signal name="SDI">
<contactref element="LCD1" pad="8"/>
<contactref element="J1" pad="P$1"/>
</signal>
<signal name="SCK">
<contactref element="LCD1" pad="9"/>
<contactref element="J1" pad="P$3"/>
</signal>
<signal name="CS">
<contactref element="LCD1" pad="12"/>
<contactref element="R2" pad="2"/>
<contactref element="J1" pad="P$4"/>
</signal>
<signal name="VDDA">
<contactref element="LCD1" pad="10"/>
<contactref element="FB1" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="LCD1" pad="11"/>
<contactref element="C4" pad="1"/>
<contactref element="FB1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="LCD1" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="J1" pad="P$8"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="Q1" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="LED">
<contactref element="R3" pad="1"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="LEDK">
<contactref element="LCD1" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="P$7"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
