<!--This work is licensed under a Creative Commons Attribution-ShareAlike 4.0 International License (CC BY-SA) with Design Exception 1.0-->
<eagle version="7.1.0">
<drawing>
<library>
<packages>
<package name="QFN50P300X300X100-17N">
</package>
</packages>
<symbols>
<symbol name="BQ24075RGTR">
<pin name="!CE" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="SYSOFF" direction="in"/>
<pin name="BAT_2"/>
<pin name="BAT_3"/>
<pin name="ILIM" direction="in"/>
<pin name="ISET"/>
<pin name="!CHG" direction="out"/>
<pin name="OUT_10" direction="out"/>
<pin name="OUT_11" direction="out"/>
<pin name="!PGOOD" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="TS" direction="in"/>
<pin name="TMR" direction="in"/>
<pin name="EXP" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BQ24075RGTR" prefix="U">
<description>Standalone 1-cell 1.5-A linear charger, Power Path, 4.2-V VBAT and 5.5-V VOUT 16-VQFN -40 to 85  &lt;a href="https://pricing.snapeda.com/parts/BQ24075RGTR/Texas%20Instruments/view-part?ref=eda"&gt;Check availability&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="BQ24075RGTR"/>
</gates>
<devices>
<device name="" package="QFN50P300X300X100-17N">
<connects>
<connect gate="G$1" pin="!CE" pad="4"/>
<connect gate="G$1" pin="!CHG" pad="9"/>
<connect gate="G$1" pin="!PGOOD" pad="7"/>
<connect gate="G$1" pin="BAT_2" pad="2"/>
<connect gate="G$1" pin="BAT_3" pad="3"/>
<connect gate="G$1" pin="EN1" pad="6"/>
<connect gate="G$1" pin="EN2" pad="5"/>
<connect gate="G$1" pin="EXP" pad="17"/>
<connect gate="G$1" pin="ILIM" pad="12"/>
<connect gate="G$1" pin="IN" pad="13"/>
<connect gate="G$1" pin="ISET" pad="16"/>
<connect gate="G$1" pin="OUT_10" pad="10"/>
<connect gate="G$1" pin="OUT_11" pad="11"/>
<connect gate="G$1" pin="SYSOFF" pad="15"/>
<connect gate="G$1" pin="TMR" pad="14"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MP" value="BQ24075RGTR"/>
<attribute name="Availability" value="In Stock"/>
<attribute name="Description" value="
Standalone 1-cell 1.5-A linear battery charger, Power Path, 4.2-V VBAT and 5.5-V VOUT
"/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="Purchase-URL" value="https://pricing.snapeda.com/search/part/BQ24075RGTR/?ref=eda"/>
<attribute name="Price" value="None"/>
<attribute name="Package" value="VQFN-16 Texas Instruments"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
