<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="44.45" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="35.56" y2="0" width="0" layer="20"/>
<wire x1="35.56" y1="0" x2="35.56" y2="44.45" width="0" layer="20"/>
<wire x1="35.56" y1="44.45" x2="0" y2="44.45" width="0" layer="20"/>
<text>P6</text>
<text>P4</text>
<text>P5</text>
<text>P3</text>
<text>P2</text>
<text>P1</text>
<text>WAKE</text>
<text>RST</text>
<text>P7</text>
<text>GND</text>
<text>3.3V</text>
<text>VIN</text>
<text>P8</text>
<text>P0</text>
<text>3.3V</text>
<text>P6</text>
<text>P5</text>
<text>P4</text>
<text>P3</text>
<text>P2</text>
<text>P1</text>
<text>P0</text>
<text>GND</text>
<text>VIN</text>
<text>P7</text>
<text>P8</text>
<text>RST</text>
<text>WAKE</text>
<text>OpenMV RT R1</text>
<text>3.21.23</text>
<text>VIN 5V Max</text>
<text>P10</text>
<text>P10</text>
<text>P9</text>
<text>P9</text>
<text>IR</text>
<text>W</text>
<text>https://openmv.io</text>
<text>I/Os 3.3V
Tolerant
</text>
<text>ELED
ERXN
ERXP
ETXN
ETXP
PBTN
RAW
GND</text>
<text>3.7V LiPo</text>
</plain>
<libraries>
<library name="sfe">
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 2.8 mm, round</description>
</package>
</packages>
</library>
<library name="openmv">
<packages>
<package name="OMV-LOGO">
</package>
<package name="WEEE">
</package>
<package name="ROHS">
</package>
<package name="OMV-LOGO-SMALL">
</package>
</packages>
</library>
<library name="adafruit-updated">
<packages>
<package name="JST-PH-2-THM-RA">
<description>&lt;b&gt;S2B-PH-K-S&lt;/b&gt; 
&lt;p&gt;
JST PH 2-pin thru-home side entry</description>
</package>
</packages>
</library>
<library name="LBEE5KL1DX-TEMP">
<packages>
<package name="XCVR_LBEE5KL1DX-TEMP">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0201">
<description>Source: http://www.avxcorp.com/docs/catalogs/cx5r.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="USB4105-GF-A">
<packages>
<package name="GCT_USB4105-GF-A">
</package>
</packages>
</library>
<library name="BQ24075RGTR">
<packages>
<package name="QFN50P300X300X100-17N">
</package>
</packages>
</library>
<library name="UHD1110-FKA-CL1A13R3Q1BBQFMF3">
<packages>
<package name="LED_UHD1110-FKA-CL1A13R3Q1BBQFMF3">
</package>
</packages>
</library>
<library name="LM66200DRLR">
<description>&lt;1.6-V to 5.5-V, 40-m, 2.5-A, low-IQ, dual ideal diode&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOTFL50P160X60-8N">
<description>&lt;b&gt;DRL0008A&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="AP61300Z6-7">
<description>&lt;DCDC Conv LV Buck SOT563 T&amp;R 3K&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOTFL50P162X60-6N">
<description>&lt;b&gt;SOT563&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="2N7002KW_R1_00001">
<description>&lt;MOSFET 60V N-Channel Enhancement Mode MOSFET - ESD Protected&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT65P210X110-3N">
<description>&lt;b&gt;SOT 323&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="MAKK2016T1R0M">
<packages>
<package name="INDC2016X100N">
</package>
</packages>
</library>
<library name="CPDQT5V0HE-HF">
<description>&lt;ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="CPDQT5V0HEHF">
<description>&lt;b&gt;CPDQT5V0HE-HF-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="IS42S16160G-6BL">
<description>&lt;DRAM 256M 16Mx16 166Mhz SDR SDRAM, 3.3V&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="BGA54C80P9X9_800X800X120">
<description>&lt;b&gt;TF-BGA 54 LEAD&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="IS25LP128F-JKLE-TR">
<description>&lt;NOR Flash 128M 2.3-3.6V 166Mhz Serial NOR Flash&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SON127P500X595X80-9N">
<description>&lt;b&gt;6 8 CONTACT ULTRA-THIN SMALL OUTLINE NO-LEAD (WSON) PACKAGE 6X5MM (K)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="ATECC608B-MAHDA-T">
<description>&lt;CryptoAuthentication 8-Pin UDFN EP T/R&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SON50P300X200X60-9N">
<description>&lt;b&gt;8-Lead Plastic DFN (MN)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="MXC4005XC">
<description>&lt;Accelerometers Monolithic and Wafer Level Packaged Three-Axis Accelerometer&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="MXC4005XC">
<description>&lt;b&gt;MXC4005XC-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="MIMXRT1052DVL6B">
<description>&lt;Processors - Application Specialized MIMXRT1052DVL6B/LFBGA196///STANDARD MARKING * TRAY&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="BGA196C65P14X14_1000X1000X143">
<description>&lt;b&gt;10 x 10 mm BGA(pitch 0.65mm)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="EMIF06-1005M12">
<description>&lt;EMI Filter Circuits 6lin lw cpcitnc EMI 45pF -35db @ 900MHz&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SON40P150X250X65-13N">
<description>&lt;b&gt;QFN 2.5 x 1.5&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="3221-10-0300-00">
<packages>
<package name="CNC_3221-10-0300-00">
</package>
</packages>
</library>
<library name="KSZ8081RNDCA-TR">
<description>&lt;Ethernet ICs 10/100 BASE-TX Physical Layer Transceiver&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="QFN50P400X400X90-25N">
<description>&lt;b&gt;KSZ8081RNAIA-TR-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="AMCA31-2R450G-S1F-T3">
<description>&lt;ABRACON - AMCA31-2R450G-S1F-T3 - ANTENNA, CHIP, 2.45GHZ, 50 OHM, 1206&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="ANTC3216X140N">
<description>&lt;b&gt;ACMA31&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="GRM0335C1H1R5BA01D">
<description>&lt;Chip Capacitor value 1R5&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="CAPC0603X33N">
<description>&lt;b&gt;GRM03_0.03 L=0.6mm W=0.3mm T=0.3mm&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="MAKK2016T2R2M">
<packages>
<package name="INDC2016X100N">
</package>
</packages>
</library>
<library name="2337019-1">
<description>&lt;RF Connectors / Coaxial Connectors MicroCoax receptacle UMCC Gen 1&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="23370191">
<description>&lt;b&gt;2337019-1-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-Coils">
<description>&lt;h3&gt;SparkFun Coils&lt;/h3&gt;
In this library you'll find magnetics.

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;Inductors&lt;/li&gt;
&lt;li&gt;Ferrite Beads&lt;/li&gt;
&lt;li&gt;Transformers&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;

&lt;br&gt;
&lt;p&gt;We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.&lt;/p&gt;</description>
<packages>
<package name="0402">
<description>&lt;p&gt;&lt;b&gt;Generic 1005 (0402) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="MAKK2016T4R7M">
<packages>
<package name="INDC2016X100N">
</package>
</packages>
</library>
<library name="XRCGB24M000F3M00R0">
<description>&lt;Murata 24MHz Crystal +/-30ppm SMD 4-Pin 2 x 1.6 x 0.7mm&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="XRCGB24M000F3M00R0">
<description>&lt;b&gt;XRCGB24M000F3M00R0-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="ABS07-32.768KHZ-7-T">
<packages>
<package name="XTAL_ABS07-32.768KHZ-7-T">
</package>
</packages>
</library>
<library name="MIC5365-3.3YMT-TZ">
<packages>
<package name="VREG_MIC5365-3.3YMT-TZ">
</package>
</packages>
</library>
<library name="9774030151R">
<packages>
<package name="9774030151R">
</package>
</packages>
</library>
<library name="DF12-36-DS">
<packages>
<package name="DF12-36-DS">
</package>
</packages>
</library>
<library name="ECMF02-4CMX8">
<description>&lt;Common Mode Filter &amp; ESD Prot. USB uQFN8 STMicroelectronics ECMF02 Series, Signal Filter uQFN SMD, Flat Contact Termination, 2.6 x 1.3 x 0.6mm&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="ECMF024CMX8">
<description>&lt;b&gt;Micro QFN-8L&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="EXB-2HV104JV">
<description>&lt;Resistor Networks &amp; Arrays Resistor Array Chip 8 Elements 1506&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="EXB2HV104JV">
<description>&lt;b&gt;EXB-2HV104JV-4&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FIDUCIAL-1X2">
<description>&lt;h3&gt;Fiducial - Circle, 1mm&lt;/h3&gt;
&lt;p&gt;Point-of-reference for pick-and-place machines and other optical instruments.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FIDUCIAL&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="1040310811">
<description>Generated from &lt;b&gt;rt10.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="1040310811">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="H2" library="holes" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8">
<attribute name="POPULARITY" value="6"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="H1" library="holes" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8">
<attribute name="POPULARITY" value="6"/>
<attribute name="POPULATE" value="0"/>
</element>
<element name="U$3" library="openmv" package="OMV-LOGO" value=""/>
<element name="U$1" library="openmv" package="WEEE" value=""/>
<element name="U$2" library="openmv" package="ROHS" value=""/>
<element name="U$4" library="openmv" package="OMV-LOGO-SMALL" value=""/>
<element name="M2" library="9774030151R" package="9774030151R" value="9774030151R">
<attribute name="MPN" value="9774030151R"/>
</element>
<element name="M1" library="9774030151R" package="9774030151R" value="9774030151R">
<attribute name="MPN" value="9774030151R"/>
</element>
<element name="J4" library="DF12-36-DS" package="DF12-36-DS" value="DF12-36-DS">
<attribute name="MPN" value="DF12NB-36DS-0.5V(51)"/>
<attribute name="NAME"/>
</element>
<element name="U3" library="LBEE5KL1DX-TEMP" package="XCVR_LBEE5KL1DX-TEMP" value="LBEE5KL1DX-883">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" WICED Transceiver; 802.11 b/g/n _Wi-Fi, WiFi, WLAN_, Bluetooth® Smart Ready 4.x Dual Mode For Use With BCM4343W, i.MX 6 "/>
<attribute name="MF" value="Murata Electronics"/>
<attribute name="MP" value="LBEE5KL1DX-TEMP"/>
<attribute name="MPN" value="LBEE5KL1DX-883"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="sfe" package="C0402" value="100">
<attribute name="MPN" value="MFBM1V1608-101-R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X08" value="DNP">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X08" value="DNP">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="USB4105-GF-A" package="GCT_USB4105-GF-A" value="USB4105-GF-A">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" USB-C (USB TYPE-C) USB 2.0 Receptacle Connector 24 (16+8 Dummy) Position Surface Mount, Right Angle; Through Hole "/>
<attribute name="MF" value="GCT"/>
<attribute name="MP" value="USB4105-GF-A"/>
<attribute name="MPN" value="USB4105-GF-A"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/USB4105-GF-A/?ref=eda"/>
</element>
<element name="R6" library="sfe" package="0402-RES" value="5.1K">
<attribute name="MPN" value="RMC1/20-512FPA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="sfe" package="0402-RES" value="5.1K">
<attribute name="MPN" value="RMC1/20-512FPA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="sfe" package="C0402" value="100">
<attribute name="MPN" value="MFBM1V1608-101-R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="BQ24075RGTR" package="QFN50P300X300X100-17N" value="BQ24075RGTR">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" Standalone 1-cell 1.5-A linear battery charger, Power Path, 4.2-V VBAT and 5.5-V VOUT "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="BQ24075RGTR"/>
<attribute name="MPN" value="BQ24075RGTR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="VQFN-16 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/BQ24075RGTR/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="CN1" library="adafruit-updated" package="JST-PH-2-THM-RA" value="S2B-PH-K-S(LF)(SN)">
<attribute name="MPN" value="S2B-PH-K-S(LF)(SN)"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="UHD1110-FKA-CL1A13R3Q1BBQFMF3" package="LED_UHD1110-FKA-CL1A13R3Q1BBQFMF3" value="UHD1110-FKA-CL1A13R3Q1BBQFMF3">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" Red, Green, Blue (RGB) - LED Indication - Discrete 1.9V Red, 2.9V Green, 2.9V Blue 0404 (1010 Metric) "/>
<attribute name="MF" value="Cree Inc."/>
<attribute name="MP" value="UHD1110-FKA-CL1A13R3Q1BBQFMF3"/>
<attribute name="MPN" value="UHD1110-FKA-CL1A13r3q1BBQFMF3"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0404 Cree Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/UHD1110-FKA-CL1A13R3Q1BBQFMF3/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="sfe" package="0402-RES" value="1.13K">
<attribute name="MPN" value="CRCW04021K13FKED"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="sfe" package="0402-RES" value="46.4K">
<attribute name="MPN" value="WR04X4642FTL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="sfe" package="0402-RES" value="1.18K">
<attribute name="MPN" value="AC0402FR-071K18L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="sfe" package="0402-RES" value="10K">
<attribute name="MPN" value="AC0402FR-1310KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="sfe" package="0402-RES" value="1K">
<attribute name="MPN" value="0402WGF1001TCE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="sfe" package="0402-RES" value="1K">
<attribute name="MPN" value="0402WGF1001TCE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="LM66200DRLR" package="SOTFL50P160X60-8N" value="LM66200DRLR">
<attribute name="DESCRIPTION" value="1.6-V to 5.5-V, 40-m, 2.5-A, low-IQ, dual ideal diode"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LM66200DRLR"/>
<attribute name="MOUSER_PART_NUMBER" value="595-LM66200DRLR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/LM66200DRLR?qs=Rp5uXu7WBW90hnpZAkIOdQ%3D%3D"/>
<attribute name="MPN" value="LM66200DRLR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="sfe" package="0402-RES" value="1K">
<attribute name="MPN" value="0402WGF1001TCE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="AP61300Z6-7" package="SOTFL50P162X60-6N" value="AP61300Z6-7">
<attribute name="DESCRIPTION" value="DCDC Conv LV Buck SOT563 T&amp;R 3K"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="MANUFACTURER_NAME" value="Diodes Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="AP61300Z6-7"/>
<attribute name="MOUSER_PART_NUMBER" value="621-AP61300Z6-7"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/AP61300Z6-7?qs=HBWAp0VN4Ri0dzb0XP2pEA%3D%3D"/>
<attribute name="MPN" value="AP61300Z6-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="2N7002KW_R1_00001" package="SOT65P210X110-3N" value="2N7002KW_R1_00001">
<attribute name="DESCRIPTION" value="MOSFET 60V N-Channel Enhancement Mode MOSFET - ESD Protected"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="PANJIT"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="2N7002KW_R1_00001"/>
<attribute name="MOUSER_PART_NUMBER" value="241-2N7002KWR100001"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Panjit/2N7002KW_R1_00001?qs=sPbYRqrBIVliWKATqv7jNA%3D%3D"/>
<attribute name="MPN" value="2N7002KW_R1_00001"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="sfe" package="0402-RES" value="200K">
<attribute name="MPN" value="CRCW0402200KFKEDC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="sfe" package="0402-RES" value="44.2K">
<attribute name="MPN" value="AC0402FR-0744K2L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="MAKK2016T1R0M" package="INDC2016X100N" value="MAKK2016T1R0M">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 1 µH Shielded Drum Core, Wirewound Inductor 2.2 A 75mOhm Max 0806 (2016 Metric) "/>
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MP" value="MAKK2016T1R0M"/>
<attribute name="MPN" value="MAKK2016T1R0M"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2016 Taiyo Yuden"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/MAKK2016T1R0M/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
</element>
<element name="IC3" library="IS42S16160G-6BL" package="BGA54C80P9X9_800X800X120" value="IS42S16160G-6BL">
<attribute name="DESCRIPTION" value="DRAM 256M 16Mx16 166Mhz SDR SDRAM, 3.3V"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="MANUFACTURER_NAME" value="Integrated Silicon Solution Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="IS42S16160G-6BL"/>
<attribute name="MOUSER_PART_NUMBER" value="870-IS42S16160G-6BL"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/ISSI/IS42S16160G-6BL?qs=9hm%252BDT1Jr7yvZBhvmJyecQ%3D%3D"/>
<attribute name="MPN" value="IS42S16160G-6BL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="IS25LP128F-JKLE-TR" package="SON127P500X595X80-9N" value="IS25LP064D-JKLE-TR">
<attribute name="DESCRIPTION" value="NOR Flash 64M 2.3-3.6V 166Mhz Serial NOR Flash"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Integrated Silicon Solution Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="IS25LP064D-JKLE-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="870-5LP064D-JKLE-TR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/ProductDetail/ISSI/IS25LP064D-JKLE-TR?qs=xZ%2FP%252Ba9zWqa2pmLA1ByOew%3D%3D"/>
<attribute name="MPN" value="IS25LP064D-JKLE-TR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="IS25LP128F-JKLE-TR" package="SON127P500X595X80-9N" value="IS25LP128F-JKLE-TR">
<attribute name="DESCRIPTION" value="NOR Flash 128M 2.3-3.6V 166Mhz Serial NOR Flash"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Integrated Silicon Solution Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="IS25LP128F-JKLE-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="870-IS25LP128FJKLETR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/ISSI/IS25LP128F-JKLE-TR?qs=F5EMLAvA7IC8MN2X519UUw%3D%3D"/>
<attribute name="MPN" value="IS25LP128F-JKLE-TR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="ATECC608B-MAHDA-T" package="SON50P300X200X60-9N" value="ATECC608B-MAHDA-T">
<attribute name="DESCRIPTION" value="CryptoAuthentication 8-Pin UDFN EP T/R"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATECC608B-MAHDA-T"/>
<attribute name="MOUSER_PART_NUMBER" value="579-TECC608B-MAHDA-T"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Microchip-Technology/ATECC608B-MAHDA-T?qs=W%2FMpXkg%252BdQ71cGyt0Wo3Jw%3D%3D"/>
<attribute name="MPN" value="ATECC608B-MAHDA-T"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="MXC4005XC" package="MXC4005XC" value="MXC4005XC">
<attribute name="DESCRIPTION" value="Accelerometers Monolithic and Wafer Level Packaged Three-Axis Accelerometer"/>
<attribute name="HEIGHT" value="0.885mm"/>
<attribute name="MANUFACTURER_NAME" value="MEMSIC"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MXC4005XC"/>
<attribute name="MOUSER_PART_NUMBER" value="438-MXC4005XC"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/MEMSIC/MXC4005XC?qs=RcG8xmE7yp3iyYgWLmAtUw%3D%3D"/>
<attribute name="MPN" value="MXC4005XC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="sfe" package="0402-RES" value="2.7K">
<attribute name="MPN" value="AC0402JR-072K7L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="sfe" package="0402-RES" value="2.7K">
<attribute name="MPN" value="AC0402JR-072K7L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="sfe" package="0402-RES" value="2.7K">
<attribute name="MPN" value="AC0402JR-072K7L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="UHD1110-FKA-CL1A13R3Q1BBQFMF3" package="LED_UHD1110-FKA-CL1A13R3Q1BBQFMF3" value="UHD1110-FKA-CL1A13R3Q1BBQFMF3">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" Red, Green, Blue (RGB) - LED Indication - Discrete 1.9V Red, 2.9V Green, 2.9V Blue 0404 (1010 Metric) "/>
<attribute name="MF" value="Cree Inc."/>
<attribute name="MP" value="UHD1110-FKA-CL1A13R3Q1BBQFMF3"/>
<attribute name="MPN" value="UHD1110-FKA-CL1A13r3q1BBQFMF3"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0404 Cree Inc."/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/UHD1110-FKA-CL1A13R3Q1BBQFMF3/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="sfe" package="0402-RES" value="220">
<attribute name="MPN" value="CRGCQ0402F220R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="sfe" package="0402-RES" value="220">
<attribute name="MPN" value="CRGCQ0402F220R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="sfe" package="0402-RES" value="220">
<attribute name="MPN" value="CRGCQ0402F220R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC8" library="MIMXRT1052DVL6B" package="BGA196C65P14X14_1000X1000X143" value="MIMXRT1052DVL6B">
<attribute name="DESCRIPTION" value="Processors - Application Specialized MIMXRT1052DVL6B/LFBGA196///STANDARD MARKING * TRAY"/>
<attribute name="HEIGHT" value="1.43mm"/>
<attribute name="MANUFACTURER_NAME" value="NXP"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MIMXRT1052DVL6B"/>
<attribute name="MOUSER_PART_NUMBER" value="771-MIMXRT1052DVL6B"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/NXP-Semiconductors/MIMXRT1052DVL6B?qs=r5DSvlrkXmLhWvqckzJtSg%3D%3D"/>
<attribute name="MPN" value="MIMXRT1052DVL6B"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FL3" library="EMIF06-1005M12" package="SON40P150X250X65-13N" value="EMIF06-1005M12">
<attribute name="DESCRIPTION" value="EMI Filter Circuits 6lin lw cpcitnc EMI 45pF -35db @ 900MHz"/>
<attribute name="HEIGHT" value="0.65mm"/>
<attribute name="MANUFACTURER_NAME" value="STMicroelectronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="EMIF06-1005M12"/>
<attribute name="MOUSER_PART_NUMBER" value="511-EMIF06-1005M12"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/STMicroelectronics/EMIF06-1005M12?qs=VJaATVMq%252BXo0u09ZqtQg3A%3D%3D"/>
<attribute name="MPN" value="EMIF06-1005M12"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="3221-10-0300-00" package="CNC_3221-10-0300-00" value="3221-10-0300-00">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" Connector Header Surface Mount 10 position 0.050 (1.27mm) "/>
<attribute name="MF" value="CNC Tech"/>
<attribute name="MP" value="3221-10-0300-00"/>
<attribute name="MPN" value="3221-10-0300-00"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/3221-10-0300-00/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="FL5" library="EMIF06-1005M12" package="SON40P150X250X65-13N" value="EMIF06-1005M12">
<attribute name="DESCRIPTION" value="EMI Filter Circuits 6lin lw cpcitnc EMI 45pF -35db @ 900MHz"/>
<attribute name="HEIGHT" value="0.65mm"/>
<attribute name="MANUFACTURER_NAME" value="STMicroelectronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="EMIF06-1005M12"/>
<attribute name="MOUSER_PART_NUMBER" value="511-EMIF06-1005M12"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/STMicroelectronics/EMIF06-1005M12?qs=VJaATVMq%252BXo0u09ZqtQg3A%3D%3D"/>
<attribute name="MPN" value="EMIF06-1005M12"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="sfe" package="0402-RES" value="10K">
<attribute name="MPN" value="AC0402FR-1310KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="sfe" package="C0402" value="100">
<attribute name="MPN" value="MFBM1V1608-101-R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="sfe" package="0402-RES" value="4.7K">
<attribute name="MPN" value="AC0402FR-074K7L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="sfe" package="0402-RES" value="4.7K">
<attribute name="MPN" value="AC0402FR-074K7L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC9" library="KSZ8081RNDCA-TR" package="QFN50P400X400X90-25N" value="KSZ8081RNDCA-TR">
<attribute name="DESCRIPTION" value="Ethernet ICs 10/100 BASE-TX Physical Layer Transceiver"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="KSZ8081RNDCA-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="998-KSZ8081RNDCATR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Microchip-Technology-Atmel/KSZ8081RNDCA-TR?qs=U6T8BxXiZAXLXXdn%2FieQKw%3D%3D"/>
<attribute name="MPN" value="KSZ8081RNDCA-TR"/>
<attribute name="NAME"/>
</element>
<element name="R35" library="sfe" package="0402-RES" value="220">
<attribute name="MPN" value="CRGCQ0402F220R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="sfe" package="0402-RES" value="6.49K">
<attribute name="MPN" value="CR0402-FX-6491GLF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C84" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C83" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C89" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C96" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C82" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C85" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="L8" library="sfe" package="C0402" value="100">
<attribute name="MPN" value="MFBM1V1608-101-R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="sfe" package="0402-RES" value="1K">
<attribute name="MPN" value="0402WGF1001TCE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="sfe" package="0402-RES" value="1K">
<attribute name="MPN" value="0402WGF1001TCE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FL2" library="EMIF06-1005M12" package="SON40P150X250X65-13N" value="EMIF06-1005M12">
<attribute name="DESCRIPTION" value="EMI Filter Circuits 6lin lw cpcitnc EMI 45pF -35db @ 900MHz"/>
<attribute name="HEIGHT" value="0.65mm"/>
<attribute name="MANUFACTURER_NAME" value="STMicroelectronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="EMIF06-1005M12"/>
<attribute name="MOUSER_PART_NUMBER" value="511-EMIF06-1005M12"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/STMicroelectronics/EMIF06-1005M12?qs=VJaATVMq%252BXo0u09ZqtQg3A%3D%3D"/>
<attribute name="MPN" value="EMIF06-1005M12"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FL4" library="EMIF06-1005M12" package="SON40P150X250X65-13N" value="EMIF06-1005M12">
<attribute name="DESCRIPTION" value="EMI Filter Circuits 6lin lw cpcitnc EMI 45pF -35db @ 900MHz"/>
<attribute name="HEIGHT" value="0.65mm"/>
<attribute name="MANUFACTURER_NAME" value="STMicroelectronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="EMIF06-1005M12"/>
<attribute name="MOUSER_PART_NUMBER" value="511-EMIF06-1005M12"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/STMicroelectronics/EMIF06-1005M12?qs=VJaATVMq%252BXo0u09ZqtQg3A%3D%3D"/>
<attribute name="MPN" value="EMIF06-1005M12"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C65" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X08" value="DNP">
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="D5" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="2N7002KW_R1_00001" package="SOT65P210X110-3N" value="2N7002KW_R1_00001">
<attribute name="DESCRIPTION" value="MOSFET 60V N-Channel Enhancement Mode MOSFET - ESD Protected"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="PANJIT"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="2N7002KW_R1_00001"/>
<attribute name="MOUSER_PART_NUMBER" value="241-2N7002KWR100001"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Panjit/2N7002KW_R1_00001?qs=sPbYRqrBIVliWKATqv7jNA%3D%3D"/>
<attribute name="MPN" value="2N7002KW_R1_00001"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ANT1" library="AMCA31-2R450G-S1F-T3" package="ANTC3216X140N" value="AMCA31-2R450G-S1F-T3">
<attribute name="DESCRIPTION" value="ABRACON - AMCA31-2R450G-S1F-T3 - ANTENNA, CHIP, 2.45GHZ, 50 OHM, 1206"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="MANUFACTURER_NAME" value="ABRACON"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="AMCA31-2R450G-S1F-T3"/>
<attribute name="MOUSER_PART_NUMBER" value="815-CA312R450GS1FT3"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/ABRACON/AMCA31-2R450G-S1F-T3?qs=AAveGqk956GLuOddQEK40Q%3D%3D"/>
<attribute name="MPN" value="AMCA31-2R450G-S1F-T3"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C77" library="GRM0335C1H1R5BA01D" package="CAPC0603X33N" value="GRM0335C1H1R5BA01D">
<attribute name="DESCRIPTION" value="Chip Capacitor value 1R5"/>
<attribute name="HEIGHT" value="0.33mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM0335C1H1R5BA01D"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM0335C1H1R5BA1D"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM0335C1H1R5BA01D?qs=7vGxPDjevFPFqveGwv%252BPUQ%3D%3D"/>
<attribute name="MPN" value="GRM0335C1H1R5BA01D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L9" library="MAKK2016T2R2M" package="INDC2016X100N" value="MAKK2016T2R2M">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 2.2 µH Shielded Drum Core, Wirewound Inductor 1.5 A 160mOhm Max 0806 (2016 Metric) "/>
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MP" value="MAKK2016T2R2M"/>
<attribute name="MPN" value="MAKK2016T2R2M"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2016 Taiyo Yuden"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/MAKK2016T2R2M/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C92" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C91" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C93" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C74" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C75" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C76" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C78" library="GRM0335C1H1R5BA01D" package="CAPC0603X33N" value="DNP">
<attribute name="DESCRIPTION" value="Chip Capacitor value 1R5"/>
<attribute name="HEIGHT" value="0.33mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="GRM0335C1H1R5BA01D"/>
<attribute name="MOUSER_PART_NUMBER" value="81-GRM0335C1H1R5BA1D"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/GRM0335C1H1R5BA01D?qs=7vGxPDjevFPFqveGwv%252BPUQ%3D%3D"/>
<attribute name="MPN" value="GRM0335C1H1R5BA01D"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="2337019-1" package="23370191" value="DNP">
<attribute name="DESCRIPTION" value="RF Connectors / Coaxial Connectors MicroCoax receptacle UMCC Gen 1"/>
<attribute name="HEIGHT" value="1.4mm"/>
<attribute name="MANUFACTURER_NAME" value="TE Connectivity"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="2337019-1"/>
<attribute name="MOUSER_PART_NUMBER" value="571-2337019-1"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/TE-Connectivity/2337019-1?qs=l4Gc20tDgJIuN7nS9rJkJw%3D%3D"/>
<attribute name="MPN" value="2337019-1"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="L7" library="SparkFun-Coils" package="0402" value="3.9NH">
<attribute name="MPN" value="L-07C3N9SV6T"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="NDUC-13457"/>
<attribute name="VALUE"/>
</element>
<element name="C81" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C90" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C66" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C68" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C86" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C87" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C94" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C97" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C99" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C98" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C103" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C100" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C53" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C54" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C55" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C69" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C70" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C102" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C107" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C109" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="sfe" package="0402-RES" value="30K">
<attribute name="MPN" value="0402WGF3002TCE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C62" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C57" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C58" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="L5" library="MAKK2016T4R7M" package="INDC2016X100N" value="MAKK2016T4R7M">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 4.7 µH Shielded Drum Core, Wirewound Inductor 1 A 380mOhm Max 0806 (2016 Metric) "/>
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MP" value="MAKK2016T4R7M"/>
<attribute name="MPN" value="MAKK2016T4R7M"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2016 Taiyo Yuden"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/MAKK2016T4R7M/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C101" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C108" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C104" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L6" library="sfe" package="C0402" value="100">
<attribute name="MPN" value="MFBM1V1608-101-R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C60" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C59" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="sfe" package="0402-RES" value="10K">
<attribute name="MPN" value="AC0402FR-1310KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C64" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C67" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C88" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C95" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C71" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C72" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C61" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C73" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="2N7002KW_R1_00001" package="SOT65P210X110-3N" value="2N7002KW_R1_00001">
<attribute name="DESCRIPTION" value="MOSFET 60V N-Channel Enhancement Mode MOSFET - ESD Protected"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="PANJIT"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="2N7002KW_R1_00001"/>
<attribute name="MOUSER_PART_NUMBER" value="241-2N7002KWR100001"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Panjit/2N7002KW_R1_00001?qs=sPbYRqrBIVliWKATqv7jNA%3D%3D"/>
<attribute name="MPN" value="2N7002KW_R1_00001"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C63" library="rcl" package="C0201" value="0.22uF">
<attribute name="MPN" value="GRM033R60J224ME15D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="Y2" library="XRCGB24M000F3M00R0" package="XRCGB24M000F3M00R0" value="XRCGB24M000F3M00R0">
<attribute name="DESCRIPTION" value="Murata 24MHz Crystal +/-30ppm SMD 4-Pin 2 x 1.6 x 0.7mm"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="XRCGB24M000F3M00R0"/>
<attribute name="MOUSER_PART_NUMBER" value="81-XRCGB24M000F3M0R0"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/XRCGB24M000F3M00R0?qs=e%252BE4OD6MgMefDn8VvwDdfw%3D%3D"/>
<attribute name="MPN" value="XRCGB24M000F3M00R0"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C105" library="rcl" package="C0201" value="4.7pF">
<attribute name="MPN" value="GRM0335C1E4R7CA01D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C106" library="rcl" package="C0201" value="4.7pF">
<attribute name="MPN" value="GRM0335C1E4R7CA01D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="sfe" package="0402-RES" value="2.2M">
<attribute name="MPN" value="RC0402FR-072M2L"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="ABS07-32.768KHZ-7-T" package="XTAL_ABS07-32.768KHZ-7-T" value="SC32S-7PF20PPM">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 32.768 kHz ±20ppm Crystal 7pF 70 kOhms 2-SMD, No Lead "/>
<attribute name="MF" value="Abracon"/>
<attribute name="MP" value="ABS07-32.768KHZ-7-T"/>
<attribute name="MPN" value="SC32S-7PF20PPM"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SMD-2 Abracon LLC"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/ABS07-32.768KHZ-7-T/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C80" library="rcl" package="C0201" value="18pF">
<attribute name="MPN" value="GRM0335C1E180JA01D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C79" library="rcl" package="C0201" value="18pF">
<attribute name="MPN" value="GRM0335C1E180JA01D"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="sfe" package="0402-CAP" value="4.7uF">
<attribute name="MPN" value="JMK105BBJ475MV-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="2N7002KW_R1_00001" package="SOT65P210X110-3N" value="2N7002KW_R1_00001">
<attribute name="DESCRIPTION" value="MOSFET 60V N-Channel Enhancement Mode MOSFET - ESD Protected"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="PANJIT"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="2N7002KW_R1_00001"/>
<attribute name="MOUSER_PART_NUMBER" value="241-2N7002KWR100001"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Panjit/2N7002KW_R1_00001?qs=sPbYRqrBIVliWKATqv7jNA%3D%3D"/>
<attribute name="MPN" value="2N7002KW_R1_00001"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="2N7002KW_R1_00001" package="SOT65P210X110-3N" value="2N7002KW_R1_00001">
<attribute name="DESCRIPTION" value="MOSFET 60V N-Channel Enhancement Mode MOSFET - ESD Protected"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="PANJIT"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="2N7002KW_R1_00001"/>
<attribute name="MOUSER_PART_NUMBER" value="241-2N7002KWR100001"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Panjit/2N7002KW_R1_00001?qs=sPbYRqrBIVliWKATqv7jNA%3D%3D"/>
<attribute name="MPN" value="2N7002KW_R1_00001"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="sfe" package="0402-RES" value="1K">
<attribute name="MPN" value="0402WGF1001TCE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="MIC5365-3.3YMT-TZ" package="VREG_MIC5365-3.3YMT-TZ" value="MIC5365-3.3YMT-TZ">
<attribute name="MPN" value="MIC5365-3.3YMT-TZ"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FL1" library="ECMF02-4CMX8" package="ECMF024CMX8" value="ECMF02-4CMX8">
<attribute name="DESCRIPTION" value="Common Mode Filter &amp; ESD Prot. USB uQFN8 STMicroelectronics ECMF02 Series, Signal Filter uQFN SMD, Flat Contact Termination, 2.6 x 1.3 x 0.6mm"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="STMicroelectronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ECMF02-4CMX8"/>
<attribute name="MOUSER_PART_NUMBER" value="511-ECMF02-4CMX8"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/STMicroelectronics/ECMF02-4CMX8?qs=xYt8xtm2zhmK7GoDlDZR3A%3D%3D"/>
<attribute name="MPN" value="ECMF02-4CMX8"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN2" library="EXB-2HV104JV" package="EXB2HV104JV" value="EXB-2HV104JV">
<attribute name="DESCRIPTION" value="Resistor Networks &amp; Arrays Resistor Array Chip 8 Elements 1506"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="MANUFACTURER_NAME" value="Panasonic"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="EXB-2HV104JV"/>
<attribute name="MOUSER_PART_NUMBER" value="667-EXB-2HV104JV"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Panasonic/EXB-2HV104JV?qs=9MgLB97nXf9MD%252BafCCtPcA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="1040310811" package="1040310811" value="USD-1040310811">
<attribute name="MPN" value="104031-0811"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN1" library="EXB-2HV104JV" package="EXB2HV104JV" value="EXB-2HV104JV">
<attribute name="DESCRIPTION" value="Resistor Networks &amp; Arrays Resistor Array Chip 8 Elements 1506"/>
<attribute name="HEIGHT" value="0.55mm"/>
<attribute name="MANUFACTURER_NAME" value="Panasonic"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="EXB-2HV104JV"/>
<attribute name="MOUSER_PART_NUMBER" value="667-EXB-2HV104JV"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Panasonic/EXB-2HV104JV?qs=9MgLB97nXf9MD%252BafCCtPcA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="FD1" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD5" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD6" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD2" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD3" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD7" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD4" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD8" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J4" pad="19"/>
<contactref element="J4" pad="27"/>
<contactref element="J4" pad="5"/>
<contactref element="J6" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="J1" pad="A1_B12"/>
<contactref element="J1" pad="B1_A12"/>
<contactref element="L3" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="17"/>
<contactref element="C10" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="15"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="C5" pad="1"/>
<contactref element="IC1" pad="5"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="D2" pad="2"/>
<contactref element="CN1" pad="2"/>
<contactref element="IC3" pad="E3"/>
<contactref element="C13" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C17" pad="1"/>
<contactref element="IC3" pad="D7"/>
<contactref element="IC3" pad="C3"/>
<contactref element="IC3" pad="B7"/>
<contactref element="IC3" pad="A1"/>
<contactref element="IC3" pad="A3"/>
<contactref element="C31" pad="1"/>
<contactref element="C30" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="IC3" pad="J1"/>
<contactref element="IC5" pad="4"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="1"/>
<contactref element="IC5" pad="9"/>
<contactref element="C24" pad="2"/>
<contactref element="C25" pad="1"/>
<contactref element="IC6" pad="4"/>
<contactref element="IC6" pad="9"/>
<contactref element="IC4" pad="4"/>
<contactref element="IC4" pad="9"/>
<contactref element="C20" pad="2"/>
<contactref element="C27" pad="1"/>
<contactref element="C26" pad="2"/>
<contactref element="IC7" pad="3"/>
<contactref element="FL3" pad="13"/>
<contactref element="C36" pad="2"/>
<contactref element="C35" pad="1"/>
<contactref element="C37" pad="2"/>
<contactref element="D6" pad="2"/>
<contactref element="J8" pad="5"/>
<contactref element="J8" pad="3"/>
<contactref element="D10" pad="2"/>
<contactref element="FL5" pad="13"/>
<contactref element="R37" pad="2"/>
<contactref element="C39" pad="1"/>
<contactref element="C40" pad="1"/>
<contactref element="C42" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="R27" pad="2"/>
<contactref element="C51" pad="2"/>
<contactref element="C83" pad="1"/>
<contactref element="C84" pad="2"/>
<contactref element="C89" pad="2"/>
<contactref element="C96" pad="2"/>
<contactref element="IC9" pad="22"/>
<contactref element="IC9" pad="25"/>
<contactref element="C82" pad="2"/>
<contactref element="C85" pad="2"/>
<contactref element="R38" pad="2"/>
<contactref element="FL2" pad="13"/>
<contactref element="FL4" pad="13"/>
<contactref element="C65" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="D5" pad="2"/>
<contactref element="D4" pad="2"/>
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="37"/>
<contactref element="U3" pad="33"/>
<contactref element="U3" pad="32"/>
<contactref element="C91" pad="1"/>
<contactref element="U3" pad="21"/>
<contactref element="U3" pad="29"/>
<contactref element="U3" pad="43"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="40"/>
<contactref element="U3" pad="19"/>
<contactref element="U3" pad="35"/>
<contactref element="U3" pad="42"/>
<contactref element="U3" pad="45"/>
<contactref element="U3" pad="44"/>
<contactref element="U3" pad="46"/>
<contactref element="U3" pad="12"/>
<contactref element="C92" pad="1"/>
<contactref element="C93" pad="1"/>
<contactref element="C76" pad="2"/>
<contactref element="C75" pad="2"/>
<contactref element="C74" pad="2"/>
<contactref element="C77" pad="2"/>
<contactref element="C78" pad="2"/>
<contactref element="J7" pad="3"/>
<contactref element="J7" pad="2"/>
<contactref element="C81" pad="1"/>
<contactref element="C90" pad="1"/>
<contactref element="IC8" pad="A1"/>
<contactref element="IC8" pad="A14"/>
<contactref element="IC8" pad="B5"/>
<contactref element="IC8" pad="B10"/>
<contactref element="IC8" pad="E2"/>
<contactref element="IC8" pad="E13"/>
<contactref element="IC8" pad="G7"/>
<contactref element="IC8" pad="G8"/>
<contactref element="C103" pad="1"/>
<contactref element="C99" pad="1"/>
<contactref element="C98" pad="1"/>
<contactref element="C97" pad="1"/>
<contactref element="C94" pad="1"/>
<contactref element="C87" pad="1"/>
<contactref element="C86" pad="1"/>
<contactref element="C68" pad="1"/>
<contactref element="C66" pad="1"/>
<contactref element="C100" pad="1"/>
<contactref element="IC8" pad="K6"/>
<contactref element="IC8" pad="H8"/>
<contactref element="IC8" pad="H7"/>
<contactref element="IC8" pad="J8"/>
<contactref element="IC8" pad="J7"/>
<contactref element="IC8" pad="K2"/>
<contactref element="IC8" pad="K13"/>
<contactref element="IC8" pad="L9"/>
<contactref element="IC8" pad="N5"/>
<contactref element="IC8" pad="N8"/>
<contactref element="IC8" pad="P1"/>
<contactref element="IC8" pad="P14"/>
<contactref element="C34" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="IC8" pad="K9"/>
<contactref element="C55" pad="2"/>
<contactref element="C56" pad="2"/>
<contactref element="C53" pad="2"/>
<contactref element="C54" pad="2"/>
<contactref element="C70" pad="2"/>
<contactref element="IC8" pad="N1"/>
<contactref element="IC8" pad="N2"/>
<contactref element="C102" pad="2"/>
<contactref element="C107" pad="2"/>
<contactref element="C109" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="C57" pad="1"/>
<contactref element="C58" pad="1"/>
<contactref element="C101" pad="1"/>
<contactref element="C108" pad="1"/>
<contactref element="C104" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C64" pad="2"/>
<contactref element="C67" pad="2"/>
<contactref element="C41" pad="1"/>
<contactref element="C50" pad="2"/>
<contactref element="C88" pad="2"/>
<contactref element="C95" pad="1"/>
<contactref element="D8" pad="2"/>
<contactref element="C63" pad="2"/>
<contactref element="C62" pad="2"/>
<contactref element="C69" pad="2"/>
<contactref element="C106" pad="2"/>
<contactref element="C105" pad="2"/>
<contactref element="Y2" pad="4"/>
<contactref element="Y2" pad="2"/>
<contactref element="R40" pad="2"/>
<contactref element="C79" pad="2"/>
<contactref element="C80" pad="2"/>
<contactref element="C61" pad="1"/>
<contactref element="C60" pad="1"/>
<contactref element="C59" pad="2"/>
<contactref element="C71" pad="2"/>
<contactref element="C72" pad="1"/>
<contactref element="C73" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="C48" pad="2"/>
<contactref element="C49" pad="1"/>
<contactref element="C47" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="D7" pad="2"/>
<contactref element="C52" pad="1"/>
<contactref element="C32" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="EP"/>
<contactref element="FL1" pad="8"/>
<contactref element="FL1" pad="5"/>
<contactref element="J5" pad="CD$2"/>
<contactref element="J5" pad="P$6"/>
<contactref element="J5" pad="G$1"/>
<contactref element="J5" pad="G$2"/>
<contactref element="J5" pad="G$3"/>
<contactref element="J5" pad="G$4"/>
<contactref element="D9" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="VBUS">
<contactref element="L1" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="U2" pad="13"/>
<contactref element="IC8" pad="N6"/>
<contactref element="C88" pad="1"/>
<contactref element="C95" pad="2"/>
<contactref element="FL1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="J2" pad="1"/>
<contactref element="IC2" pad="6"/>
<contactref element="C7" pad="1"/>
<contactref element="L2" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="IC3" pad="A7"/>
<contactref element="IC3" pad="A9"/>
<contactref element="IC3" pad="B3"/>
<contactref element="IC3" pad="C7"/>
<contactref element="IC3" pad="D3"/>
<contactref element="C13" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C17" pad="2"/>
<contactref element="C19" pad="1"/>
<contactref element="IC3" pad="J9"/>
<contactref element="C31" pad="2"/>
<contactref element="C30" pad="1"/>
<contactref element="IC3" pad="E7"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="C23" pad="2"/>
<contactref element="IC5" pad="8"/>
<contactref element="C22" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="C25" pad="2"/>
<contactref element="C24" pad="1"/>
<contactref element="IC6" pad="8"/>
<contactref element="IC4" pad="8"/>
<contactref element="C20" pad="1"/>
<contactref element="IC7" pad="6"/>
<contactref element="R16" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="C26" pad="1"/>
<contactref element="C27" pad="2"/>
<contactref element="D3" pad="4"/>
<contactref element="C36" pad="1"/>
<contactref element="C35" pad="2"/>
<contactref element="C37" pad="1"/>
<contactref element="D6" pad="1"/>
<contactref element="J8" pad="1"/>
<contactref element="D10" pad="1"/>
<contactref element="J4" pad="10"/>
<contactref element="J4" pad="20"/>
<contactref element="J4" pad="30"/>
<contactref element="J4" pad="36"/>
<contactref element="J4" pad="2"/>
<contactref element="L4" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C44" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="R31" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="R24" pad="2"/>
<contactref element="R29" pad="2"/>
<contactref element="L8" pad="2"/>
<contactref element="R36" pad="2"/>
<contactref element="R39" pad="2"/>
<contactref element="IC9" pad="14"/>
<contactref element="C89" pad="1"/>
<contactref element="C96" pad="1"/>
<contactref element="R34" pad="2"/>
<contactref element="D4" pad="1"/>
<contactref element="U3" pad="30"/>
<contactref element="C92" pad="2"/>
<contactref element="U3" pad="36"/>
<contactref element="C93" pad="2"/>
<contactref element="C75" pad="1"/>
<contactref element="C76" pad="1"/>
<contactref element="C90" pad="2"/>
<contactref element="IC8" pad="F5"/>
<contactref element="IC8" pad="F10"/>
<contactref element="C86" pad="2"/>
<contactref element="C99" pad="2"/>
<contactref element="IC8" pad="E9"/>
<contactref element="C68" pad="2"/>
<contactref element="IC8" pad="E6"/>
<contactref element="C66" pad="2"/>
<contactref element="IC8" pad="J6"/>
<contactref element="IC8" pad="J10"/>
<contactref element="IC8" pad="K4"/>
<contactref element="IC8" pad="K5"/>
<contactref element="IC8" pad="L1"/>
<contactref element="IC8" pad="L2"/>
<contactref element="C56" pad="1"/>
<contactref element="C55" pad="1"/>
<contactref element="C53" pad="1"/>
<contactref element="C54" pad="1"/>
<contactref element="IC8" pad="P12"/>
<contactref element="C109" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="C57" pad="2"/>
<contactref element="C58" pad="2"/>
<contactref element="C108" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C64" pad="1"/>
<contactref element="C67" pad="1"/>
<contactref element="C41" pad="2"/>
<contactref element="C50" pad="1"/>
<contactref element="R33" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="L6" pad="2"/>
<contactref element="C32" pad="1"/>
<contactref element="Q4" pad="1"/>
<contactref element="Q5" pad="1"/>
<contactref element="R28" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="RN2" pad="1"/>
<contactref element="RN2" pad="2"/>
<contactref element="RN2" pad="3"/>
<contactref element="RN2" pad="4"/>
<contactref element="RN2" pad="5"/>
<contactref element="J5" pad="P$4"/>
<contactref element="RN1" pad="6"/>
<contactref element="RN1" pad="5"/>
<contactref element="RN1" pad="4"/>
<contactref element="RN1" pad="3"/>
<contactref element="RN1" pad="2"/>
<contactref element="RN1" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="RN1" pad="8"/>
<contactref element="RN1" pad="7"/>
<contactref element="RN2" pad="6"/>
<contactref element="RN2" pad="7"/>
<contactref element="RN2" pad="8"/>
</signal>
<signal name="DCMI_D0">
<contactref element="J4" pad="31"/>
<contactref element="IC8" pad="J14"/>
</signal>
<signal name="DCMI_D1">
<contactref element="J4" pad="29"/>
<contactref element="IC8" pad="G12"/>
</signal>
<signal name="DCMI_PCLK">
<contactref element="J4" pad="14"/>
<contactref element="IC8" pad="D13"/>
</signal>
<signal name="DCMI_HSYNC">
<contactref element="J4" pad="18"/>
<contactref element="IC8" pad="L10"/>
</signal>
<signal name="DCMI_VSYNC">
<contactref element="J4" pad="16"/>
<contactref element="IC8" pad="D14"/>
</signal>
<signal name="DCMI_CLK">
<contactref element="J4" pad="12"/>
<contactref element="IC8" pad="B14"/>
</signal>
<signal name="DCMI_RST">
<contactref element="R27" pad="1"/>
<contactref element="J4" pad="21"/>
<contactref element="IC8" pad="B11"/>
</signal>
<signal name="DCMI_PWDN">
<contactref element="J4" pad="25"/>
<contactref element="R29" pad="1"/>
<contactref element="IC8" pad="C11"/>
</signal>
<signal name="DCMI_D2">
<contactref element="J4" pad="35"/>
<contactref element="IC8" pad="H11"/>
</signal>
<signal name="DCMI_D3">
<contactref element="J4" pad="28"/>
<contactref element="IC8" pad="H12"/>
</signal>
<signal name="DCMI_D4">
<contactref element="J4" pad="26"/>
<contactref element="IC8" pad="J13"/>
</signal>
<signal name="DCMI_D5">
<contactref element="J4" pad="33"/>
<contactref element="IC8" pad="L13"/>
</signal>
<signal name="DCMI_D6">
<contactref element="J4" pad="24"/>
<contactref element="IC8" pad="G14"/>
</signal>
<signal name="DCMI_D7">
<contactref element="J4" pad="22"/>
<contactref element="IC8" pad="F11"/>
</signal>
<signal name="LED_G">
<contactref element="R20" pad="1"/>
<contactref element="IC8" pad="A10"/>
</signal>
<signal name="LED_B">
<contactref element="R19" pad="1"/>
<contactref element="IC8" pad="C14"/>
</signal>
<signal name="LED_R">
<contactref element="R21" pad="1"/>
<contactref element="IC8" pad="D9"/>
</signal>
<signal name="RAW">
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="7"/>
<contactref element="C4" pad="2"/>
<contactref element="D1" pad="4"/>
<contactref element="IC2" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="D5" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="Q3" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="SD_CD">
<contactref element="IC8" pad="L11"/>
<contactref element="D9" pad="1"/>
<contactref element="J5" pad="CD$1"/>
<contactref element="RN1" pad="9"/>
</signal>
<signal name="VDDA">
<contactref element="L4" pad="1"/>
<contactref element="J4" pad="4"/>
<contactref element="C51" pad="1"/>
<contactref element="C52" pad="2"/>
</signal>
<signal name="WIFI_D0">
<contactref element="U3" pad="24"/>
<contactref element="IC8" pad="L12"/>
<contactref element="RN2" pad="14"/>
</signal>
<signal name="WIFI_D1">
<contactref element="U3" pad="26"/>
<contactref element="IC8" pad="K12"/>
<contactref element="RN2" pad="12"/>
</signal>
<signal name="WIFI_CLK">
<contactref element="U3" pad="20"/>
<contactref element="IC8" pad="M13"/>
</signal>
<signal name="WIFI_CMD">
<contactref element="U3" pad="22"/>
<contactref element="IC8" pad="H13"/>
<contactref element="RN2" pad="16"/>
</signal>
<signal name="WIFI_D3">
<contactref element="U3" pad="25"/>
<contactref element="IC8" pad="K10"/>
<contactref element="RN2" pad="13"/>
</signal>
<signal name="USB_D_P">
<contactref element="IC8" pad="L8"/>
<contactref element="FL1" pad="7"/>
</signal>
<signal name="WL_REG_ON">
<contactref element="U3" pad="28"/>
<contactref element="IC8" pad="E10"/>
</signal>
<signal name="WL_H_WAKE">
<contactref element="U3" pad="27"/>
<contactref element="IC8" pad="E11"/>
</signal>
<signal name="BT_H_WAKE">
<contactref element="U3" pad="38"/>
<contactref element="IC8" pad="H14"/>
</signal>
<signal name="BT_REG_ON">
<contactref element="U3" pad="14"/>
<contactref element="R37" pad="1"/>
<contactref element="IC8" pad="F13"/>
</signal>
<signal name="BT_D_WAKE">
<contactref element="U3" pad="39"/>
<contactref element="IC8" pad="L7"/>
</signal>
<signal name="VIN">
<contactref element="IC1" pad="6"/>
<contactref element="C5" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="D7" pad="1"/>
</signal>
<signal name="TS">
<contactref element="R9" pad="1"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="ISET">
<contactref element="U2" pad="16"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="BAT">
<contactref element="C8" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="CN1" pad="1"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="CHG">
<contactref element="U2" pad="9"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="CC1">
<contactref element="R6" pad="1"/>
<contactref element="J1" pad="A5"/>
</signal>
<signal name="CC2">
<contactref element="R7" pad="1"/>
<contactref element="J1" pad="B5"/>
</signal>
<signal name="SHELL_GND">
<contactref element="J1" pad="S1"/>
<contactref element="J1" pad="S2"/>
<contactref element="J1" pad="S4"/>
<contactref element="J1" pad="S3"/>
<contactref element="L3" pad="2"/>
</signal>
<signal name="D_P">
<contactref element="J1" pad="B6"/>
<contactref element="J1" pad="A6"/>
<contactref element="FL1" pad="2"/>
</signal>
<signal name="D_N">
<contactref element="J1" pad="B7"/>
<contactref element="J1" pad="A7"/>
<contactref element="FL1" pad="3"/>
</signal>
<signal name="ILIM">
<contactref element="U2" pad="12"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="TMR">
<contactref element="R11" pad="1"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="PGOOD">
<contactref element="U2" pad="7"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="LED_PGOOD">
<contactref element="R4" pad="2"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="LED_CHG">
<contactref element="R1" pad="2"/>
<contactref element="D1" pad="3"/>
</signal>
<signal name="ST">
<contactref element="IC1" pad="8"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="LED_ST">
<contactref element="D1" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="SW">
<contactref element="IC2" pad="4"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="FB">
<contactref element="IC2" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="EN">
<contactref element="IC2" pad="5"/>
<contactref element="R3" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="PMIC_ON_REQ">
<contactref element="Q1" pad="2"/>
<contactref element="IC8" pad="K7"/>
</signal>
<signal name="SDRAM_A8">
<contactref element="IC3" pad="H1"/>
<contactref element="IC8" pad="A4"/>
</signal>
<signal name="SDRAM_A7">
<contactref element="IC3" pad="H2"/>
<contactref element="IC8" pad="A5"/>
</signal>
<signal name="SDRAM_A6">
<contactref element="IC3" pad="H3"/>
<contactref element="IC8" pad="B1"/>
</signal>
<signal name="SDRAM_A0">
<contactref element="IC3" pad="H7"/>
<contactref element="IC8" pad="C2"/>
</signal>
<signal name="SDRAM_A1">
<contactref element="IC3" pad="H8"/>
<contactref element="IC8" pad="G1"/>
</signal>
<signal name="SDRAM_A10">
<contactref element="IC3" pad="H9"/>
<contactref element="IC8" pad="G2"/>
</signal>
<signal name="SDRAM_A5">
<contactref element="IC3" pad="J2"/>
<contactref element="IC8" pad="B6"/>
</signal>
<signal name="SDRAM_A4">
<contactref element="IC3" pad="J3"/>
<contactref element="IC8" pad="A6"/>
</signal>
<signal name="SDRAM_A3">
<contactref element="IC3" pad="J7"/>
<contactref element="IC8" pad="H1"/>
</signal>
<signal name="SDRAM_A2">
<contactref element="IC3" pad="J8"/>
<contactref element="IC8" pad="G3"/>
</signal>
<signal name="SDRAM_CS">
<contactref element="IC3" pad="G9"/>
<contactref element="R18" pad="2"/>
<contactref element="IC8" pad="E1"/>
</signal>
<signal name="SDRAM_BA1">
<contactref element="IC3" pad="G8"/>
<contactref element="IC8" pad="F1"/>
</signal>
<signal name="SDRAM_BA0">
<contactref element="IC3" pad="G7"/>
<contactref element="IC8" pad="C1"/>
</signal>
<signal name="SDRAM_A9">
<contactref element="IC3" pad="G3"/>
<contactref element="IC8" pad="B2"/>
</signal>
<signal name="SDRAM_A12">
<contactref element="IC3" pad="G1"/>
<contactref element="IC8" pad="A3"/>
</signal>
<signal name="SDRAM_A11">
<contactref element="IC3" pad="G2"/>
<contactref element="IC8" pad="B4"/>
</signal>
<signal name="SDRAM_WE">
<contactref element="IC3" pad="F9"/>
<contactref element="IC8" pad="D1"/>
</signal>
<signal name="SDRAM_RAS">
<contactref element="IC3" pad="F8"/>
<contactref element="IC8" pad="D2"/>
</signal>
<signal name="SDRAM_CAS">
<contactref element="IC3" pad="F7"/>
<contactref element="IC8" pad="D3"/>
</signal>
<signal name="SDRAM_CKE">
<contactref element="IC3" pad="F3"/>
<contactref element="IC8" pad="A2"/>
</signal>
<signal name="SDRAM_CLK">
<contactref element="IC3" pad="F2"/>
<contactref element="IC8" pad="B3"/>
</signal>
<signal name="SDRAM_DQMH">
<contactref element="IC3" pad="F1"/>
<contactref element="IC8" pad="D6"/>
</signal>
<signal name="SDRAM_DQ7">
<contactref element="IC3" pad="E9"/>
<contactref element="IC8" pad="H4"/>
</signal>
<signal name="SDRAM_DQML">
<contactref element="IC3" pad="E8"/>
<contactref element="IC8" pad="H3"/>
</signal>
<signal name="SDRAM_DQ15">
<contactref element="IC3" pad="A2"/>
<contactref element="IC8" pad="E4"/>
</signal>
<signal name="SDRAM_DQ0">
<contactref element="IC3" pad="A8"/>
<contactref element="IC8" pad="E3"/>
</signal>
<signal name="SDRAM_DQ14">
<contactref element="IC3" pad="B1"/>
<contactref element="IC8" pad="C3"/>
</signal>
<signal name="SDRAM_DQ13">
<contactref element="IC3" pad="B2"/>
<contactref element="IC8" pad="E5"/>
</signal>
<signal name="SDRAM_DQ2">
<contactref element="IC3" pad="B8"/>
<contactref element="IC8" pad="F4"/>
</signal>
<signal name="SDRAM_DQ1">
<contactref element="IC3" pad="B9"/>
<contactref element="IC8" pad="F3"/>
</signal>
<signal name="SDRAM_DQ12">
<contactref element="IC3" pad="C1"/>
<contactref element="IC8" pad="D4"/>
</signal>
<signal name="SDRAM_DQ11">
<contactref element="IC3" pad="C2"/>
<contactref element="IC8" pad="C4"/>
</signal>
<signal name="SDRAM_DQ4">
<contactref element="IC3" pad="C8"/>
<contactref element="IC8" pad="F2"/>
</signal>
<signal name="SDRAM_DQ3">
<contactref element="IC3" pad="C9"/>
<contactref element="IC8" pad="G4"/>
</signal>
<signal name="SDRAM_DQ10">
<contactref element="IC3" pad="D1"/>
<contactref element="IC8" pad="D5"/>
</signal>
<signal name="SDRAM_DQ9">
<contactref element="IC3" pad="D2"/>
<contactref element="IC8" pad="C5"/>
</signal>
<signal name="SDRAM_DQ6">
<contactref element="IC3" pad="D8"/>
<contactref element="IC8" pad="H5"/>
</signal>
<signal name="SDRAM_DQ5">
<contactref element="IC3" pad="D9"/>
<contactref element="IC8" pad="G5"/>
</signal>
<signal name="SDRAM_DQ8">
<contactref element="IC3" pad="E1"/>
<contactref element="IC8" pad="C6"/>
</signal>
<signal name="P_FLASH_CE">
<contactref element="IC5" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="IC8" pad="L3"/>
</signal>
<signal name="P_FLASH_IO1">
<contactref element="IC5" pad="2"/>
<contactref element="IC8" pad="N4"/>
</signal>
<signal name="P_FLASH_IO2">
<contactref element="IC5" pad="3"/>
<contactref element="IC8" pad="P4"/>
</signal>
<signal name="P_FLASH_IO3">
<contactref element="IC5" pad="7"/>
<contactref element="IC8" pad="P5"/>
</signal>
<signal name="P_FLASH_SCK">
<contactref element="IC5" pad="6"/>
<contactref element="IC8" pad="L4"/>
</signal>
<signal name="P_FLASH_IO0">
<contactref element="IC5" pad="5"/>
<contactref element="IC8" pad="P3"/>
</signal>
<signal name="S_FLASH_CE">
<contactref element="R14" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="IC8" pad="N3"/>
</signal>
<signal name="S_FLASH_IO1">
<contactref element="IC6" pad="2"/>
<contactref element="IC8" pad="M3"/>
</signal>
<signal name="S_FLASH_IO2">
<contactref element="IC6" pad="3"/>
<contactref element="IC8" pad="M5"/>
</signal>
<signal name="S_FLASH_IO3">
<contactref element="IC6" pad="7"/>
<contactref element="IC8" pad="L5"/>
</signal>
<signal name="S_FLASH_SCK">
<contactref element="IC6" pad="6"/>
<contactref element="IC8" pad="P2"/>
</signal>
<signal name="S_FLASH_IO0">
<contactref element="IC6" pad="5"/>
<contactref element="IC8" pad="M4"/>
</signal>
<signal name="INT_I2C_INT">
<contactref element="R17" pad="1"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC8" pad="D11"/>
</signal>
<signal name="LED_B_INT">
<contactref element="D3" pad="1"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="LED_G_INT">
<contactref element="D3" pad="2"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="LED_R_INT">
<contactref element="D3" pad="3"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="SD_DAT2_INT">
<contactref element="FL3" pad="12"/>
<contactref element="J5" pad="P$1"/>
</signal>
<signal name="SD_DAT3_INT">
<contactref element="FL3" pad="11"/>
<contactref element="J5" pad="P$2"/>
</signal>
<signal name="SD_CMD_INT">
<contactref element="J5" pad="P$3"/>
<contactref element="FL3" pad="10"/>
</signal>
<signal name="SD_CLK_INT">
<contactref element="J5" pad="P$5"/>
<contactref element="FL3" pad="9"/>
</signal>
<signal name="SD_DAT0">
<contactref element="IC8" pad="J1"/>
<contactref element="FL3" pad="5"/>
<contactref element="RN1" pad="14"/>
</signal>
<signal name="SD_DAT1">
<contactref element="IC8" pad="K1"/>
<contactref element="FL3" pad="6"/>
<contactref element="RN1" pad="13"/>
</signal>
<signal name="SD_DAT2">
<contactref element="IC8" pad="H2"/>
<contactref element="FL3" pad="1"/>
<contactref element="RN1" pad="10"/>
</signal>
<signal name="SD_DAT3">
<contactref element="IC8" pad="J2"/>
<contactref element="FL3" pad="2"/>
<contactref element="RN1" pad="11"/>
</signal>
<signal name="SD_CMD">
<contactref element="IC8" pad="J4"/>
<contactref element="FL3" pad="3"/>
<contactref element="RN1" pad="12"/>
</signal>
<signal name="SD_CLK">
<contactref element="IC8" pad="J3"/>
<contactref element="FL3" pad="4"/>
</signal>
<signal name="JTAG_TMS_INT">
<contactref element="FL5" pad="8"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="JTAG_TCK_INT">
<contactref element="J8" pad="4"/>
<contactref element="FL5" pad="9"/>
</signal>
<signal name="JTAG_TDO_INT">
<contactref element="FL5" pad="10"/>
<contactref element="J8" pad="6"/>
</signal>
<signal name="JTAG_TDI_INT">
<contactref element="J8" pad="8"/>
<contactref element="FL5" pad="11"/>
</signal>
<signal name="P12_RST_N_EXT">
<contactref element="J6" pad="8"/>
<contactref element="J8" pad="10"/>
<contactref element="FL5" pad="12"/>
</signal>
<signal name="JTAG_TMS">
<contactref element="IC8" pad="E14"/>
<contactref element="FL5" pad="5"/>
</signal>
<signal name="JTAG_TCK">
<contactref element="IC8" pad="F12"/>
<contactref element="FL5" pad="4"/>
</signal>
<signal name="JTAG_TDO">
<contactref element="FL5" pad="3"/>
<contactref element="IC8" pad="G13"/>
</signal>
<signal name="JTAG_TDI">
<contactref element="IC8" pad="F14"/>
<contactref element="FL5" pad="2"/>
</signal>
<signal name="JTAG_TRSTB">
<contactref element="FL5" pad="6"/>
<contactref element="IC8" pad="G10"/>
</signal>
<signal name="P12_RST_N">
<contactref element="IC8" pad="M7"/>
<contactref element="C63" pad="1"/>
<contactref element="R33" pad="2"/>
<contactref element="FL5" pad="1"/>
</signal>
<signal name="JTAG_TRSTB_INT">
<contactref element="FL5" pad="7"/>
<contactref element="J8" pad="9"/>
</signal>
<signal name="DCMI_SCL">
<contactref element="J4" pad="32"/>
<contactref element="R30" pad="1"/>
<contactref element="IC8" pad="J11"/>
</signal>
<signal name="DCMI_SDA">
<contactref element="J4" pad="34"/>
<contactref element="R31" pad="1"/>
<contactref element="IC8" pad="K11"/>
</signal>
<signal name="DCMI_SCLK">
<contactref element="J4" pad="13"/>
<contactref element="IC8" pad="D8"/>
</signal>
<signal name="DCMI_MISO">
<contactref element="J4" pad="15"/>
<contactref element="IC8" pad="E7"/>
</signal>
<signal name="DCMI_MOSI">
<contactref element="J4" pad="17"/>
<contactref element="IC8" pad="E8"/>
</signal>
<signal name="DCMI_SSEL">
<contactref element="J4" pad="11"/>
<contactref element="R24" pad="1"/>
<contactref element="IC8" pad="D7"/>
</signal>
<signal name="ETH_TXEN">
<contactref element="IC9" pad="19"/>
<contactref element="IC8" pad="A13"/>
</signal>
<signal name="ETH_TXD0">
<contactref element="IC9" pad="20"/>
<contactref element="IC8" pad="B12"/>
</signal>
<signal name="ETH_TXD1">
<contactref element="IC9" pad="21"/>
<contactref element="IC8" pad="A12"/>
</signal>
<signal name="ETH_MDIO">
<contactref element="IC9" pad="10"/>
<contactref element="R39" pad="1"/>
<contactref element="IC8" pad="C7"/>
</signal>
<signal name="ETH_MDC">
<contactref element="IC9" pad="11"/>
<contactref element="IC8" pad="A7"/>
</signal>
<signal name="ETH_RXD1">
<contactref element="IC9" pad="12"/>
<contactref element="IC8" pad="D12"/>
</signal>
<signal name="ETH_INT">
<contactref element="IC9" pad="18"/>
<contactref element="R36" pad="1"/>
<contactref element="IC8" pad="C10"/>
</signal>
<signal name="ETH_RXERR">
<contactref element="IC9" pad="17"/>
<contactref element="IC8" pad="C13"/>
</signal>
<signal name="ETH_RXD0">
<contactref element="IC9" pad="13"/>
<contactref element="IC8" pad="E12"/>
</signal>
<signal name="MDI_RX_P">
<contactref element="IC9" pad="4"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="MDI_TX_N">
<contactref element="IC9" pad="5"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="MDI_TX_P">
<contactref element="IC9" pad="6"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="ETH_VDDA_3.3">
<contactref element="C82" pad="1"/>
<contactref element="IC9" pad="2"/>
<contactref element="C85" pad="1"/>
<contactref element="L8" pad="1"/>
<contactref element="C81" pad="2"/>
</signal>
<signal name="ETH_VDD_1.2">
<contactref element="C84" pad="1"/>
<contactref element="IC9" pad="1"/>
<contactref element="C83" pad="2"/>
</signal>
<signal name="ETH_RXDV">
<contactref element="IC9" pad="15"/>
<contactref element="IC8" pad="C12"/>
</signal>
<signal name="ETH_RST">
<contactref element="IC9" pad="24"/>
<contactref element="R34" pad="1"/>
<contactref element="C65" pad="2"/>
<contactref element="IC8" pad="D10"/>
</signal>
<signal name="ETH_LED">
<contactref element="IC9" pad="23"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="MDI_LED">
<contactref element="R35" pad="2"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="ETH_TXCLK">
<contactref element="IC9" pad="8"/>
<contactref element="IC8" pad="B13"/>
</signal>
<signal name="REXT">
<contactref element="R38" pad="1"/>
<contactref element="IC9" pad="9"/>
</signal>
<signal name="P0_MOSI">
<contactref element="FL2" pad="1"/>
<contactref element="IC8" pad="H10"/>
</signal>
<signal name="P1_MISO">
<contactref element="FL2" pad="2"/>
<contactref element="IC8" pad="M11"/>
</signal>
<signal name="P2_SCLK">
<contactref element="FL2" pad="3"/>
<contactref element="IC8" pad="M14"/>
</signal>
<signal name="P3_NSS">
<contactref element="FL2" pad="4"/>
<contactref element="IC8" pad="G11"/>
</signal>
<signal name="P4_SCL">
<contactref element="FL2" pad="5"/>
<contactref element="IC8" pad="K14"/>
</signal>
<signal name="P5_SDA">
<contactref element="FL2" pad="6"/>
<contactref element="IC8" pad="L14"/>
</signal>
<signal name="P6_ADC_INT">
<contactref element="J2" pad="2"/>
<contactref element="FL4" pad="12"/>
</signal>
<signal name="P6_ADC">
<contactref element="FL4" pad="1"/>
<contactref element="IC8" pad="M12"/>
</signal>
<signal name="P11_WAKEUP">
<contactref element="R22" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="FL4" pad="6"/>
</signal>
<signal name="P9_PWM">
<contactref element="FL4" pad="4"/>
<contactref element="IC8" pad="A11"/>
</signal>
<signal name="P8_PWM">
<contactref element="IC8" pad="A9"/>
<contactref element="FL4" pad="3"/>
</signal>
<signal name="P7_PWM">
<contactref element="IC8" pad="A8"/>
<contactref element="FL4" pad="2"/>
</signal>
<signal name="P0_MOSI_INT">
<contactref element="J2" pad="8"/>
<contactref element="FL2" pad="12"/>
</signal>
<signal name="P1_MISO_INT">
<contactref element="J2" pad="7"/>
<contactref element="FL2" pad="11"/>
</signal>
<signal name="P2_SCLK_INT">
<contactref element="J2" pad="6"/>
<contactref element="FL2" pad="10"/>
</signal>
<signal name="P3_NSS_INT">
<contactref element="J2" pad="5"/>
<contactref element="FL2" pad="9"/>
</signal>
<signal name="P4_SCL_INT">
<contactref element="J2" pad="4"/>
<contactref element="FL2" pad="8"/>
</signal>
<signal name="P5_SDA_INT">
<contactref element="J2" pad="3"/>
<contactref element="FL2" pad="7"/>
</signal>
<signal name="P11_WAKEUP_INT">
<contactref element="J6" pad="7"/>
<contactref element="FL4" pad="7"/>
</signal>
<signal name="P9_PWM_INT">
<contactref element="J6" pad="5"/>
<contactref element="FL4" pad="9"/>
</signal>
<signal name="P8_PWM_INT">
<contactref element="J6" pad="4"/>
<contactref element="FL4" pad="10"/>
</signal>
<signal name="P7_PWM_INT">
<contactref element="J6" pad="3"/>
<contactref element="FL4" pad="11"/>
</signal>
<signal name="P10_PWM">
<contactref element="Q4" pad="3"/>
<contactref element="R26" pad="1"/>
<contactref element="FL4" pad="5"/>
</signal>
<signal name="P10_PWM_INT">
<contactref element="J6" pad="6"/>
<contactref element="FL4" pad="8"/>
</signal>
<signal name="PMIC_ONOFF">
<contactref element="J3" pad="3"/>
<contactref element="R23" pad="1"/>
<contactref element="Q3" pad="3"/>
<contactref element="D8" pad="1"/>
</signal>
<signal name="WAKEUP">
<contactref element="Q2" pad="2"/>
<contactref element="IC8" pad="L6"/>
</signal>
<signal name="SR_VLX">
<contactref element="U3" pad="34"/>
<contactref element="L9" pad="1"/>
</signal>
<signal name="WIFI_D2">
<contactref element="U3" pad="23"/>
<contactref element="IC8" pad="J12"/>
<contactref element="RN2" pad="15"/>
</signal>
<signal name="BT_UART_RX">
<contactref element="U3" pad="3"/>
<contactref element="IC8" pad="C9"/>
</signal>
<signal name="BT_UART_TX">
<contactref element="U3" pad="2"/>
<contactref element="IC8" pad="B9"/>
</signal>
<signal name="VIN_LDO">
<contactref element="U3" pad="31"/>
<contactref element="L9" pad="2"/>
<contactref element="C91" pad="2"/>
<contactref element="C74" pad="1"/>
</signal>
<signal name="FEED">
<contactref element="ANT1" pad="1"/>
<contactref element="C78" pad="1"/>
<contactref element="L7" pad="1"/>
</signal>
<signal name="ANT">
<contactref element="U3" pad="41"/>
<contactref element="C77" pad="1"/>
<contactref element="L7" pad="2"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="DCDC_LP">
<contactref element="IC8" pad="M1"/>
<contactref element="IC8" pad="M2"/>
<contactref element="L5" pad="2"/>
</signal>
<signal name="INT_I2C_SDA">
<contactref element="R16" pad="1"/>
<contactref element="IC7" pad="5"/>
<contactref element="IC8" pad="B8"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="INT_I2C_SCL">
<contactref element="R15" pad="1"/>
<contactref element="IC7" pad="1"/>
<contactref element="IC8" pad="C8"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="VCC_SOC">
<contactref element="IC8" pad="F6"/>
<contactref element="C87" pad="2"/>
<contactref element="IC8" pad="F7"/>
<contactref element="C94" pad="2"/>
<contactref element="IC8" pad="F8"/>
<contactref element="C97" pad="2"/>
<contactref element="IC8" pad="F9"/>
<contactref element="C98" pad="2"/>
<contactref element="IC8" pad="G6"/>
<contactref element="C100" pad="2"/>
<contactref element="IC8" pad="G9"/>
<contactref element="C103" pad="2"/>
<contactref element="IC8" pad="H6"/>
<contactref element="C34" pad="1"/>
<contactref element="IC8" pad="H9"/>
<contactref element="C38" pad="1"/>
<contactref element="IC8" pad="J5"/>
<contactref element="IC8" pad="J9"/>
<contactref element="C45" pad="1"/>
<contactref element="C46" pad="2"/>
<contactref element="C47" pad="1"/>
<contactref element="C48" pad="1"/>
<contactref element="C49" pad="2"/>
<contactref element="L5" pad="1"/>
</signal>
<signal name="VDD_SNVS_CAP">
<contactref element="IC8" pad="M10"/>
<contactref element="C70" pad="1"/>
</signal>
<signal name="RTC_XTALI">
<contactref element="IC8" pad="N9"/>
<contactref element="Y1" pad="2"/>
<contactref element="C80" pad="1"/>
</signal>
<signal name="XTALO">
<contactref element="IC8" pad="N11"/>
<contactref element="Y2" pad="1"/>
<contactref element="C105" pad="1"/>
</signal>
<signal name="VDDA_ADC_3P3">
<contactref element="IC8" pad="N14"/>
<contactref element="L6" pad="1"/>
<contactref element="C59" pad="1"/>
<contactref element="C60" pad="2"/>
<contactref element="C61" pad="2"/>
</signal>
<signal name="ONOFF">
<contactref element="Q3" pad="2"/>
<contactref element="IC8" pad="M6"/>
</signal>
<signal name="RTC_XTALO">
<contactref element="IC8" pad="P9"/>
<contactref element="C79" pad="1"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="XTALI">
<contactref element="IC8" pad="P11"/>
<contactref element="Y2" pad="3"/>
<contactref element="C106" pad="1"/>
<contactref element="R40" pad="1"/>
</signal>
<signal name="DCDC_PSWITCH">
<contactref element="IC8" pad="K3"/>
<contactref element="R32" pad="1"/>
<contactref element="C62" pad="1"/>
</signal>
<signal name="USB_VBUS">
<contactref element="J1" pad="A4_B9"/>
<contactref element="J1" pad="B4_A9"/>
<contactref element="L1" pad="1"/>
<contactref element="FL1" pad="4"/>
</signal>
<signal name="V_BATT">
<contactref element="U2" pad="5"/>
<contactref element="C10" pad="2"/>
<contactref element="U2" pad="10"/>
<contactref element="U2" pad="11"/>
<contactref element="IC1" pad="3"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="VDD_SNVS">
<contactref element="IC8" pad="M9"/>
<contactref element="C69" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="VDD_HIGH_CAP">
<contactref element="IC8" pad="P8"/>
<contactref element="C102" pad="1"/>
<contactref element="C101" pad="2"/>
</signal>
<signal name="NVCC_PLL">
<contactref element="IC8" pad="P10"/>
<contactref element="C107" pad="1"/>
<contactref element="C104" pad="2"/>
</signal>
<signal name="VDD_USB_CAP">
<contactref element="IC8" pad="K8"/>
<contactref element="C71" pad="1"/>
<contactref element="C72" pad="2"/>
<contactref element="C73" pad="2"/>
</signal>
<signal name="PWM_FSIN">
<contactref element="Q4" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="IC8" pad="B7"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="DCMI_FSIN">
<contactref element="J4" pad="23"/>
<contactref element="R28" pad="1"/>
<contactref element="Q5" pad="3"/>
</signal>
<signal name="USB_D_N">
<contactref element="IC8" pad="M8"/>
<contactref element="FL1" pad="6"/>
</signal>
<signal name="MDI_RX_N">
<contactref element="IC9" pad="3"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="SD_DAT0_INT">
<contactref element="J5" pad="P$7"/>
<contactref element="FL3" pad="8"/>
</signal>
<signal name="SD_DAT1_INT">
<contactref element="J5" pad="P$8"/>
<contactref element="FL3" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
