<?xml version="1.0" encoding="utf-8"?>
<!--/327437/1088951/2.50/16/3/Integrated Circuit/-->
<!DOCTYPE curve SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>&lt;3-V To 5.5-V Single Channel RS-232 1 Mbit/s Line Driver/Receiver&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOP65P640X120-16N">
<description>&lt;b&gt;PW0016A&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="SN65C3221EPWR">
<pin name="!EN" direction="io"/>
<pin name="C1+" direction="io"/>
<pin name="V+" direction="io"/>
<pin name="C1-" direction="io"/>
<pin name="C2+" direction="io"/>
<pin name="C2-" direction="io"/>
<pin name="V-" direction="io"/>
<pin name="RIN" direction="io"/>
<pin name="!FORCEOFF" direction="io"/>
<pin name="VCC" direction="io"/>
<pin name="GND" direction="io"/>
<pin name="DOUT" direction="io"/>
<pin name="FORCEON" direction="io"/>
<pin name="DIN" direction="io"/>
<pin name="!INVALID" direction="io"/>
<pin name="ROUT" direction="io"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SN65C3221EPWR" prefix="IC">
<description>&lt;b&gt;3-V To 5.5-V Single Channel RS-232 1 Mbit/s Line Driver/Receiver&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/gpn/sn65c3221e"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="SN65C3221EPWR"/>
</gates>
<devices>
<device name="" package="SOP65P640X120-16N">
<connects>
<connect gate="G$1" pin="!EN" pad="1"/>
<connect gate="G$1" pin="C1+" pad="2"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="C1-" pad="4"/>
<connect gate="G$1" pin="C2+" pad="5"/>
<connect gate="G$1" pin="C2-" pad="6"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="RIN" pad="8"/>
<connect gate="G$1" pin="ROUT" pad="9"/>
<connect gate="G$1" pin="!INVALID" pad="10"/>
<connect gate="G$1" pin="DIN" pad="11"/>
<connect gate="G$1" pin="FORCEON" pad="12"/>
<connect gate="G$1" pin="DOUT" pad="13"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="VCC" pad="15"/>
<connect gate="G$1" pin="!FORCEOFF" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="Mouser_Part_Number" value="595-SN65C3221EPWR"/>
<attribute name="Mouser_Price-Stock" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/SN65C3221EPWR?qs=6siQ5y5nVCwNDulozFTH8A%3D%3D"/>
<attribute name="Manufacturer_Name" value="Texas Instruments"/>
<attribute name="Manufacturer_Part_Number" value="SN65C3221EPWR"/>
<attribute name="Description" value="3-V To 5.5-V Single Channel RS-232 1 Mbit/s Line Driver/Receiver"/>
<attribute name="Height" value="1.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
