<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.56" y2="0" width="0" layer="20"/>
<wire x1="35.56" y1="0" x2="35.56" y2="26.67" width="0" layer="20"/>
<wire x1="35.56" y1="26.67" x2="0" y2="26.67" width="0" layer="20"/>
<wire x1="0" y1="26.67" x2="0" y2="0" width="0" layer="20"/>
<text>MLX9062x</text>
<text>https://openmv.io</text>
<text>FIR Shield R1</text>
<text>2/11/2016</text>
<text>P6</text>
<text>P4</text>
<text>P5</text>
<text>P3</text>
<text>P2</text>
<text>P1</text>
<text>3v3</text>
<text>P0</text>
<text>P6</text>
<text>P4</text>
<text>P5</text>
<text>P3</text>
<text>P2</text>
<text>P1</text>
<text>3v3</text>
<text>P0</text>
<text>SWD</text>
<text>SWC</text>
<text>BOOT</text>
<text>RST</text>
<text>GND</text>
<text>VCC</text>
<text>P8</text>
<text>P7</text>
<text>SWD</text>
<text>SWC</text>
<text>BOOT</text>
<text>RST</text>
<text>GND</text>
<text>VCC</text>
<text>P8</text>
<text>P7</text>
<text>Made in USA</text>
<text>Built by MacroFab</text>
<text>https://openmv.io</text>
</plain>
<libraries>
<library name="sfe">
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="openmv">
<packages>
<package name="OPENMV3">
</package>
<package name="OMV-LOGO-SMALL">
</package>
<package name="ROHS">
</package>
<package name="WEEE">
</package>
<package name="OMV-LOGO">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="MLX90620">
<packages>
<package name="TO39/4">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="iofault">
<packages>
<package name="OSHW_FILLX150_NOTEXT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U3" library="SparkFun" package="SOT23-5" value="2.6v">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="sfe" package="0603-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="sfe" package="0603-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="sfe" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="MLX90620" package="TO39/4" value="MLX9062x">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="sfe" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="sfe" package="0603-CAP" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="sfe" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="openmv" package="OPENMV3" value="OPENMV3"/>
<element name="U$7" library="iofault" package="OSHW_FILLX150_NOTEXT" value=""/>
<element name="U$10" library="openmv" package="OMV-LOGO-SMALL" value=""/>
<element name="U$5" library="openmv" package="ROHS" value=""/>
<element name="U$6" library="openmv" package="WEEE" value=""/>
<element name="U$3" library="openmv" package="OMV-LOGO" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U3" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U$2" pad="28"/>
<contactref element="U$2" pad="28"/>
</signal>
<signal name="VCC">
<contactref element="U3" pad="5"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$69">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="VIN">
<contactref element="U$2" pad="27"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U$2" pad="16"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U$2" pad="15"/>
</signal>
<signal name="3.3V">
<contactref element="U$2" pad="18"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="C3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
